{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet2"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet2","index":0,"n_rows":681,"n_cols":11,"rows_kept":681,"merged":[[0,0,0,1],[1,0,1,10],[3,0,3,10],[211,8,212,8],[211,9,212,9],[211,10,212,10],[313,0,313,10],[482,0,482,10]],"flags":["formulas_cached_only"]}
["附 件"]
["安徽省安全应急产业重点产品库（2022年版）"]
["序号","重点产品","类别"," 产品介绍及用途（50字以内）","适用行业","企业名称","地市","县（区、市）","企业地址","联系人","联系方式"]
["一、安全防护类（309种）"]
[1,"偏振编码QKD产品","安全防护类","基于诱骗态BB84量子密钥分发协议，采用偏振编码进行量子密钥分发，为量子保密通信网络提供不可窃听、不可破译的量子密钥","专用安全生产 ","科大国盾量子技术股份有限公司","合肥","合肥高新区","望江西路800号创新产业园D3栋","岳德钊",13955130346]
[2,"防火阻燃通用塑料","安全防护类","防火阻燃材料，应用于火灾应急安全","化学原料和化学制品制造业","会通新材料股份有限公司","合肥","合肥高新区","柏堰科技园芦花路2号","朱伟","0551-2229358"]
[3,"ESP安装支架","安全防护类","车辆电子稳定系统安装关键材料","安全材料 ","合肥至信机械制造有限公司","合肥","合肥高新区","响洪甸路960号","柯珂",18556551837]
[4,"振动筛","安全防护类","振动筛是利用振子激振所产生的复旋型振动而工作的。振子的上旋转重锤使筛面产生平面回旋振动，而下旋转重锤则使筛面产生锥面回转振动，其联合作用的效果则使筛面产生复旋型振动，保障矿山工作安全","采矿业","合肥约翰芬雷矿山装备有限公司","合肥","合肥高新区","柏堰科技园长安路58号","张莉",18356030133]
[5,"离心机","安全防护类","以离心力作为推动力，迫使物料加速过滤、沉降或分离，作为安全应急分离设备","专用安全生产 ","合肥约翰芬雷矿山装备有限公司","合肥","合肥高新区","柏堰科技园长安路58号","张莉",18356030133]
[6,"配电装置","安全防护类","城市基础设施专用安全生产装备，能够保障城市安全、正常运行的专用安全装备","专用安全生产 ","合肥元贞电力科技股份有限公司","合肥","合肥高新区","长安路66号","余婷婷",15155964028]
[7,"电气柜","安全防护类","微机保护测控、 SCADA-NT集成化保护自动化监控系统、EPS、UPS、高低压成套开关柜等研发、生产","专用安全生产 ","合肥英特电力设备有限公司","合肥","合肥高新区","西四路9号","方瑜",13866727936]
[8,"电机控制器","安全防护类","电机控制器作为“三电”核心，将电池的直流电转换成三相交流电，驱动电机转动，同时与整车控制器进行实时信息交互，确保新能源汽车安全高效运行","专用安全生产 ","合肥阳光电动力科技有限公司","合肥","合肥高新区","梧桐路88号","何文靓",13635513372]
[9,"化工无泄漏屏蔽电泵","安全防护类","化工管道系统中输送具有腐蚀性、挥发性、易燃性、爆炸性、放射性等有害、有毒及贵重的各种高压、高温、极低温、高融点或含有杂质的液体","化学原料和化学制品制造业","合肥新沪屏蔽泵有限公司","合肥","合肥高新区","杨林路1号","施润霞",13705604998]
[10,"防火墙、存储","安全防护类","防火墙指的是一个有软件和硬件设备组合而成、在内部网和外部网之间、专用网与公共网之间的界面上构造的保护屏障。其作用是信息安全防护。","其他安全防护 ","合肥未来计算机技术开发有限公司","合肥","合肥高新区","创新大道与云飞路交口F1栋3层","史丹媛",15055123101]
[11,"特种车辆机电综合管理系统","安全防护类","对整车电气设备协调、统一管理和控制，实现车辆控制自动化、信息综合化，提升特种车辆在实际使用场合的感知生存能力","铁路、船舶、航空航天和其他运输设备制造业","合肥同智机电控制技术有限公司","合肥","合肥高新区","永和路66号","刘佩",18855125298]
[12,"碰撞防护系统","安全防护类","汽车前防撞系统总成：在汽车受到意外碰撞时的应急处理装置，可吸收中低速碰撞能量，减小车身结构变形量，从而减轻对车上乘员的伤害，保护车上乘员的人身安全","铁路、船舶、航空航天和其他运输设备制造业","合肥腾海汽车零部件有限公司","合肥","合肥高新区","南岗镇响洪甸路与长宁大道","苏丹丹",15255125145]
[13,"MS快速断路器","安全防护类","瞬时切除故障，保障电网及设备安全；避免电压波动，确保生产连续性","专用安全生产 ","合肥麦斯韦舜捷电力科技有限公司","合肥","合肥高新区","明珠产业园5栋B区4楼","李荣",13856056557]
[14,"快速切换装置","安全防护类","针对不直接接地系统，完成快速接地保护、母线电压监测、过电压抑制、异相接地短路故障开断、小电流选线与故障线路跳闸开出等功能","电力、热力、燃气及水生产和供应业","合肥麦斯韦舜捷电力科技有限公司","合肥","合肥高新区","明珠产业园5栋B区4楼","李荣",13856056557]
[15,"电池包充放电测试电源","安全防护类","本测试电源具有短路保护、反接保护、瞬间高压自动保护功能。在电池包维修、快恢复和检测时应急使用","电力、热力、燃气及水生产和供应业","合肥科威尔电源系统股份有限公司企业技术中心","合肥","合肥高新区","大龙山路8号","吴敏",15209899013]
[16,"电池模拟器","安全防护类","电池模拟器具有短路、反接、过流、过热检测和保护功能，设备实时检测异常状态。在新能源汽车检修时可作为动力电池应急使用","专用安全生产 ","合肥科威尔电源系统股份有限公司企业技术中心","合肥","合肥高新区","大龙山路8号","吴敏",15209899013]
[17,"燃料电池发动机测试系统","安全防护类","本系统具有多点氢气泄漏监测、产品实时绝缘检测和强排换气装置，具有独立安全监控回路。通过以上措施，可以充分保证测试过程中的人、产品和设备的安全","专用安全生产 ","合肥科威尔电源系统股份有限公司企业技术中心","合肥","合肥高新区","大龙山路8号","吴敏",15209899013]
[18,"工业在线检测及分析产品","安全防护类","矿山专用安全生产装备，用于矿产品质量监测","采矿业","合肥海明科技股份有限公司","合肥","合肥高新区","创新大道106号明珠产业园3号楼5层A区","程晨",13805691734]
[19,"KJ293（A）矿用轨道运输监控系统","安全防护类","系统是一套用于恶劣环境的分布式工业控制系统。可实现对井下轨道机车运输的区段占用状态检测等功能，指挥矿井机车按规定线路安全高效运行","专用安全生产 ","合肥工大高科信息科技股份有限公司","合肥","合肥高新区","肥西县习友路1682","赵晓云",13966691877]
[20,"KJ303(A)煤矿人员管理（精确定位）系统","安全防护类","该系统主要用于对矿山井下工作人员及移动设备进行定位管理与调度。可对煤矿下井人员进行实时分米级高精度跟踪和定位，便于管理","采矿业","合肥工大高科信息科技股份有限公司","合肥","合肥高新区","肥西县习友路1682","赵晓云",13966691877]
[21,"KJZ21矿井轨道电机车（含单轨吊）无人驾驶系统","安全防护类","系统是一套基于AI技术，面向井下低照度、易爆环境的矿用机车无人驾驶系统。可实现电机车物料矿石装运卸全过程的无人化驾驶作业","专用安全生产 ","合肥工大高科信息科技股份有限公司","合肥","合肥高新区","肥西县习友路1682","赵晓云",13966691877]
[22,"KJZ16矿井胶轮车运输监控系统","安全防护类","系统是一套用于恶劣环境的分布式工业控制系统。可实现胶轮车安全有序行进，防止车辆追尾、相撞等恶性事故的发生","专用安全生产 ","合肥工大高科信息科技股份有限公司","合肥","合肥高新区","肥西县习友路1682","赵晓云",13966691877]
[23,"KJZ17矿井车皮物料自动跟踪及管理系统","安全防护类","系统是一套用于矿山井下车辆识别与跟踪管理的工业监测系统。可实现矿井车辆自动识别、位置跟踪等功能的有机结合。","专用安全生产 ","合肥工大高科信息科技股份有限公司","合肥","合肥高新区","肥西县习友路1682","赵晓云",13966691877]
[24,"车辆迫停系统","安全防护类","针对公共区域驾车问冲关与袭击、犯罪分子驾车逃跑等情况，通过高功率微波的扰乱作用，强迫机动车辆熄火，达到阻止袭击与抓捕的目的","铁路、船舶、航空航天和其他运输设备制造业","合肥博雷电气有限公司","合肥","合肥高新区","香樟大道168号科技实业园C5二层","陈阿松",18755193569]
[25,"无人机管控系统","安全防护类","针对机场、保密机构、大型赛事等场所，对黑飞无人机进行迫降驱离处置，保障重点目标及区域安全","专用安全生产 ","合肥博雷电气有限公司","合肥","合肥高新区","香樟大道168号科技实业园C5二层","陈阿松",18755193569]
[26,"脉冲紫外线杀菌设备","安全防护类","针对海关、物流生鲜集散地、机场、医院等须病毒细菌消杀的公共场所进行物理快速消杀防护","专用安全生产 ","合肥博雷电气有限公司","合肥","合肥高新区","香樟大道168号科技实业园C5二层","陈阿松",18755193569]
[27,"被动式太赫兹人体安检系统","安全防护类","被动式太赫兹人体安检系统应用于地铁等大客流安检，在“无接触、不察觉”情况下，快速完成测温及安检，避免了人群聚集","专用安全生产 ","博微太赫兹信息科技有限公司","合肥","合肥高新区","创新产业园二期F4栋5楼","陈小磊",18005513887]
[28,"过电压保护系统、配电网的智能接地故障管理系统","安全防护类","对配电网运行状态进行实时监控，根据监测信息判定配电网故障的类型并能快速恢复，防范配网发生故障事故","电力、热力、燃气及水生产和供应业","安徽一天电气技术股份有限公司","合肥","合肥高新区","永和路99号","宋琴",15256905101]
[29,"无功补偿及谐波治理装置","安全防护类","专注于无功补偿、谐波治理等电能质量领域的产品研发、生产，产品广泛应用于冶金、汽车制造、石油化工、医院等领域","专用安全生产 ","安徽一天电能质量技术有限公司","合肥","合肥高新区","永和路99号","许善影","0551-62727079"]
[30,"车载记录仪、行车后视镜","安全防护类","采用语音交互、ADAS智能驾驶辅助、胎压监测、数字降噪等技术，实现了智能辅助驾驶，提升了驾驶员及乘客的安全性。可选4G通讯、WIFI连接、手机APP互联，抓拍、视频分享等","专用安全生产 ","安徽协创物联网技术有限公司","合肥","合肥高新区","创新大道99号协创物联网合肥产业园","王兆琪",18255167289]
[31,"安防摄像机","安全防护类","具备先进的高清远程监控、360°无死角摄像、双向语音、人脸识别、哭声报警、移动追踪等技术应用，解决了安防监控问题，实现了远程视频监控，保证了人身及财物安全，提高了监控效率","专用安全生产 ","安徽协创物联网技术有限公司","合肥","合肥高新区","创新大道99号协创物联网合肥产业园","王兆琪",18255167289]
[32,"智能闸机","安全防护类","是一种通道阻挡装置，主要用于交通管理中，规范行人出入，可用于各种收费、门禁场合的入口通道中，用于应急人流管理","专用安全生产 ","安徽三联交通应用技术股份有限公司","合肥","合肥高新区","生物医药园支路","潘婷","0551-65331908"]
[33,"视频监控系统","安全防护类","由摄像、传输、控制、显示、记录登记五大部分组成，可进行车牌识别，车速测量，流量统计等，提升交通应急管理处置水平","专用安全生产 ","安徽三联交通应用技术股份有限公司","合肥","合肥高新区","生物医药园支路","潘婷","0551-65331908"]
[34,"汽车驾驶模拟系统","安全防护类","利用现代高科技手段让体验者在一个虚拟的驾驶环境中，感受到接近真实效果的汽车驾驶体验，适用于研究机构进行汽车工程、交通工程等模拟实验平台，提高同场景应急安全试验能力","专用安全生产 ","安徽三联交通应用技术股份有限公司","合肥","合肥高新区","生物医药园支路","潘婷","0551-65331908"]
[35,"驾驶适应性检测系统","安全防护类","是一种应用现代电子信息及光电机一体化技术，检测机动车驾驶员心理、生理方面是否符合机动车驾驶员身体要求的综合系统。可用于公安交警部门等系统中对驾驶员的测评，提升突发场景应急安全适应能力","专用安全生产 ","安徽三联交通应用技术股份有限公司","合肥","合肥高新区","生物医药园支路","潘婷","0551-65331908"]
[36,"线缆监测系统","安全防护类","该系统主要用于旋转类或往复式设备的状态监测，包括有线采集站、各种类型的传感器、传感器信号线缆、数据传输光缆、系统服务器等。","专用安全生产 ","安徽容知日新科技股份有限公司","合肥","合肥高新区","生物医药园支路59号","罗敏",18949883781]
[37,"稳态监测系统","安全防护类","包括无线监测器、无线通讯站、数据传输光缆（选用）、系统服务器等稳态设备的状态监测","专用安全生产 ","安徽容知日新科技股份有限公司","合肥","合肥高新区","生物医药园支路59号","罗敏",18949883781]
[38,"工业监测设备","安全防护类","主要用于工业企业内部日常的巡检、网络化设备状态监测与故障诊断等专业点检需求，包括精密点检仪、双通道频谱分析仪等","化学原料和化学制品制造业","安徽容知日新科技股份有限公司","合肥","合肥高新区","生物医药园支路59号","罗敏",18949883781]
[39,"散热保护板","安全防护类","核心技术是将散热器的导热风管和锂电池保护板上的导热口互相插接，利用导热口的铝片和导热风管的铝片贴合，便于热量导出，易于大功率保护板的散热，起到安全保护作用","电力、热力、燃气及水生产和供应业","安徽日竞控制技术有限公司","合肥","合肥高新区","云飞路3-1号","单红华",17775338849]
[40,"高清智能布控球","安全防护类","高清智能布控球是一款为无线超高清一体化的便携终端。支持人脸识别、车牌识别、安全帽识别、抽烟检测等智能化应用，可视化巡检、移动执法监控、应急指挥调度、安全生产智能应用等业务管理","铁路、船舶、航空航天和其他运输设备制造业","安徽清新互联信息科技有限公司","合肥","合肥高新区","创新大道2800号创新产业园二期J1区A座","汪莉莉",15375439298]
[41,"智能安全帽","安全防护类","装备可记录作业现场情况、作业行为记录、规范施工等，实时音视频信息传输、语音对讲、本地视频存储等功能，协同后端监控调度指挥平台，实现现场人员的远程调度及指挥，保障施工作业人员安全，同时记录作业现场突发事件的功能","个体防护 ","安徽南瑞继远电网技术有限公司","合肥","合肥高新区","科学大道90号","王丽",18505511291]
[42,"MS系统快切装置","安全防护类","“瞬时”切除故障，保障电网及设备安全；避免电压波动，确保生产连续性","专用安全生产 ","安徽徽电科技股份有限公司","合肥","合肥高新区","合欢路","李荣",13856056557]
[43,"YFC快速真空断路","安全防护类","永磁保持、安全可靠 涡流驱动、快速直接 快速分闸、阻断故障全面领先的技术参数，提高电路应急安全处置水平","电力、热力、燃气及水生产和供应业","安徽徽电科技股份有限公司","合肥","合肥高新区","合欢路","李荣",13856056557]
[44,"BOPET电工膜","安全防护类","绝缘材料，相对电容率为2.9~3.4、体积电阻率为1014~1016Ω·m、直流击穿电压为2.0~2.7kV，具有厚度薄，绝缘性良好，电气强度高，用于直流的电气绝缘薄膜。","专用安全生产 ","安徽国风塑业股份有限公司","合肥","合肥高新区","铭传路1000号","葛芮",13505695276]
[45,"应急救援加热管","安全防护类","电工电器专用安全生产装备，属于基本材料，本产品隶属于应用于电气电工安全设备领域，对于楼体、道路、矿山、河流、等相关领域，在地震、水灾、及暴风，山体滑坡，火灾等相关领域其机械化救援方面应用具有极高的应用作用","电力、热力、燃气及水生产和供应业","安徽国安电气股份有限公司","合肥","合肥高新区","磨子潭路01588号","刘兰琳",18949811580]
[46,"三维环视实景系统","安全防护类","车辆专用安全生产装备、交通专用安全生产装备、安防专用安全生产装备，主要防范灾害的发生，及安全隐患消除，应用于现代交通领域的安全防控，安全应急，安全救治，安全预防等方面","电力、热力、燃气及水生产和供应业","安徽富煌科技股份有限公司","合肥","合肥高新区","骆岗街道五台山路77号富煌新视觉A座","黄兴亮",18255129910]
[47,"视频监控系统","安全防护类","车辆专用安全生产装备、交通专用安全生产装备、安防专用安全生产装备监控是各行业重点部门或重要场所进行实时监控的物理基础，管理部门用以提供高效、及时地指挥和高度、布置警力、处理案件等。","专用安全生产 ","安徽富煌科技股份有限公司","合肥","合肥高新区","骆岗街道五台山路77号富煌新视觉A座","黄兴亮",18255129910]
[48,"无线高清布控球","安全防护类","安防专用装备，支持无线高清音视频传输、图像传输、车辆及人脸识别，内置高性能锂电池组，可以实现快速布控、一键报警联动","专用安全生产 ","安徽创世科技股份有限公司","合肥","合肥高新区","黄山路622号信息产业基地软件研究中心b座","黄燕","0551-65898200"]
[49,"记录仪","安全防护类","安防专用装备，可以摄录、照相、录音，拥有夜视功能、北斗/GPS定位功能、激光定位功能等","专用安全生产 ","安徽创世科技股份有限公司","合肥","合肥高新区","黄山路622号信息产业基地软件研究中心b座","黄燕","0551-65898200"]
[50,"智能视频监控系统软件","安全防护类","安防专用系统，智能视频监控系统是采用图像处理、模式识别和计算机视觉技术，快速准确的定位事故现场，判断监控画面中的异常情况，并以最快和最佳的方式发出警报或触发其它动作，从而有效进行事前预警、事中处理、事后及时取证","铁路、船舶、航空航天和其他运输设备制造业","安徽创世科技股份有限公司","合肥","合肥高新区","黄山路622号信息产业基地软件研究中心b座","黄燕","0551-65898200"]
[51,"汽车门铰链/行李箱铰链","安全防护类","汽车门铰链是确定车门与车身的相对位置，并能控制车门运动轨迹的装置，它加工精度高，可有效保证产品强度和安全应急。\n汽车行李箱铰链是通过铰链连接轴固定车身件和罩上件的装置，它加工精度高，可有效保证产品强度和安全应急。","安全材料 ","安徽爱德夏汽车零部件有限公司","合肥","合肥高新区","玉兰大道1号","冯伟",13349114255]
[52,"陶瓷衬垫","安全防护类","陶瓷衬垫耐火、隔热性能优异，用于消除火灾隐患","安全材料 ","3M材料技术（合肥）有限公司","合肥","合肥高新区","习友路3588号","陈绮",13866109574]
[53,"负折射平板透镜","安全防护类","一种具有负折射功能的新型材料，可将发散的光线在空中重新汇聚，从而形成不需要介质承载的实像，结合交互控制技术，可实现人与空中实像的直接交互。可广泛应用于医疗显示、智能车载、信息安全、公共设施等领域","专用安全生产 ","安徽省东超科技有限公司","合肥","合肥高新区","望江西路900号","李国文",17355888808]
[54,"无接触电梯按钮终端","安全防护类","用户可直接于空中操控电梯按钮，整体过程中均不存在任何接触。交互响应灵敏，成像更具科技感，使用过程稳定、安全、可靠","建筑业","安徽省东超科技有限公司","合肥","合肥高新区","望江西路900号","李国文",17355888808]
[55,"无接触自助终端","安全防护类","无需屏幕等介质，即可将设备操作界面呈现于空中，用户可直接在空中操作设备，完成预约、挂号、缴费、支付等所有流程，有效隔绝了因人体与物体表面接触时产生的细菌和病毒感染，提供零交叉感染的安全交互体验","专用安全生产 ","安徽省东超科技有限公司","合肥","合肥高新区","望江西路900号","李国文",17355888808]
[56,"网络安全检测系统-人脸认证","安全防护类","人脸认证旨在帮助客户实现人脸门禁等项目落地，助力公共场所的安全现代化、管理现代化，减少人力成本，增加智能化场景的价值和效益","个体防护 ","科大国创云网科技有限公司","合肥","合肥高新区","文曲路355号办公楼4层","陈娇娇",18055160556]
[57,"安防监控系统","安全防护类","安防监控系统可以实现事前预警、实时显示、事后追踪，是应急安全监控的有力手段","道路运输业","合肥未来计算机技术开发有限公司","合肥","合肥高新区","创新大道与云飞路交口F1栋3层","史丹媛",15055123101]
[58,"危化品运输、仓储及现场处置一体化监管系统","安全防护类","危化品运输仓储及现场处置一体化监管系统旨在实现危化品存储、运输及现场处置一体化监管理。","社会安全事件监测预警 ","安徽清新互联信息科技有限公司","合肥","合肥高新区","创新大道2800号创新产业园二期J1区A座","汪莉莉",15375439298]
[59,"巡检机器人","安全防护类","运用导航定位、运动控制、5G通信等技术，在特殊场景中代替人工，保障人身安全，提升巡检效率","采矿业","科大智能电气技术有限公司","合肥","合肥高新区","望江西路5111号","刘丹",18356289296]
[60,"汽车用防护安全气囊","安全防护类","DAB主驾驶气囊，PAB副驾驶气囊，SAB侧气囊，CAB气帘，可应用于突发事故时对人员人身安全的保护","专用安全生产 ","合肥江淮太航常青汽车安全系统有限公司","合肥","合肥经开区","佛掌路东耕耘路北1#标准化厂房一、二、三层西","沈燕","18656989229"]
[61,"熔喷布、阻燃塑料粒子等各类新材料","安全防护类","阻燃塑料粒子等材料，是防护类用品的重要原材料，同时本公司生产的熔喷布是医用防护口罩的核心材料","安全材料 ","合肥杰事杰新材料股份有限公司","合肥","合肥经开区","莲花路2388号","郝鑫楼","18655180181"]
[62,"医用防护服、隔离衣","安全防护类","本产品可用于公共卫生领域的医疗防护，实现医护人员与病人的有效隔离","安全材料 ","华润纺织（合肥）有限公司","合肥","合肥经开区","莲花路","赵春雨","15055169603"]
[63,"医用防护服、隔离衣","安全防护类","本产品可用于公共卫生领域的医疗防护，实现医护人员与病人的有效隔离","安全材料 ","安徽汇源制衣有限责任公司","合肥","合肥经开区","丹霞路107号2号楼1层","张新茹","13695655728"]
[64,"医用防护服、隔离衣","安全防护类","本产品可用于公共卫生领域的医疗防护，实现医护人员与病人的有效隔离","安全材料 ","合肥联亚制衣有限公司","合肥","合肥经开区","紫蓬路2886号","徐东","17705694472"]
[65,"医用外科口罩","安全防护类","供临床医务人员在有创操作过程中佩带，覆盖住使用者的口、鼻及下颌，为防止病原体、微生物、体液、颗粒物等的直接透过提供物理屏障","安全材料 ","安徽瑞德医疗设备制造有限公司","合肥","合肥经开区","宿松路以西观海路以南瑞德医疗产业园4#、5#厂房","钱月梅","15956984541"]
[66,"非医用口罩","安全防护类","适用于在日常生活中空气污染环境下滤除颗粒物所佩带的防护型口罩","安全材料 ","安徽瑞德医疗设备制造有限公司","合肥","合肥经开区","宿松路以西观海路以南瑞德医疗产业园4#、5#厂房","钱月梅","15956984541"]
[67,"防冲撞驾驶舱","安全防护类","为应用于救援抢险的挖掘机等工程机械提供防冲撞驾驶舱，可对驾驶人员提供充分的安全防护，避免受到溅落、冲击等伤害","专用安全生产 ","合肥二宫机械有限公司","合肥","合肥经开区","卧云路152号","孙悦","19855811406"]
[68,"清华合肥院熠能星安全文教体验馆","安全防护类","清华合肥院熠能星安全文教体验馆是安全文化教育研究发展中心对外传播安全文化的重要平台。体验馆重点面向青少年群体，以“一天的安全生活”为故事线索，紧密围绕居家安全、交通安全、校园安全三大主题设置近20个展项，综合运用多媒体、虚拟现实、人机交互等先进技术手段，为观众开启一场安全之旅","专用安全生产 ","辰安云服技术有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院2号楼4层","梁光华","13911763375"]
[69,"室内防火舱","安全防护类","内置多层隔热层，集火灾避险、隐秘藏身、物品储藏等多功能于一体","专用安全生产 ","安徽百世伽德安防科技有限公司","合肥","合肥经开区","九龙路168号东湖创新中心18-2-503室","胡可可","19856552593"]
[70,"消毒水等消毒用品","安全防护类","为公共场所、密闭空间实现快速消毒等目的而制造的各类消毒用品","个体防护 ","合肥诚志生物制药有限公司","合肥","合肥经开区","汤口路与青鸾路口","张利","18756938760"]
[71,"手术室及ICU净化系统工程","安全防护类","可用于医院手术室及ICU等重要场所的空气净化系统","专用安全生产 ","安徽华亿医疗净化工程有限公司","合肥","合肥经开区","繁华大道与九龙路交叉口东湖创新中心17幢801号","李玉茹","13956999613"]
[72,"气凝胶毡","安全防护类","气凝胶毡产品是利用专有技术，将纳米多孔气凝胶与纤维材料复合而成的一种柔软、疏水、高温稳定、防火阻燃、不掉粉绝热保温毡。产品广泛应用于航空航天、军事国防、石化管道、建筑保温、电力电网、车辆运输、冷藏冷链、日常保温等诸多领域。","安全材料 ","安徽弘徽科技有限公司","合肥","安巢经开区","巢湖市成芳路与振兴路交叉路口往东北约120米","朱孟伟",18551027716]
[73,"玻璃纤维毡","安全防护类","玻璃纤维毡是以玻璃纤维为原料，采用针刺的制备工艺，将玻璃纤维毡层之间交错排列并相互缠结，使得纤维毡层得以加固而制成毡状绝热保温材料，广泛应用于管道保温、建筑保温隔音、交通防火隔热、电器设备等领域。","安全材料 ","安徽弘徽科技有限公司","合肥","安巢经开区","巢湖市成芳路与振兴路交叉路口往东北约120米","朱孟伟",18551027716]
[74,"氢氧化铝阻燃剂","安全防护类","主要成分为AL(OH)3,适用于橡胶、塑料制品等阻燃领域，如矿用运输带、矿用导风筒涂覆布、胶管、胶板、地毯、电线电缆护套、皮革、防火板、建筑材料、阻尼板，阻尼膏、电子等","采矿业","合肥中科阻燃新材料有限公司","合肥","肥东县","肥东县经开区祥和路36号","王英琦",13956967206]
[75,"氢氧化镁阻燃剂","安全防护类","主要成分为Mg(OH)2,是近几年来研究开发的一种新型填充型阻燃剂，广泛应用于橡胶、化工、建材、塑料、红磷母料，及电子、不饱和聚酯和油漆、涂料等高分子材料","安全材料 ","合肥中科阻燃新材料有限公司","合肥","肥东县","肥东县经开区祥和路36号","王英琦",13956967206]
[76,"沥青阻燃剂","安全防护类","公路隧道铺装沥青混凝土专用无卤环保阻燃剂。具有阻燃、消烟、无毒、耐寒耐热、不易析出、宜分散、热稳定性好等优点","安全材料 ","合肥中科阻燃新材料有限公司","合肥","肥东县","肥东县经开区祥和路36号","王英琦",13956967206]
[77,"新型无卤环保阻燃剂","安全防护类","针对乳胶制品、胶水、建材、防火板等使用的新型无卤环保阻燃剂。有阻燃、消烟、填充、耐寒耐热、热稳定性好等优点","安全材料 ","合肥中科阻燃新材料有限公司","合肥","肥东县","肥东县经开区祥和路36号","王英琦",13956967206]
[78,"木材、织物阻燃剂","安全防护类","木材、织物专用无卤环保阻燃剂可根据木材、织物、稻草的阻燃氧指数、工艺等调整用量，将该阻燃剂制成20%-30%的溶液，直接喷涂（必须喷透）或浸泡其中（约10-30分钟）后直接自然晾干即可","安全材料 ","合肥中科阻燃新材料有限公司","合肥","肥东县","肥东县经开区祥和路36号","王英琦",13956967206]
[79,"人造革专用阻燃剂","安全防护类","该阻燃剂具有优越的渗透性、无毒、无腐蚀性、不变色、热稳定性好等优点。特别适用于PVC、PU、超纤革基布阻燃处理，处理工艺简单，易操作，该阻燃剂在人造革材料中还起到一定阻燃抑烟的效果，无滴落，是一种理想的高效无卤阻燃剂","安全材料 ","合肥中科阻燃新材料有限公司","合肥","肥东县","肥东县经开区祥和路36号","王英琦",13956967206]
[80,"油烟净化机组","安全防护类","该产品采用机械离心分离、金属及非金属丝网吸附、消声等处理技术，将油烟气进 行综合高效捕集，使油烟气混合污染物聚集后吸附到过滤层，达到高效净化，主要实用于宾馆、饭店、酒家、餐厅、食堂及商业综合体和美食街餐饮场所的油烟污染气体的净化治理，能有效减少空气污染","安全材料 ","安徽国茂机电设备有限公司","合肥","肥东县","肥东龙塘工业区","邱灵洁",15209888896]
[81,"安全帽","安全防护类","采用ABS或玻璃钢材质，具有极好的冲击强度、尺寸稳定性、电绝缘性好，耐磨性、抗化学品性较好。用于建筑安装冶金冶炼、石油化工、电力煤炭、港口港务、造船重工、矿山矿井、运输装卸、林业消防等作业场所","个体防护 ","安徽省富光实业股份有限公司","合肥","肥西县","肥西县三河镇","杨二云",15155945986]
[82,"均质改性防火保温板","安全防护类","均质改性防火保温板是有机材料和无机材料双结合制成A级不燃产品。主要应用于新建、扩建、改建的居住建筑和公共建筑外墙的节能保温工程","化学原料和化学制品制造业","合肥神舟建筑集团有限公司","合肥","肥西县","肥西县花岗镇工业园区","江玲",13866175988]
[83,"医用外科口罩","安全防护类","供临床医务人员在有创操作过程中佩带，覆盖住使用者的口、鼻及下颌，为防止病原体、微生物、体液、颗粒物等的直接透过提供物理屏障","个体防护 ","安徽省锦瑞汽车部件有限公司","合肥市","肥西县","经开区桃花工业园桥湾路1号","朱冬冬",13155192172]
[84,"防静电材料","安全防护类","该产品添加入塑料中可以避免由于高聚物本身的绝缘性能而产生的静电从而使其能够适应IT产品、医疗手术环境要求和特殊抗静电制品的生产，对于制品的表面防尘有良好效果。","专用安全生产 ","合肥丽红塑胶材料有限公司","合肥","长丰县","下塘工业园纬五路","张文东",13505610701]
[85,"防颗粒物材料","安全防护类","熔喷料是熔喷布原材料。空隙多、结构蓬松、抗褶皱能力好，具有独特的毛细结构的超细纤维增加单位面积纤维的数量和表面积.可用于空气、液体过滤材料、隔离材料、吸纳材料、口罩材料、保暖材料、吸油材料及擦拭布等领域","专用安全生产 ","合肥丽红塑胶材料有限公司","合肥","长丰县","下塘工业园纬五路","张文东",13505610701]
[86,"防火阻燃材料","安全防护类","阻燃材料是能够抑制或者延滞燃烧而自己并不容易燃烧的材料，广泛应用于服装、石油、化工、冶金、造船、消防、国防等领域。","化学原料和化学制品制造业","合肥丽红塑胶材料有限公司","合肥","长丰县","下塘工业园纬五路","张文东",13505610701]
[87,"安全网","安全防护类","密目式安全立网，垂直于水平面安装，用于阻挡人员、视线、自然风、飞溅及失控小物体的网，简称为密目网，由网体、开眼环扣、边绳和附加系绳组成。材质：聚乙烯。","专用安全生产 ","合肥新大唐工贸有限公司","合肥","长丰县下塘镇","长丰县下塘镇下塘工业园","唐正义",13866755500]
[88,"密目式安全立网","安全防护类","安全网用于防止人、物坠落，或用于避免、减轻坠落及物击伤害的网具，安全网采用锦纶、维纶、涤纶或其他的耐侯性不低于上述品种（耐侯性）的材料制成。","专用安全生产 ","合肥新大唐工贸有限公司","合肥","长丰县下塘镇","长丰县下塘镇下塘工业园","唐正义",13866755500]
[89,"高倍率18650防爆电池","安全防护类","特种设备、通信装置、特种机器人等领域使用的锂离子蓄电池组和电芯，-25摄氏度放电容量不低于额定容量的75%，循环使用应大于400次","电力、热力、燃气及水生产和供应业","合肥众禾动力新能源科技有限公司","合肥","庐江县","庐江县高新区移湖西路58号","徐继胜",15255638898]
[90,"应急发电设备（锂离子圆柱电池）","安全防护类","单体效能高，通过串并联可以形成电池模组，具有应急发电作用","专用安全生产 ","国轩新能源（庐江）有限公司","合肥","庐江县","庐江县城西大道111号","刘瑞",18919666543]
[91,"水泥基渗透结晶型防水涂料","安全防护类","水泥基渗透结晶型防水涂料是一款专用于混凝土基层的刚性防水涂料，主要应用于大型混凝土结构防水","建筑业","安徽朗凯奇防水科技股份有限公司","合肥","庐江县","庐江县同大镇马河路18号","朱华林",13866128353]
[92,"聚合物防水涂料","安全防护类","产品是由德国进口高性能合成丙烯酸乳液和无机聚合物干粉复配而成的双组份产品。具有优良的抗渗、防腐、粘结性能。","专用安全生产 ","安徽朗凯奇防水科技股份有限公司","合肥","庐江县","庐江县同大镇马河路18号","朱华林",13866128353]
[93,"应急发电设备（移动电池系统应急电源）","安全防护类","新能源便携式锂电池储能系统应急供电方案，无噪音、无污染，快速应急供电的一套安全应急电源系统。用途：手机等电器充电，照明，发电机","电力、热力、燃气及水生产和供应业","安徽潜川动力锂电科技有限公司","合肥","庐江县","磙桥路196号","傅钊",13355651568]
[94,"自动变黑滤镜电焊头盔","安全防护类","焊接防护，变光变色，保护眼睛","专用安全生产 ","安徽恒裕光电有限公司","合肥","庐江县","庐城镇移湖北路232号","孙业宏","0551-87306357"]
[95,"发电机","安全防护类","发电效率高、温升低、波形畸变率低、动态性能好、AVR 并联运行稳定、与各种动力系统匹配良好等优点。广泛应用于油田矿山、国防军工等行业","电力、热力、燃气及水生产和供应业","安徽德科电气科技有限公司","合肥","庐江县","庐江高新技术产业开发区苏河路9号","丁惠林",15256525200]
[96,"锚链","安全防护类","用于航标配套固定、船舶配套，是连接锚和船体之间的链条，用来传递和缓冲船舶所受的外力","专用安全生产 ","巢湖群力船用锚链有限公司","巢湖市","巢湖市","中垾镇","徐朝进",13605656190]
[97,"锚链","安全防护类","用于航标配套固定、船舶配套，是连接锚和船体之间的链条，用来传递和缓冲船舶所受的外力","专用安全生产 ","安徽凤凰机械有限公司","巢湖市","巢湖市","烔炀镇","蒋世林",13705656553]
[98,"锚链","安全防护类","该产品广泛运用在江湖航道上起助航作用；还应用在近海远洋作为环境气象监测平台。从大趋势看，由于绿色环保高分子航标逐步取代钢质航标","专用安全生产 ","安徽省巢湖市凤凰锚链有限公司","巢湖市","巢湖市","烔炀镇","徐占发",13705657788]
[99,"锚链","安全防护类","主要由钢板,型材,电机,减速构成,技术参照JB-T 3926.1-1999用于提升输送设备,下游客户类型有建材,冶金,钢厂,化工","专用安全生产 ","安徽星辉工业科技有限公司","巢湖市","巢湖市","中垾镇","祝善辉",13905652693]
[100,"锚链","安全防护类","用于和船体、航标、水上平台的连接，公司产二级锚链经过正火处理，三级锚链经过调质处理，其拉力强度大、韧性大，适用大吨位，大负荷平台的需要","专用安全生产 ","安徽亚太锚链制造有限公司为锚链企业","巢湖市","巢湖市","凤凰山街道","张平",13956661980]
[101,"防火窗","安全防护类","该产品安装在防火墙或者防火隔墙上，具有一定的耐火完整性，满足GB16809-2008标准的全部要求：外观质量、防火玻璃、尺寸偏差、抗风压性能、气密性能、耐火性能等指标","建筑业","安徽钟南消防科技有限公司","合肥","包河区","徽商总部广场A座17层","涂  蓓",18755161509]
[102,"医用外科口罩","安全防护类","该产品由口罩体、鼻夹及口罩带组成，材料为无纺布、熔喷布、耳带和鼻梁条。覆盖住使用者的口、鼻及下颌，为防止病原体、微生物、体液、颗粒物等的直接透过提供物理屏障","个体防护 ","安徽电气集团股份有限公司","合肥","包河区","雨雾山路6号","罗雪",13855129654]
[103,"低压开关柜JXF","安全防护类","本装置主要用于三相四线制供电，交流50Hz、额定电压380V、低压侧中心点接地的变压器低压侧馈电、控制、计量及保护。本装置用于户外，更可用于户内","电力、热力、燃气及水生产和供应业","安徽华兴电器开关有限公司","合肥","庐阳区","庐阳经开区秀水路4号","卢先明",18326068869]
[104,"高压开关柜","安全防护类","涉及一次和二次设备成套组装的一种高压配电装配。其主要是电厂和变配电所中作为节制和保护发机电，电力变压器和高压线路之用","专用安全生产 ","合肥开关厂有限公司","合肥","庐阳区","庐阳经开区阜阳北路1011号","卞文群",18856030522]
[105,"低压开关柜","安全防护类","按一定的接线方案将涉及低压开关电器成套组装的一种低压配电装配。在1kv以下的供电体系中作为动力和照明电之用","专用安全生产 ","合肥开关厂有限公司","合肥","庐阳区","庐阳经开区阜阳北路1011号","卞文群",18856030522]
[106,"矿用防爆电气设备","安全防护类","专供煤矿使用。适用于煤矿低瓦斯高瓦斯和有煤尘与瓦斯突出喷出的区域","石油、煤炭及其燃料加工业","合肥开关厂有限公司","合肥","庐阳区","庐阳经开区阜阳北路1011号","卞文群",18856030522]
[107,"转向助力油泵","安全防护类","油泵主要部件采用铝合金材料，采用耐磨、补偿、降噪、限压限流等技术，辅助车辆实现轻松转向。用于工程机械的汽车，如卡车、吊车、客车、特种车等","道路运输业","合肥力威汽车油泵有限公司","合肥","庐阳区","庐阳经开区汲桥路53号","史芳婷",18356536939]
[108,"一次性使用医用口罩","安全防护类","供临床各类人员在非有创操作过程中佩带，覆盖住使用者的口、鼻及下颌，为防止病原体微生物、颗粒物等的直接透过提供一定的物理屏障","个体防护 ","安徽盈科安防装备有限公司","淮北","濉溪县","濉溪县濉芜产业园苏铁路与银桦路交叉口","马  超",18949562222]
[109,"一次性医用防护服","安全防护类","适用于医务人员工作时接触具有潜在感染性的患者血液、体液、分泌物、空气中的颗粒物等提供阻隔、防护作用","个体防护 ","安徽盈科安防装备有限公司","淮北","濉溪县","濉溪县濉芜产业园苏铁路与银桦路交叉口","马  超",18949562222]
[110,"防火门","安全防护类","一定时间内能满足耐火稳定性、完整性和隔热性要求的门。更具有阻止火势蔓延和烟气扩散的作用，可在一定时间内阻止火势的蔓延，确保人疏散","建筑业","安徽盈科安防装备有限公司","淮北","濉溪县","濉溪县濉芜产业园苏铁路与银桦路交叉口","马  超",18949562222]
[111,"JS防水涂料","安全防护类","JS防水涂料是以高弹性、高分子有机液料和无机粉料按一定比例复合而成的防水涂料，尤其适用于道路及桥梁防水工业及民用建筑的屋面防水；厕浴间、厨房防水、防潮工程；墙面、地下室、游泳池、槽罐的防水等","专用安全生产 ","安徽尊龙环保节能建材有限公司","淮北","相山区","经济开发区凤池路与栖凤路交叉口东北100米","许  慎",18956180067]
[112,"结晶防水涂料","安全防护类","结晶防水涂料是引进国际先进技术生产的绿色环保的新型刚性防水材料。用于地下隧道、地下涵洞、地下砼或钢砼管道、地下室、、人防工程、屋面、浴厕间、污水池、饮用水池、游泳池、水坝、船闸、港口码头、屋顶花园等新建工程的防水施工","专用安全生产 ","安徽尊龙环保节能建材有限公司","淮北","相山区","经济开发区凤池路与栖凤路交叉口东北100米","许  慎",18956180067]
[113,"聚氨酯防水涂料","安全防护类","水性聚氨酯防水涂料是一种高弹性彩色高分子纳米防水材料是以防水专用的自交联纯丙乳液。用于地下工程、隧道、桥梁、水库等;潮湿或干燥的混凝土、金属、彩钢瓦等基面上直接施工","专用安全生产 ","安徽尊龙环保节能建材有限公司","淮北","相山区","经济开发区凤池路与栖凤路交叉口东北100米","许  慎  ",18956180067]
[114,"室内厚型钢结构防火涂料","安全防护类","室内厚型钢结构防火涂料由高强度粘接剂，阻燃纤维；耐高温材料；隔热材料等原材料经先进工艺制备而成。适应于工业民用建筑、宾馆、写字楼、商场、发电厂及大跨度厂房等建筑物","专用安全生产 ","安徽尊龙环保节能建材有限公司","淮北","相山区","经济开发区凤池路与栖凤路交叉口东北100米","许  慎",18956180067]
[115,"室内超薄型钢结构防火涂料","安全防护类","室内超薄型钢结构防火涂料以有机合成树脂做基料，添加新型阻燃剂、发泡剂、成碳剂及各种助剂经先进工艺制备而成。广泛适用于民用、工业高层建筑、体育场馆等建筑物室内或隐蔽工程的钢结构防火","建筑业","安徽尊龙环保节能建材有限公司","淮北","相山区","经济开发区凤池路与栖凤路交叉口东北100米","许  慎",18956180067]
[116,"隧道防火涂料","安全防护类","隧道防火涂料主要原材料采用于多孔型隔热材料，与无机绝热材料组成，该产品无毒、不燃、耐冻融、耐酸碱、耐潮湿、抗老化等优良的理化性能，具有重量轻耐腐蚀、隔热性等特点","专用安全生产 ","安徽尊龙环保节能建材有限公司","淮北","相山区","经济开发区凤池路与栖凤路交叉口东北100米","许  慎",18956180067]
[117,"一次性医用口罩","安全防护类","用于医务人员和相关工作人员对经空气传播的呼吸道传染病的防护","个体防护 ","淮北新兴皇苑制衣有限公司","淮北","濉溪县","濉溪县濉溪经济开发区白杨路2号","肖国臣",18705610196]
[118,"医用防护服","安全防护类","用于液体阻隔、微生物阻隔和对颗粒物质的阻隔等方面","个体防护 ","淮北新兴皇苑制衣有限公司","淮北","濉溪县","濉溪县濉溪经济开发区白杨路2号","肖国臣",18705610196]
[119,"活性炭","安全防护类","产品选用优质炭化料，采用物理活化法制成，为黑色颗粒状、粉状、蜂窝状等，无毒无味，具有吸附能力强，过滤速度快等优点，广泛用于饮用水的提纯净化及工业废水、污水、江河污水水质的除臭净化、深度改良以及工业废气的脱硫等","安全材料 ","淮北市洁力活性炭有限责任公司","淮北","濉溪县","濉溪县濉溪经济开发区巴河路","徐敬东",13909617018]
[120,"丁腈手套","安全防护类","弹性好、拉伸性强、耐酸碱、耐油性、抗静电、无过敏性，用于医用检查、简单医疗手术、食品加工、化工电子等","安全材料 ","安徽英科医疗用品有限公司","淮北","濉溪县","濉溪县濉芜产业园海棠南路6号","牛  兢",18956120101]
[121,"PVC手套","安全防护类","产品穿戴容易、透气性好，可用于医用检查、食品加工、化工电子、清洁卫生","安全材料 ","安徽英科医疗用品有限公司","淮北","濉溪县","濉溪县濉芜产业园海棠南路6号","牛  兢",18956120101]
[122,"活性炭","安全防护类","产品选用优质炭化料，采用物理活化法制成，为黑色颗粒状、粉状、蜂窝状等，无毒无味，具有吸附能力强，过滤速度快等优点，广泛用于饮用水的提纯净化及工业废水、污水、江河污水水质的除臭净化、深度改良以及工业废气的脱硫等","安全材料 ","淮北市森化碳吸附剂有限责任公司","淮北","杜集区","淮北市杜集区腾飞路6号","李  森",13856106633]
[123,"电缆附件","安全防护类","连接各种规格大小不同的电缆、保护高低压配电柜里裸露的线端","电力、热力、燃气及水生产和供应业","安徽伊法拉电力科技有限公司","亳州","亳芜园区","亳芜现代产业园汤王大道以西纬三路以南","戴冕",15814268765]
[124,"锌合金门、不锈钢门","安全防护类","锌合金门、不锈钢门具有防火、防盗作用，适用于住宅、办公等场合","建筑业","安徽智扬门业股份有限公司","亳州","蒙城县","蒙城县经济开发区南区庄子大道396号","侯伟峰",13966511786]
[125,"建筑模板、铝合金模板","安全防护类","铝合金模板：用于高层建筑防护、具有安全环保防火、安全施工、混凝土施工过程中组装简单快捷环保、承载力高、稳定性好、施工环境安全、干净、整洁","建筑业","安徽中嘉环保建材科技有限公司","亳州","蒙城县","蒙城县经济开发区庄子大道南段333号","李冬冬",15556770692]
[126,"非医用口罩","安全防护类","具有低抗液体、过滤细小颗粒物和细菌等效用","个体防护 ","安徽新亳华扬服饰有限公司","亳州","谯城区","谯城区大杨镇交警中队北侧","宁坤",15551535333]
[127,"非医用应急防护服","安全防护类","具有良好的透湿性和阻隔性，能有效抵抗酒精、血液、空气粉尘、细菌的渗透","个体防护 ","安徽新亳华扬服饰有限公司","亳州","谯城区","谯城区大杨镇交警中队北侧","宁坤",15551535333]
[128,"免洗手消毒凝胶","安全防护类","本产品是将黄芩、金银花等中药材作为生产杀菌消毒的主要成份，可杀灭肠道致病菌，化脓性球菌和医院感染常见细菌","个体防护 ","安徽天马生物科技有限公司","亳州","亳芜园区","亳芜园区汤王大道与月季路交叉口","苏晓松",13170177982]
[129,"消杀防疫产品","安全防护类","中药多功能消毒剂，免洗手消毒液等。 适用于外科手消毒和卫生手消毒及皮肤消毒，能高效杀菌、快速洁净、不伤手，科学配比，安全防护，有效杀菌率可达99.99%","个体防护 ","安徽亿人安股份有限公司","亳州","高新区","亳州经济开发区亳菊路916号","支允坤",15178078989]
[130,"一次性医用口罩","安全防护类","用途：用于佩戴者在不存在体液和喷溅风险的普通医疗环境下的卫生护理","个体防护 ","利辛县富亚纱网有限公司","亳州","利辛县","利辛县经开区永兴路8号","朱亚军",13856737777]
[131,"非医用口罩","安全防护","主要用于防止有毒有害粉尘颗粒、污染物进入呼吸器官的防护用品","个体防护 ","宿州市鸿正服装服饰有限公司","宿州","埇桥区","北二环路鸿正服装工业园","韩斌",18905577905]
[132,"附着式升降爬架","安全防护","用于高层建设施工主体防护，对于超载、超限和其他异常情况进行预警并自动断电停机","专用安全生产 ","安徽省标诺建筑科技有限公司","宿州","埇桥区","埇桥区汴河东路与龙华路交叉口","杨孝飞",13866548966]
[133,"非医用口罩","安全防护","主要用于防止有毒有害粉尘颗粒、污染物进入呼吸器官的防护用品","个体防护 ","宿州市福瑞诗医疗器械有限公司","宿州","埇桥区","宿州市埇桥区符离镇","祝业超",13705573372]
[134,"防火门","安全防护","用于建筑物隔离、隔热、防火、阻燃","专用安全生产 ","安徽省宿州市王中王门业有限公司","宿州","埇桥区","汴河办事处北十里家具工业园","王飞",17705571588]
[135,"架空乘人装置","安全防护","用于自动运输人员的井下缆车，可远程监测控制，具有自动预警和自动保护功能","采矿业","宿州华征矿业设备有限公司","宿州","埇桥区","埇桥区朱仙镇庄新河村","赵崇明",13395576661]
[136,"防火阻燃反光材料","安全防护","该阻燃反光布主要用于防火及安全救援，可用于火场反光警示标志。","专用安全生产 ","安徽硕明安全科技有限公司","宿州","埇桥区","开发区曹村镇三环村","丁咚",18095691888]
[137,"隔离衣","安全防护类","采用非织造布为主要原料，经裁剪，热合制成。非无菌提供，一次性使用。","个体防护 ","安徽德大康美医疗用品有限公司","宿州","开发区","磬云南路与鞋城三路交叉口鞋城标准化厂房","上官苗苗",18734034608]
[138,"一次性防滑袜","安全防护类","纱线为主要原料，经针织，点塑制成，一次性使用，非灭菌","个体防护 ","安徽德大康美医疗用品有限公司","宿州","开发区","磬云南路与鞋城三路交叉口鞋城标准化厂房","上官苗苗",18734034608]
[139,"矿用隔爆型移动变电站","安全防护类","用于有甲烷混合气体和煤尘，并有爆炸危险的矿井中，作为煤矿井下综合机械化采掘设备的配电装置","采矿业","电光防爆电气（宿州）有限公司","宿州","开发区","开发区金河路18号","周磊磊","0557-3932888"]
[140,"焊接机器人","安全防护类","能够直接或间接防止机械或机电工作设备对人体安全或他种工作设备产生危害的专用安全设备","电力、热力、燃气及水生产和供应业","安徽悦得自动化有限公司","宿州","砀山县","砀山县经济开发区","周爽",17355731991]
[141,"配电装置","安全防护类","能够直接或间接防止电子电工工作设备对人体安全或他种工作设备产生危害的专用安全设备","电力、热力、燃气及水生产和供应业","安徽耐得电气设备有限公司","宿州","砀山县","砀山县经济开发区","周爽",17355731992]
[142,"阻燃光缆","安全防护类","具有防止或阻止火焰蔓延性能的材料","采矿业","安徽兴华电缆有限公司","宿州","砀山县","砀山县经济开发区","仇宇",18105579325]
[143,"医用转运车","安全防护类","由床面（推车面板、担架面）、支撑架组成。附加输液架、护栏、脚轮、刹车、手摇机构。为单车。无源产品。用于医疗机构运送、移动患者。","专用安全生产 ","安徽省江海医疗器械有限公司","宿州","灵璧县","灵璧县下楼镇工业园区","徐玉",18952292269]
[144,"隔离衣","安全防护类","采用非织造布为原料，经裁减、缝纫制成非无菌一次性长袍式或连体式身体防护服。隔离衣用于门诊、病房、检验室等普通隔离，或用于防疫防控人员的普通隔离防护。","个体防护 ","宿州千鹤卫生用品有限公司","宿州","灵璧县","灵璧县南部开发区平山路东奇石大道南","张利",18656818990]
[145,"防静电帽","安全防护类","具有防静电防尘效果，防止头发掉入净化车间，防静电帽子不发尘，不吸尘，耐洗涤。款式有防静电鸭舌帽、防静电披肩帽。","专用安全生产 ","宿州先进服饰","宿州","灵璧县","灵壁县南部开发区","姜毅/刘凯",13916447558]
[146,"防尘帽","安全防护类","1.防尘的作用，可加披肩。\n2.防止头部、面部、颈部受到灰尘的伤害及长头发被机器皮带卷入，防止脱落的头发、头皮掉入生产产品内。","专用安全生产 ","宿州先进服饰","宿州","灵璧县","灵壁县南部开发区","姜毅/刘凯",13916447558]
[147,"防尘帽","安全防护类","是一种防电磁辐射帽,包括防护层,在防护层内表面设置有防电磁辐射屏蔽层,兼具防电磁辐射的功能.","专用安全生产 ","宿州先进服饰","宿州","灵璧县","灵壁县南部开发区","姜毅/刘凯",13916447558]
[148,"防尘帽","安全防护类","能防止蚊虫、昆虫小咬伤害的特制帽子。因其特殊物料织物制成。既能防蚊虫对人头、脸、颈部位的伤害，还不影响视线和听觉。多用于丛林、水草丛生地区","专用安全生产 ","宿州先进服饰","宿州","灵璧县","灵壁县南部开发区","姜毅/刘凯",13916447558]
[149,"一次性PVC手套","安全防护类","一次性PVC手套主要由聚氯乙烯树脂粉及增塑剂混合而成；主要起隔绝传染等防护作用。产品广泛用于医疗、科研、食品建工、印刷、化工、电子工业，家庭等多个领域。","个体防护 ","安徽安成橡塑科技有限公司","宿州","萧县","萧县经济开发区","陈峰",17355735599]
[150,"跑道绝缘涂料","安全防护类","绝缘材料、三混酚生产、销售及加工","专用安全生产 ","萧县亚太绝缘材料有限公司","宿州","萧县","萧县永堌镇许岗子萧县轻化工业园","神小勇",15852115024]
[151,"钢结构网架","安全防护类","工程机械及配件技术开发、生产、销售；装配式多层钢结构、重钢结构、网架结构、空间索膜结构","建筑业","安徽玖环重工科技有公司","宿州","萧县","萧县龙城镇姬村工业园","吴小俊",13805205333]
[152,"橡胶和塑料制品","安全防护类","新型防水建材生产、销售","专用安全生产 ","萧县金虹新型防水建材有限公司","宿州","萧县","萧县永堌轻化工业园","余敏侠",18855792219]
[153,"内窥镜、摄像机","安全防护类","医疗机械的研发生产","专用安全生产 ","安徽尤泰克医疗科技有限公司","宿州","萧县","萧县龙城镇顺河路100号10#楼","李辉",18955797620]
[154,"防爆电气","安全防护类","在有爆炸性危险气体混合物的场合中，能够防止爆炸事故发生的各类电气。保障石油、化工等工厂的安全生产","电力、热力、燃气及水生产和供应业","二工防爆科技股份有限公司","蚌埠","淮上区","淮上区盛华路285号中恒产业园内","王春",15057506363]
[155,"84消毒液","安全防护类","本品主要成份：次氯酸钠4.05%-5.55%，可用于一般物体表面、果蔬、白色衣物、及医院污染物、消毒杀菌","个体防护 ","蚌埠科卫消毒药剂有限公司","蚌埠","淮上区","淮上区中小企业产业园内果园路和龙兴路交叉口","张超",13905523932]
[156,"碘伏消毒液","安全防护类","本品主要成份：碘含量0.45%-0.55%，可用于卫生洗手消毒、外科术前洗手、术前皮肤、注射部位皮肤、小伤口创面消毒","个体防护 ","蚌埠科卫消毒药剂有限公司","蚌埠","淮上区","淮上区中小企业产业园内果园路和龙兴路交叉口","张超",13905523932]
[157,"75%酒精消毒液","安全防护类","本品主要成份：乙醇70%-75%，可用于皮肤消毒、物体表面、医疗器械消毒","个体防护 ","蚌埠科卫消毒药剂有限公司","蚌埠","淮上区","淮上区中小企业产业园内果园路和龙兴路交叉口","张超",13905523932]
[158,"免洗手消毒凝胶","安全防护类","本产品主要成份：乙醇 含量75±5%，主要用于卫生手消毒和外科手消毒","个体防护 ","蚌埠科卫消毒药剂有限公司","蚌埠","淮上区","淮上区中小企业产业园内果园路和龙兴路交叉口","张超",13905523932]
[159,"过氧乙酸杀菌剂","安全防护类","过氧乙酸消毒液是透明至或淡黄色液体的杀菌剂。无色有刺激性气味，并带有乙酸气味，过氧乙酸具有很强的氧化作用，可将菌体蛋白质氧化而使微生物死亡。","个体防护 ","安徽华凯轻工科技有限公司","蚌埠","怀远县","怀远县经济开发区兴业路11号","杨连开",13805520739]
[160,"安全绳","安全防护类","用于高楼逃生，结实，轻便，外表美观绳子直径在14mm-16mm，一头带扣，带保险卡锁，拉力强度达到国家标准","个体防护 ","太和县双飞绳业有限公司","阜阳","太和县","太和县皮条孙镇陈桥街","高炯",13505660669]
[161,"安全绳、防护网","安全防护类","用于高楼逃生，结实，轻便，外表美观绳子直径在14mm-16mm，一头带扣，带保险卡锁，拉力强度达到国家标准，长度根据用户需求定制。","个体防护 ","太和县彬峰绳网有限公司","阜阳","太和县","太和县皮条孙镇工业园","王建斌",13956762663]
[162,"安全绳","安全防护类","用于高楼逃生，结实，轻便，外表美观绳子直径在14mm-16mm，一头带扣，带保险卡锁，拉力强度达到国家标准，长度根据用户需求定制","个体防护 ","太和县丝榞绳网有限公司","阜阳","太和县","太和县皮条孙镇先锋街北头路西","高炯",13335586999]
[163,"一次性医用口罩、医用防护服","安全防护类","具有高阻隔、高强度、高韧度，防止撕裂和顶破，产品低落絮，减少悬浮颗粒，透汽薄膜有效抵挡细菌和体液，同时确保穿着舒适，减少医疗相关感染","个体防护 ","安徽锦海医药科技有限责任公司","阜阳","太和县","太和县经济开发区医药产业园颍阳大道北侧","李怡飞",13615670507]
[164,"一次性医用口罩、医用防护服","安全防护类","医用口罩(具有抵抗液体、过滤细小颗粒物和细菌等效用)、医用防护服（供临床医务人员在工作时接触到的具有潜在感染性的患者血液、体液、分泌物等提供阻隔、防护作用）","个体防护 ","太和县柯润戈生物科技有限公司","阜阳","太和县","太和县经济开发区B区","安利利",15755849090]
[165,"免洗速干手皮肤消毒凝胶","安全防护类","本品的主要成分为乙醇聚六亚甲基胍双胍盐酸盐为主要成分的消毒液，本品可杀灭肠道致病菌，化脓性球菌，致病性酵母菌和医院感染常见细菌","个体防护 ","安徽洁羱医疗器械有限公司","阜阳","太和县","太和县城关镇工业园区","徐前前",19165586787]
[166,"雨鞋","安全防护类","用于防水防滑、绝缘、耐磨等功能，也可用于工业生产中，具有可防止有毒或腐蚀性液体，保护劳动者安全与健康","个体防护 ","安徽冠泓塑业有限公司","阜阳","界首市","界首市光武科技园繁兴四路北侧","申乾成",13955834999]
[167,"编织袋","安全防护类","编织袋用途、用于填装、容量直径90厘米宽，长120厘米，厚一毫米。","安全材料 ","界首市聚屹包装材料有限公司","阜阳","高新区","界首市高新区北城科技园","王耀明",17856589776]
[168,"垃圾桶、管道","安全防护类","产品类型主要有塑料垃圾桶、塑料托盘、收纳柜、用途医用垃圾收集。\n","安全材料 ","安徽创恒塑业科技有限公司","阜阳","高新区","界首市高新区北城科技园","刘壮恒",15018222288]
[169,"KL6LM(A)本安型矿灯","安全防护类","开灯即录像，实现全过程自动记录，每盏矿灯可存储20-200小时影像资料，具有网络互联功能，可实现远程监控","采矿业","淮南龙科智能科技有限公司","淮南","高新区","科技企业孵化器 ","左映映 ",18109640580]
[170,"煤矿综合自动化信息系统","安全防护类","煤矿综合自动化信息系统采用煤矿生产的安全、高效、少人化、无人化管理理念设计，应用先进的自动化控制技术、计算机通信技术、信息网络技术等科技手段，建设煤矿生产管理、安全管理、经营管理的一体化的安全、高效的现代化矿井","其他安全防护 ","淮南万泰电子股份有限公司","淮南","高新区","国槐路和春申大街交叉口 ","黄健 ",15955463175]
[171,"电能安全管理云平台","安全防护类","电能安全管理平台是一种基于大数据的新型配电管理平台，实现变电站自动化、配电自动化、调度自动化、电能量计费、变电站管理、能源管理及智能运维、无人值守等众多应用功能","专用安全生产 ","淮南万泰电子股份有限公司","淮南","高新区","国槐路和春申大街交叉口 ","黄健 ",15955463175]
[172,"煤矿巷道随掘超前探测系统","安全防护类","使用了国内先进的散射波叠加成像算法，通过多次叠加原理大大地提高了原始地震资料的信噪比及反演结果准确度。利用深度域绕射扫描偏移叠加成像技术，进行巷道迎头前方三维地质成像","其他安全防护 ","淮南万泰电子股份有限公司","淮南","高新区","国槐路和春申大街交叉口 ","黄健 ",15955463175]
[173,"矿山安全专用设备","安全防护类","全矿井安全监控系统，矿山除尘系统及装备、矿山安全传感器、瓦斯抽采设备等","采矿业","平安开诚智能安全装备有限责任公司","淮南","经开区","吉兴路与景秀路交叉口 ","毕汉一",15055422521]
[174,"新型高温耐火绝缘低烟无卤控制电缆","安全防护类","采用先进的高分子耐火绝缘材料和新型耐火结构。具有重量轻、体积小、耐火性能好等特点，还具备低碳和环保性。可应用于医院、车站、机场、煤矿、化工、石油、军事、核电站、造船等领域","安全材料 ","安徽光神航天电子技术有限公司","淮南","经开区","建设南路39号","汪元林",13909644955]
[175,"安全防护类电工电器专用安全生产装备","安全防护类","阻燃耐热电缆：专业研发和生产氟塑料绝缘（耐高温）特种电线电缆具有耐高低温、耐腐蚀、耐辐射、耐热老化、体积小、柔软性好、剥头容易、阻燃和耐化学稳定性等特点","电力、热力、燃气及水生产和供应业","淮南文峰航天电缆有限公司","淮南","经开区","吉兴路6号","徐文峰",13956425797]
[176,"安全防护类专业抢修器材装备","安全防护类","防水电缆、通信电缆：水密型通信控制电缆适用于各种舰船、海上石油平台、深海资源勘测等领域固定敷设有水密要求的控制和通信系统","安全材料 ","淮南文峰航天电缆有限公司","淮南","经开区","吉兴路6号","徐文峰",13956425797]
[177,"安全防护类绝缘材料","安全防护类","六氟化硫绝缘PC薄膜、绝缘油、绝缘漆、绝缘胶、绝缘纸、绝缘纤维制品、电工用薄膜、电工用层压制品、绝缘服面料、绝缘手套材料等","安全材料 ","淮南文峰航天电缆有限公司","淮南","经开区","吉兴路6号","徐文峰",13956425797]
[178,"安全防护类自救器装备","安全防护类","压缩氧自救器、化学氧自救器、LED防爆灯、智能开关柜及应急电源系统等","采矿业","淮南赛力威机电设备有限责任公司","淮南","大通区","大通工业园","刘小波",13675547982]
[179,"民用爆炸物品专用安全生产装备","安全防护类","工业雷管生产装备和系统；多孔粒装铵油炸药（混装）生产装备和系统；炸药和雷管生产测试仪器；民用爆炸物品专用车辆","采矿业","淮南舜泰化工有限责任公司","淮南","八公山区","八公山区常山村","王四龙",13855429379]
[180,"封孔器及封孔材料","安全防护类","矿用封孔器是一种用于瓦斯抽放前的封孔装置，采用“堵-注-排”封孔工艺，封孔后封孔段钻孔稳定，可实现钻孔的长效密封。一般用于煤层钻孔的快速封孔，特别适合于钻孔倾角大、封孔深度深的上向或下向孔封孔。","采矿业","淮南东华欧科矿山支护设备有限责任公司","淮南","八公山区","八公山区工业园","董经纬",15055406877]
[181,"足部防护用品","安全防护类","企业为石油、化工、冶金、制造业、重工业、应急救援等多个行业提供全方位安全防护鞋具","个体防护 ","洛奇鞋业（滁州）有限公司）","滁州","经开区","滁州市淮河路408号","隋刘政",18609603171]
[182,"Vip.真空绝热板","安全防护类","主要产品，新型高效节能真空绝热板、冰箱内胆，建筑隔热板，等产品。主要用于：家电、冷库、医药保温、建筑行业","专用安全生产 ","滁州银兴新材料科技有限公司","滁州","经开区","经开区世纪大道888号","丁有成",15505508111]
[183,"钢筋混凝土防护设备、钢结构手动防护设备","安全防护类","人防门就是人民防护工程出入口的门，有普通单、双扇防护密闭门和密闭门，活门槛单、双扇防护密闭门和密闭门等多种人防设备，材质分为钢筋混凝土和钢结构两种","建筑业","安徽顺辉人防工程有限公司","滁州","琅琊区","琅琊区六安路18号","王飞",18725507922]
[184,"保温、保冷、防火材料","安全防护类","广泛用于设备的保温、保冷、防火、建筑业、化工、石油的新型节能环保材料","专用安全生产 ","安徽安徽鼎元新材料有限公司","滁州","琅琊区","琅琊经济开发区蚌埠路18号","袁军",13955003527]
[185,"改性沥青防水卷材（自粘）","安全防护类","具有延伸率大、耐水压、耐腐蚀、抗变形能力强等特点；用途：用于地下室、地铁及各种建筑物的非外露屋面防水、防潮防渗工程","专用安全生产 ","北新禹王防水科技（安徽）有限公司","滁州","全椒县","全椒县十字镇十谭现代产业园新城大道66号","晋兵青",18726626120]
[186,"防水涂料","安全防护类","具有强度高、延伸率大、耐水性好等特点，在基层表面形成一层坚韧的无缝涂膜；用途：用于地下、厕浴间、隧道、路桥、涵洞、水池等防水、防渗工程，也可用于非暴露型屋面防水工程","专用安全生产 ","北新禹王防水科技（安徽）有限公司","滁州","全椒县","全椒县十字镇十谭现代产业园新城大道66号","晋兵青",18726626120]
[187,"改性沥青防水卷材（热熔）","安全防护类","具有高强度、大延伸、耐腐蚀等优点，使地下构筑物在频繁产生机械振动环境下也能保持完整无损的密闭防水工程；用途：用于结构变形大、水位高等地铁、地下防水工程及易产生振动的其他防水工程","专用安全生产 ","北新禹王防水科技（安徽）有限公司","滁州","全椒县","全椒县十字镇十谭现代产业园新城大道66号","晋兵青",18726626120]
[188,"高分子防水卷材","安全防护类","是由高分子片材、非沥青基高分子自粘胶和特种颗粒防粘层(或隔离膜防粘层)构成的能与后浇混凝土粘接的防水卷材；用途：用于地下预铺反粘施工的防水工程","专用安全生产 ","北新禹王防水科技（安徽）有限公司","滁州","全椒县","全椒县十字镇十谭现代产业园新城大道66号","晋兵青",18726626120]
[189,"消防服、救援服","安全防护类","消防服有三层或四层结构全部成分均阻燃，。救援服分成夏季和冬季两种款式，全部成分均阻燃。是消防员在进行抢险救援时穿着的服装","个体防护 ","安徽赞瑞实业有限公司","滁州","全椒县","十字镇 十谭产业园滨水路99号","徐茂静",13721007652]
[190,"岩棉板","安全防护类","岩棉板具有优良的防火、保温和吸音性能，用于建筑墙体、屋顶的保温隔音","安全材料 ","安徽泰石岩棉有限公司","滁州","全椒县","全椒县十字镇化龙村海螺大道888号","戴光明",15729111737]
[191,"安全玻璃中间膜","安全防护类","1、聚乙烯醇缩丁醛树脂 2、安全玻璃中间膜","安全材料 ","安徽美邦树脂科技有限公司","滁州","定远县","定远县炉桥镇盐化园工业园内","李仁春",18017013339]
[192,"绝缘漆","安全防护类","聚酯绝缘漆、聚酯亚胺绝缘漆、聚氨酯绝缘漆、聚酰氨酰亚胺绝缘漆","安全材料 ","定远诚宇电工材料有限公司","滁州","定远县","定远县炉桥镇盐化园工业园内","许听余",13906151658]
[193,"绝缘漆","安全防护类","聚酯绝缘漆","安全材料 ","安徽禹泰化工有限公司","滁州","定远县","定远县炉桥镇盐化园工业园内","吴梅",13655293061]
[194,"医用防护服","安全防护类","具有良好的透湿性和阻隔性，能有效抵抗酒精、血液、空气粉尘、细菌的渗透。使用安全方便，保护穿着者免受感染威胁","个体防护 ","凤阳洁宏无纺布制品有限公司","滁州","凤阳县","凤阳县浙商工业园","朱文伟",13506261308]
[195,"防火玻璃","安全防护类","具有优秀的防火性能，耐火时间超过120分钟，具有超高的透明度，可见光透过率92%。主要应用于防火幕墙、防火门窗等领域","安全材料 ","凤阳凯盛硅材料有限公司","滁州","凤阳县","凤阳县经开区","冯云喜",17755075981]
[196,"一次性医用口罩","安全防护类","具有低抗液体、过滤细小颗粒物和细菌等效用","个体防护 ","安徽宜美健医疗用品有限公司","滁州","天长市","天长市新街镇飞龙北路8号","王爱平",13809041511]
[197,"一次性医用口罩","安全防护类","具有低抗液体、过滤细小颗粒物和细菌等效用","个体防护 ","安徽新利清洁用品有限公司","滁州","天长市","万寿镇忠孝村工业园区","蔡丰富",13905508658]
[198,"一次性医用口罩、医用防护服、一次性输液器等","安全防护类","具有低抗液体、过滤细小颗粒物和细菌等防护效用","个体防护 ","安徽天康医疗科技有限公司","滁州","天长市","经济开发区纬一路228号","柏保东",13505557811]
[199,"一次性医用口罩","安全防护类","具有低抗液体、过滤细小颗粒物和细菌等效用","个体防护 ","天长市科惠医疗用品有限公司","滁州","天长市","石梁镇工业集中区经十六路2号","刘  露",15715507326]
[200,"安全帽","安全防护类","安全帽是指对人头部受坠落物及其他特定因素引起的伤害起防护作用的帽子。由帽壳、帽衬、下颏带及附件等组成","专用安全生产 ","天长市富实安全防护用品有限公司","滁州","天长市","汊涧工业园区天滁新路188号","陈世明",13956313456]
[201,"安全鞋","安全防护类","产品广泛应用于油田、电力、煤矿、机械、冶金、建筑、化工、制药等领域，具有防砸、防刺、防滑、绝缘、耐磨等功能，保护劳动者安全与健康","个体防护 ","安徽省敬烨防护科技有限公司","滁州","明光市","明光市体育路140号","许二梅",13955086194]
[202,"雨衣","安全防护类","应急用防水雨衣","个体防护 ","安徽忠旭雨衣有限公司","六安","霍邱县","霍邱县曹庙镇吴阳村","王辉堂",13812533110]
[203,"防火布","安全防护类","使用陶瓷纤维防火棉加工制作，用于建筑工程，消防防火卷帘门配套","安全材料 ","安徽尼斯纺织有限公司","六安","霍邱县","城关镇","胡中华",18606533888]
[204,"医用防护服","安全防护类","防护服是用于有重要传染病，病源微生物传染污染区域内使用的防护用品","个体防护 ","六安市泫沣防护用品有限公司","六安","叶集区","叶集区姚李工业园","刘希琴",15855943815]
[205,"漆包线绝缘漆","安全防护类","公司主要生产耐热等级达到F、H、C级的各类高质量漆包线绝缘漆产品,主要用于配套冰箱空调压缩机线圈上漆包线的绝缘，有效减少电器产品发生火灾风险","安全材料 ","艾仕得绝缘材料（安徽有限公司）","马鞍山","和县","精细化工产业基地华星路5号","刘菊芳",18916269117]
[206,"保温隔音材料","安全防护类","产品包括外墙岩棉板、屋面岩棉板、岩棉带一体化板、岩棉带复合板、岩棉净化板等，产品广泛适用于建筑、钢铁冶金保温与隔音","安全材料 ","马鞍山市鸿翮实业有限公司","马鞍山","当涂县","马鞍山市当涂县姑孰镇工业集中区","赵子龙","0555-2980248"]
[207,"建筑用钢质、钢木质防火门、防火卷帘","安全防护类","产品主要用于建筑内防火、隔绝，已通过国际质量管理体系认证、环境管理体系认证职业健康安全管理体系认证等各项体系认证","建筑业","安徽白云南粤防火门有限公司","马鞍山","当涂县","马鞍山市当涂县新桥工业集中区","王红霞","0555-6252999"]
[208,"眼面防护用品","安全防护类","主要为预防外界光线或其它对眼面部伤害的个人防护装备","个体防护 ","马鞍山奥柯环保科技发展有限公司","马鞍山","雨山区","永庆路180号","陈植花",13855575667]
[209,"头部防护用品","安全防护类","是为了防御头部不受外来物体打击和其他因素危害而配备的个人防护装备","个体防护 ","马鞍山奥柯环保科技发展有限公司","马鞍山","雨山区"]
[210,"汽车智能诊断仪","安全防护类","汽车云诊断服务系统主要用于汽车诊断和服务。可作为汽车维修店门店诊断仪，学校的教学科研设备，也可作为汽车远程服务提供商、汽车道路运行检测、车况检测及维修设备，同时也可作汽车生产厂商配套的诊断设备","专用安全生产 ","安徽省爱夫卡电子科技有限公司","马鞍山","雨山区","智能装备产业园25栋","朱志峰",13095556533]
[211,"转炉挡渣滑板","安全防护类","主要产品为转炉挡渣滑板，产品为两块开孔的耐火砖，通过挡渣机构连接、装配，并控制开孔的相对错位进行开关，提高了现场安全性，避免钢水、钢渣外流对现场设备和人员造成伤害","专用安全生产 ","马鞍山利尔开元新材料有限公司","马鞍山","经开区","雨田路151号","汪玉娇",19955544580]
[212,"智能料仓清堵系统","安全防护类","为了减少物料与仓壁的摩擦力，降低物料与仓壁之间的摩擦系数。破除粘壁棚料；该系统同时产生剪切力，造成仓内物料内聚力不平衡，物料自然坍塌。破除拱状棚料，彻底避免了人工清阻和破拱带来的人身伤害","专用安全生产 ","马鞍山市天工科技股份有限公司","马鞍山","经开区","安朱然路9号","叶琴",18705557188]
[213,"聚氨酯复合板系列","安全防护类","采用高品质彩色涂层钢板为面板，防火保温效果更佳，性能更持久，是钢建筑维护材料领先者，多用于工业建筑，仓库，大型店铺","专用安全生产 ","安徽宏志建材科技有限公司","马鞍山","慈湖高新区","银杏大道339号4","马水英",13605554038]
[214,"岩棉板、岩棉条","安全防护类","岩棉板是玄武岩经高温熔融成纤、粘结、固化加工而成,广泛应用于船舶、冶金、建筑等行业,具有良好的绝热防火、隔音降噪、节能、憎水性强等性能","专用安全生产 ","马鞍山市北益环保科技有限责任公司","马鞍山","慈湖高新区","银杏大道230号1、2、3-全部","潘政桃",13805557100]
[215,"抗震支架","安全防护类","抗震成品支吊架系列、隧道预埋槽道及配件、桥架母线槽系列、止水鱼鳞网混凝土配套件","专用安全生产 ","                  亿德顺科技有限公司","马鞍山","雨山区","雨山经济开发区永乐路6号","马率峰",15316510511]
[216,"医用外科口罩（无菌型）","安全防护类","该产品用于戴在手术室医务人员口鼻部位，以防止皮屑、呼吸道微生物传播到开放的手术创面，并阻止手术病人的体液向医务人员传播，起到双向生物防护的作用。","个体防护 ","                安徽泰恩康制药有限公司","马鞍山","当涂县","当涂经开区","柯江英",17755525399]
[217,"活性碳酸钙、橡塑钙、线缆钙、硅胶钙、油墨钙和汽车底涂钙","安全防护类","主要产品有橡塑钙、线缆钙、硅胶钙、油墨钙和汽车底涂钙，广泛应用于橡胶、塑料、造纸、涂料、纺织、化学制剂及油墨等，此外还可用于牙膏、化妆品、食品、制药等工业","专用安全生产 ","芜湖卓越纳米新材料股份有限公司","芜湖","繁昌区","繁昌区荻港镇新型建材工业园","刘昌庆",13705538722]
[218,"陶瓷化防火电缆、铜网屏蔽软电缆、新型纳米抑烟阻燃耐火电缆","安全防护类","高柔软屏蔽信号控制线缆、新型纳米抑烟阻燃耐火电缆等各种防护类电缆，主要用于新型计算机传输电缆及其制备方法","专用安全生产 ","安徽联嘉祥特种电缆有限公司","芜湖","繁昌区","繁昌区火焰山南路与纬一西路交叉口","张兰",18755302352]
[219,"特种防腐涂料、高性能重防腐工程涂料技术研发、转化及服务","安全防护类","特种防腐涂料、高性能重防腐工程涂料技术研发、转化及服务，高分子材料，用于金属、非金属表面防腐等","化学原料和化学制品制造业","芜湖市金贸环保材料科技有限公司","芜湖","繁昌区","繁昌区孙村镇九连村","毕玉琴",13695530201]
[220,"电力变压10kV油浸式电力变压器器","安全防护类","10kv油浸式电力变压器,它含有油箱,铁芯和绕组,铁芯和绕组一起浸入灌满了变压器油的油箱中,它集油箱壁上设置散热管油箱和油箱壁上设置波纹片油箱优点于一身,使用安全可靠,重量相对轻,散热效率高","电力、热力、燃气及水生产和供应业","安徽蓝翔电器成套设备有限公司","芜湖","南陵县","南陵县经济开发区","傅 俊",13855383582]
[221,"SC9型35KV级配电变压器","安全防护类","SC9型35KV级配电变压器是以环氧树脂为绝缘介质，可直接深入负荷中心进行供电。该产品电压比为35/0.4kV，变电容量大、产品结构紧凑，可广泛用于：商业中心、高层建筑、机场、港口、油库、指挥中心等重要场所","电力、热力、燃气及水生产和供应业","芜湖金牛电气股份有限公司","芜湖","南陵县","南陵经济开发区古亭路","刘朝锋",13705539218]
[222,"专用对讲产品、网络系统集成","安全防护类","公司一直从事“来邦对讲”系列产品的研发、生产及销售，自主知识产权的IP网络数字音视频技术，产品广泛应用于医院、养老院、银行、监狱、学校、高速公路、电梯等领域","水利、环境和公共设施管理业","来邦科技股份公司","芜湖","南陵县","南陵经济开发区来邦科技园","丁寿斌",13905539675]
[223,"医用外科口罩","安全防护类","日产10万只医用外科口罩能在一定程度上预防呼吸道感染","个体防护 ","芜湖悠派护理用品科技股份有限公司","芜湖","鸠江区","中国（安徽）自由贸易试验区芜湖片区","戴小平",13965167060]
[224,"护目镜","安全防护类","防护眼晴","化学原料和化学制品制造业","芜湖通联汽车部件有限公司","芜湖","鸠江区","中国(安徽)自由贸易试验区芜湖片区龙腾路8号","滕磊",13965194466]
[225,"钢筋混凝土防护密闭门","安全防护类","防护密闭门设置在出入口最外侧，具有阻挡冲击波和隔绝毒剂两种功能","建筑业","芜湖徽铠安宏人防设备有限公司","芜湖","经开区","经济技术开发区东区纬二次路南侧","汪进红",17718122971]
[226,"钢结构防护密闭门","安全防护类","产品主要用于地下车库出入口部，战争爆发时进行平战转换，防核武器5级、6级及炸弹冲击波，化学武器、生物武器等","专用安全生产 ","芜湖徽铠安宏人防设备有限公司","芜湖","经开区","经济技术开发区东区纬二次路南侧","汪进红",17718122971]
[227,"地铁隧道正线防护密闭门","安全防护类","产品主要用于地铁隧道等主要出入口部，战争爆发时进行平战转换，防核武器5级、6级及炸弹冲击波，化学武器、生物武器等","专用安全生产 ","芜湖徽铠安宏人防设备有限公司","芜湖","经开区","经济技术开发区东区纬二次路南侧","汪进红",17718122971]
[228,"可运动式应急液压千斤顶（多路同步类-4缸）","安全应急服务类","实现千斤顶能够在狭小空间自由运动和伸缩的目的,扩大液压千斤顶的应用范围.运用于各类工况需要顶举、收缩等现场维修及排险项目","采矿业","芜湖银鸿液压件有限公司","芜湖","湾沚区","银鸿液压件有限公司","汪玉平",18955396551]
[229,"防水材料","安全防护类","防水材料是指在建筑工程中起防水作用的材料，它主要用于屋面、地下建筑、水中建筑、卫生间、阳台等的防水、防潮处理。","专用安全生产 ","安徽朗盾建材科技有限公司","宣城","宣州区","高新技术产业开发区马山路1号","陈佳",15505638886]
[230,"泡沫玻璃","安全防护类","广泛应用于深冷及高温环境，导热系数小、抗压强度高、不吸水、不透湿、气密性好","专用安全生产 ","安徽汇昌新材料有限公司","宣城","宣州区","麒麟大道以南松泉路以北","许勇根",13806736363]
[231,"灭火器","安全防护类","ABC干粉手提储压式、BC干粉手提储式、推车ABC（BC）储压式、水基灭火器。用途：用于扑救石油、有机溶剂等易燃液体、可燃气体和电气设备的初期火灾。水基灭火器是一种新型的物理灭火器，具有无毒、无污染、灭火效率高，阻燃和抗复燃性能好的优点","安全材料 ","宣城金盾防火设备有限公司","宣城","郎溪县","郎溪县开发区十字园区","甘  露",13731930525]
[232,"安全帽","安全防护类","高冲ABS及玻璃钢材质，工程类安全帽及骑行类头盔","个体防护 ","旌德县电子电器配件厂（普通合伙）","宣城","绩溪县","宣城市旌德县孙村镇玉溪","李  贝",18956366828]
[233,"岩棉板","安全防护类","岩棉板是A级的不燃材料，具有保温，吸音，隔热，防火等特点，广泛应用于建筑，船舶，设备，管道等保温防火领域","化学原料和化学制品制造业","欧文斯科宁（广德）岩棉制造有限公司","宣城","广德市","广德市新杭镇经济开发区广安路 10 号","汪传峰",13311667301]
[234,"安全帽","安全防护类","小金刚安全帽系列，头部保护，进口ABS用料、SPA一锁键帽衬，利用TBC帽衬技术，具有12个自由度全方向可调节、多孔位散热。","个体防护 ","安徽华信安全设备有限公司","宣城","广德市","广德市经济开发区赵联北路 9 号","林健",13951855500]
[235,"安全鞋","安全防护类","吉豹安全鞋，结合了woshine华信近20年的专业防护及英国William&Baron公司的先进设计理念，严格按照欧洲标准生产。广泛用于存在机械危害，化学品危害，重物冲击，高温危险，电气危害等工作环境与作业场所。适用于:建筑、电力、半导体、化学、汽车制造、石油化工、机械加工等行业","个体防护 ","安徽华信安全设备有限公司","宣城","广德市","广德市经济开发区赵联北路 9 号","林健",13951855501]
[236,"岩棉板","安全防护类","1、主要用于各类建筑隔墙、幕墙、金属和石材干挂幕墙系统的防火、保温、隔音。\n2、主要用于工业炉窑、锅炉、烘箱、大口径管道、储罐以及设备的隔热、保温、防火及隔音等","化学原料和化学制品制造业","安徽轩鸣新材料有限公司","宣城","广德市","广德市经济开发区启航路 7 号","李万清",18956377589]
[237,"漆包线绝缘漆","安全防护类","以高分子聚合物为基础,能在一定的条件下固化成绝缘膜的重要绝缘材料","专用安全生产 ","艾伦塔斯电气绝缘材料(铜陵)有限公司","铜陵","经开区","经济技术开发区","许涌",13856220865]
[238,"复方氨酸注射液（18AA-VII）","安全防护类","大容量肠外营养注射液，主要用于病人的术后营养支持","专用安全生产 ","安徽富邦药业有限公司","铜陵","经开区","经济技术开发区泰山大道577号","汪云",13515620140]
[239,"人防工程防护密闭门","安全防护类","适用各类人防工程及出入口，迅速实现平战功能的转换，具有密闭、抗冲击波、防毒、滤毒能力，能阻止放射性沾染、生物和化学战剂渗入工程内部 ","建筑业","铜陵市金鑫人防工程防护设备有限公司","铜陵","经开区","经济技术开发区","吴宏霞",18756281806]
[240,"消毒湿巾","安全防护类","以水刺无纺布，纯化水为生产用水，适量添加消毒液等原料，对适用于人体、一般物体表面、医疗器械表面及其他物体表面具有清洁消毒作用的产品","个体防护 ","铜陵麟安生物科技有限公司","铜陵","经开区","经济开发区翠湖三路西段892号","张霖",13655628711]
[241," 无轨人车","安全防护类","专门运送生产作业人员、在地下矿山斜坡道和（或）巷道中行驶的自行轮胎式车辆。有独立的大梁，底盘强度较高，抗颠簸性能好","采矿业","安徽铜冠机械股份有限公司","铜陵","经开区","经济技术开发区翠湖三路西段1660号","宋宁宁",15056202078]
[242,"隔离衣","安全防护类","透气性好，透湿性好，可防止细小灰尘和液体渗透，同时允许水蒸气渗透。隔离服本身不发尘，不粘尘，阻隔性好，密度高，强度高，能有效杀菌","个体防护 ","安徽瑞峰雨具有限公司","铜陵","枞阳县","枞阳县项铺镇","陶思福","139 0966 2658"]
[243,"隔离衣","安全防护类","透气性好，透湿性好，可防止细小灰尘和液体渗透，同时允许水蒸气渗透。隔离服本身不发尘，不粘尘，阻隔性好，密度高，强度高，能有效杀菌","个体防护 ","安徽科瑞户外用品科技有限公司","铜陵","枞阳县","枞阳县枞阳镇长江路","陶思福","139 0966 2658"]
[244,"救灾帐篷","安全防护类","可以用来做临时指挥中心、医疗救援、防疫、居住等，为救灾大大提供了便捷条件","社会保障 ","枞阳县森林雨具有限责任公司","铜陵","枞阳县","枞阳县白柳镇","王胜林","189 5561 2888"]
[245,"集装袋（吨袋）","安全防护类","吨袋可以装载1吨的货物，可用于防洪抗洪抢险救灾，作为防汛袋使用；快速及规模化的物资调运，且可以用于应急工程的土方及物资运输和桥梁试压。货物装袋后即可使用叉车行车等快速整体调运，避免人工零散搬运的低效和不安全等因素，易储存、易装载","抢险救援 ","铜陵天润包装有限责任公司","铜陵","义安区","金桥工业园区","程钧雷",13705621159]
[246,"高铁稀土铝合金防火报警电缆","安全防护类","基本工艺是拉丝、绞合、成缆、铠装、护套，原料一般是绝缘材料、护套材料、辅助材料、铜丝、铝丝。组成结构、填充层、报警装置的区分，用于高铁、消防、高层建筑等","建筑业","安徽华宝电缆有限责任公司","铜陵","义安区","金桥经济开发区","后学才",13856237888]
[247,"光伏热导阻燃电缆","安全防护类","基本工艺是拉丝、绞合、成缆、铠装、护套，原料一般是绝缘材料、护套材料、辅助材料、铜丝、铝丝。从外向内依次包括最外护套、屏蔽层、中间阻燃层、阻水层等，最外护套的材料中添加有云母粉纳米颗粒。用于太阳能电站、光电设备系统","专用安全生产 ","安徽华宝电缆有限责任公司","铜陵","义安区","金桥经济开发区","后学才",13856237888]
[248,"篦冷机防寒耐磨电缆","安全防护类","基本工艺是拉丝、绞合、成缆、铠装、护套，原料一般是绝缘材料、护套材料、辅助材料、铜丝、铝丝。组成结构、最外耐磨层、防寒屏蔽层、缠绕层等依次包裹，中心隔离层、防寒屏蔽层区分，用于建筑材料行业、电力、冶金、化工","专用安全生产 ","安徽华宝电缆有限责任公司","铜陵","义安区","金桥经济开发区","后学才",13856237888]
[249,"智能交通系统","安全防护类","交通管理-前端子系统(道路车辆智能监测记录系统、机动车区间测速系统、闯红灯自动记录系统、行人闯红灯自动检测报警系统、人行横道道路交通安全违法行为监测记录系统、城市交通信号控制系统、视频监控系统、应急车道抓拍系统、车辆停车视频检测抓拍系统、智慧路口系统)","道路运输业","安徽蓝盾光电子股份有限公司","铜陵",null,"石城路工业园","贾强",15395624815]
[250,"非医用口罩","安全防护类","在日常空气污染环境下，能滤除颗粒物、有防护功能的个人防护口罩。","个体防护 ","安徽宜人医用包装有限公司","池州","东至","大渡口经济开发区纬二西路4号\n\n","龙胜","0566-8907999\n13909666042"]
[251,"门禁控制设备","安全防护类","综合运用人脸识别、二维码、IC卡等智能控制技术，有效提升门禁安全性能，起到智能防盗、防突作用。适用于学校、商务楼、小区等人员活动场所。","专用安全生产 ","安徽晶鹏智能装备科技有限公司","池州","东至","东至县大渡口镇经济开发区八百通物联网产业园4幢301","胡四九","0566-8017889\n13682627279"]
[252,"智能控制系统","安全防护类","电子智能化系统设备，运用人脸识别技术，适用于商超、街道、景区等人流密集场所监控。","专用安全生产 ","安徽晶通智能科技有限公司","池州","东至","大渡口经济开发区麻桥路03号","刘文安",18156626199]
[253,"纤维棉、纤维毯","安全防护类","主要用途：防火卷帘门、工矿窑炉节能保温、造船及大型工矿设备隔音、化工企业防火隔热毯、电器类产品绝缘隔热等。","安全材料 ","青阳县华润冶金材料有限公司","池州","青阳县","青阳县丁桥镇","陈乃忠",13905552534]
[254,"高等级无尘布","安全防护类","主要材料是外购无纺布面料作为原料，使用激光切割机按照客户要求剪裁。主要用途就是制作无尘服、无尘手套、无尘鞋和无尘口罩的原材料。","安全材料 ","安徽高芯众科半导体有限公司","池州","经开区","金安园区金同路69号","汪文学",13695660186]
[255,"无尘服","安全防护类","主要用于防护粉尘、烟、雾等颗粒污染物，通过人体自身呼吸来使用的呼吸防护用品，在工业生产及日常生活中广泛使用","个体防护 ","安徽高芯众科半导体有限公司","池州","经开区","金安园区金同路69号","汪文学",13695660186]
[256,"非医用口罩","安全防护类","主要用于防护粉尘、烟、雾等颗粒污染物，通过人体自身呼吸来使用的呼吸防护用品，在工业生产及日常生活中广泛使用","个体防护 ","安徽高芯众科半导体有限公司","池州","经开区","                                        金安园区金同路69号号路69号金安园区金同路69号","汪文学",13695660186]
[257,"无尘鞋","安全防护类","鞋子为长筒型，面板材料使用的是无尘布，鞋帮采用耐酸碱腐蚀和抗压材料，在半导体工厂中广泛运用于安全防护和防止灰尘污染车间环境。","个体防护 ","安徽高芯众科半导体有限公司","池州","经开区","金安园区金同路69号","汪文学",13695660186]
[258,"无尘手套","安全防护类","主要用于防护粉尘，保护手不被工件划伤，半导体产业最忌讳人手直接接触工件表面从而污染工件，在工业生产及日常生活中广泛使用","个体防护 ","安徽高芯众科半导体有限公司","池州","经开区","金安园区金同路69号","汪文学",13695660186]
[259,"高温压力传感器","安全防护类","在封装结构上采用薄膜隔离式结构,在油腔与波纹片所形成的密闭容腔里面填充高温硅油。要用于医疗器械、血压计、环境测量、高温反应容器内的压力、以及各种发动机腔体内的压力、测压等领域","专用安全生产 ","安徽微泰导航电子科技有限公司","池州","经开区","电子信息产业园四期","李桂新",18956268096]
[260,"MEMS恒温器TEC","安全防护类","封装工艺为键合、贴片、引线键合、封帽。半导体功率器件散热恒温，激光发射器的恒温，工业医疗检测载体表面恒温环境的提供","专用安全生产 ","安徽微泰导航电子科技有限公司","池州","经开区","电子信息产业园四期","李桂新",18956268096]
[261,"加速度传感器","安全防护类","封装工艺：通过以下基本工艺晶圆划片，晶圆贴装，烘烤，晶圆键合，平行风焊接，然后高温24小时老化后测试产品的各项参数包括：爆破压力，温漂TCR,线性等，最终筛选出符合要求的产品。产品主要应用于工业机床和桥梁的振动监测，汽车航空运动器材的姿态稳定等","专用安全生产 ","安徽微泰导航电子科技有限公司","池州","经开区","电子信息产业园四期","李桂新",18956268096]
[262,"温度传感器","安全防护类","产品制作工艺为 使用探针台对红外热点堆的MEMS晶圆测试，制作MAPING，然后晶圆使用DISCO机器进行划片。产品应该范围：非接触式的温度测量包动物和人体体温非接触探测，电子和电力工业电器/电线的表面温度变化监测等。","专用安全生产 ","安徽微泰导航电子科技有限公司","池州","经开区","电子信息产业园四期","李桂新",18956268096]
[263,"重烧白云岩","安全防护类","选用矿山优质R级白云岩，破碎后采用先进的回转窑一步煅烧，将R级白云石料烧至1900度形成重烧白云石DBD。耐火砖主要用于钢铁、水泥、玻璃行业的高温锅炉砌筑。","专用安全生产 ","禄思伟矿业资源（安徽）有限公司","池州","经开区","经济技术开发区","张靖",13913100900]
[264,"熔剂白云岩","安全防护类","质量成分低于耐火材料使用级别的白云石，叫溶剂用白云岩。在采矿场穿孔爆破后，直接装车外卖给钢厂作为炼钢熔剂。作用是为了除去钢水中的矿渣。","专用安全生产 ","禄思伟矿业资源（安徽）有限公司","池州","经开区","经济技术开发区","张靖",13913100901]
[265,"建筑用白云岩","安全防护类","质量成分达不到耐火材料或熔剂用要求的白云岩，在采矿场爆破后直接装车作为建筑石料外。用于修桥铺路等。","专用安全生产 ","禄思伟矿业资源（安徽）有限公司","池州","经开区","经济技术开发区","张靖",13913100902]
[266,"非医用口罩","安全防护类","主要用于防护粉尘、烟、雾等颗粒污染物，通过人体自身呼吸来使用的呼吸防护用品，在工业生产及日常生活中广泛使用","个体防护 ","安徽康采恩包装材料有限公司","池州","江南产业集中区","松花江路7号","陆经理",13655565735]
[267,"非医用KN95口罩","安全防护类","面料轻柔，滤料级别达到GB2626-2006，适用于成人日常出行防护使用，面罩为随弃式，不可水洗","个体防护 ","桐城兴创防护用品有限公司","安庆","桐城市","经开区兴隆路26号","黄娟",13966605225]
[268,"医用（民用）口罩等防护用品","安全防护类","生产医用（民用）口罩，产品有耳绳、熔喷布，KF94、KN95、绑带、罩杯等产品，适用于防护各类颗粒物（如粉尘、烟、雾和微生物），适用于轻工业、环卫、民用日常使用","个体防护 ","安庆美华医疗器械有限公司","安庆","桐城市","桐城市经济技术开发区经五路安徽鑫美芝光电科技有限公司院内第1幢","周苹",13671395187]
[269,"帆布手套","安全防护类","本产品质地坚牢耐磨，紧密厚实，可以很好的保护工人手部，一般用于建筑、石矿，打磨五金铸造等行业","个体防护 ","桐城花蕾实业有限公司","安庆","桐城市","桐城市青草镇青草大道","张礼婷",15155687597]
[270,"白棉手套","安全防护类","本产品采用优质精梳棉，具有柔软舒适，吸汉透气的优点，广泛用于礼仪演出，珠宝古玩店，交通指挥，家庭作业工厂作业等","个体防护 ","桐城花蕾实业有限公司","安庆","桐城市","桐城市青草镇青草大道","张礼婷",15155687597]
[271,"KN95口罩","安全防护类","KN95口罩符合国标GB2626-2019，能有效的防尘防霾防飞沫。适用于轻工业、环卫、民用日常使用","个体防护 ","安徽惠友防护用品有限公司","安庆","桐城市","桐城市青草镇青草大道","徐珊珊",15391816090]
[272,"KN95口罩、KF94口罩、杯型口罩","安全防护类","生产符合新国标GB2626-2019标准的KN95口罩，5层，6层，7层不同厚度，可以预防由患者体液或血液飞溅引起的飞沫传染，适用于居民的日常防护","个体防护 ","桐城市康宝防护用品有限公司","安庆","桐城市","桐城市青草镇同兴居委会枫树组14号","陈晓丽",15375186520]
[273,"KN95折叠式防护口罩","安全防护类","本产品采用全自动设备制造，能全方位贴脸保护，3D立体透气空间，呼吸顺畅。适用于防护各类颗粒物（如粉尘、烟、雾和微生物）","个体防护 ","桐城市新锦江劳保用品有限公司","安庆","桐城市","桐城市青草镇朝阳路","徐桂江",13505632105]
[274,"劳保口罩","安全防护类","本产品密合性良好，对悬浮于空气中的颗粒物可以有效的防护，适用于轻工业防护，居民日常防护","个体防护 ","安徽省桐城市雅格卫生材料有限公司","安庆","桐城市","桐城市青草镇青草大道","汪黉",17755666242]
[275,"一次性无纺布防护","安全防护类","主要功能是：高效率过滤 悬浮在空中的固态、液态或固态和液态的颗粒状物质。技术指标是：GB2626—2006，侧插式加湿口罩于2018年09月11日获国家知识产权局授权实用新型专利","个体防护 ","安景瑞无纺布制品有限公司","安庆","怀宁县","怀宁县高河月山大道6号","刘娴",13861641257]
[276,"一次性防护口罩","安全防护类","主要功能是：高效率过滤 悬浮在空中的固态、液态或固态和液态的颗粒状物质。技术指标是：GB2626—2006","个体防护 ","花蕾纺织材料有限公司","安庆","怀宁县","高河石牌大道与稼先大道交叉口","方逐昌",13905561064]
[277,"一次性口罩","安全防护类","防护呼吸道传染疾病，阻挡飞沫，粉尘","个体防护 ","望江县凯伦斯特劳保用品有限公司","安庆","望江县","望江县经开区鸦滩路2号","李琪",15056651881]
[278,"防毒面具","安全防护类","呼吸防护类过滤式和隔绝式防尘防毒面具，主要由面罩和滤毒罐及其他附件组成，面罩采用氯丁橡胶/硅橡胶混炼材料，这种材料质轻、柔韧性好、抗化学渗透性强。滤毒罐中采用高效合成粒空气( HESPA)过滤材料，这种材料具有优异的过滤性能，对细菌、病毒、放射性和有毒的灰尘、烟雾以及化学战剂、工业化学品都能提供有效的防护。","个体防护 ","安徽潜隆机电科技有限公司","安庆","潜山市","潜山市经济开发区中合产业园,","韩非",13855675070]
[279,"防化服","安全防护类","躯干类防护，非织物酸碱类化学品防护服，用来保护在有危险性化学物品或腐蚀性物品的现场作业的工作人员免遭化学危险品或腐蚀性物资的侵害。","个体防护 ","安徽潜隆机电科技有限公司","安庆","潜山市","潜山市经济开发区中合产业园,","韩非",13855675070]
[280,"医用防护口罩","安全防护类","为突发事件尤其是公共卫生事件的紧急医疗救护工作提供保障。适用于医务人员和相关工作人员对经空气传播的呼吸道传染病的防护。","个体防护 ","黄山安尔安卫生防护用品有限责任公司","黄山","高新区","高新区蓬莱路18号","聂万松",18905599115]
[281,"一次性医用口罩","安全防护类","适用于佩戴者在不存在体液和喷溅风险的普通医疗环境下的卫生护理。","个体防护 ","黄山安尔安卫生防护用品有限责任公司","黄山","高新区","高新区蓬莱路18号","聂万松",18905599115]
[282,"一次性防护口罩（非医用）","安全防护类","呼吸防护用品；为防止有害粉尘、有害气体及空气污染物等进入呼吸器官而使用的防护用品。","个体防护 ","黄山安尔安卫生防护用品有限责任公司","黄山","高新区","高新区蓬莱路18号","聂万松",18905599115]
[283,"KN95口罩（非医用）","安全防护类","日常生活中，空气污染环境下滤除颗粒物所佩戴的防护型口罩，要求佩戴各防护等级口罩后使吸入的PM2.5浓度降低至75微克每立方米以下，即过滤后吸入体内的空气质量达到良及以上水平。","个体防护 ","黄山安尔安卫生防护用品有限责任公司","黄山","高新区","高新区蓬莱路18号","聂万松",18905599115]
[284,"隔离衣","安全防护类","采用非织造布为主要原料，经裁剪、缝纫制成，非无菌提供，一次性使用。用于医疗机构门诊、病房、检验室等作普通隔离","个体防护 ","黄山泛帛工业有限公司","黄山","高新区","高新区梅林大道65号","江秋玲",15055984652]
[285,"医用隔离鞋套","安全防护类","采用非织造布为原材料制成，有足够的强度和阻隔性能。非无菌提供。医务人员在医疗机构中使用，防止接触到具有潜在感染性的患者血液、体液、分泌物等，起阻隔、防护作用","个体防护 ","黄山泛帛工业有限公司","黄山","高新区","高新区梅林大道65号","江秋玲",15055984652]
[286,"防水床罩、床套","安全防护类","主要产品为高档防水面料、各式防水床上用品等。产品具有防水、防湿、防螨虫、防渗透及透气的功能功效，其生产技术为目前国际领先水平","个体防护 ","黄山世达家用纺织品有限公司","黄山","高新区","高新区祁门路16号","阳芳",13685597839]
[287,"塔吊支架","安全防护类","塔吊支架采用型材、板材，包括主弦杆，斜腹杆，横杆和连接套。用于吊运材料，水平转运或垂直运输。","专用安全生产 ","黄山多杰电气有限公司","黄山","歙县","歙县经济开发区潭石路6号","刘录娟",18055978505]
[288,"隔离衣","应急救援处置类","采用非织造布为主要材料，经裁剪、缝纫制成。反穿式由前身、后身、袖子、系带等组成，袖口采用弹性收口。作为无菌服,在材料和设计上具备保护性、舒适性、作业方便性、审美性等基本性能","其他救援 ","合肥洁诺无纺布制品有限公司","合肥","肥东县","肥东县新城开发区来河路22号","张德满",13956012467]
[289,"一次性医用口罩","应急救援处置类","一次性医用口罩由面罩部分、鼻夹和口罩带组成，用途是使含有害物的空气通过口罩的滤料过滤后再被人吸入或者呼出，从而起到隔离作用","社会保障 ","金寨九信中药饮片有限公司","六安","金寨县","开发区金梧桐产业园","曾涛",13516483088]
[290,"一次性手术衣、手术铺单","应急救援处置类","企业生产一次性手术衣，主要用于手术科研人员进行手术、实验、研究时穿戴的隔离服。主要材质是无纺布、颜色有蓝色和绿色，该企业产品主要出口美国","社会保障 ","安徽尚德无纺科技有限公司","六安","金安区","金安区毛坦厂镇毛青路","姚大勇",17756421086]
[291,"医用防护服、一次性手术衣、一次性医用口罩","应急救援处置类","护服及手术衣由淋膜无纺布或无纺布经裁剪、贴胶、车缝等工序制作完成；防护服主要对临床医务人员在工作中接触到的具有潜在感染性的患者的血液、体液等提供阻隔防护用；手术衣主要用于普通医疗环境下的卫生护理；口罩主要用于防止病毒的传播","社会保障 ","安徽富美医疗科技有限公司","六安","裕安区","裕安区城南高新区","李林",15505646651]
[292,"医用隔离面罩","应急救援类","用于医疗机构中检查治疗时起防护作用，阻隔体液、血液飞溅或泼溅","社会保障 ","宁国市康宁悦康医疗器械有限公司","宣城","宁国市","宁国市东城大道众益工业广场7幢401号","甘纪华",13905638702]
[293,"儿童卫生口罩","应急救援类","适用于6岁及以上、14岁及以下，用于过滤空气中的颗粒物，阻隔微生物、花粉、飞沫等","社会保障 ","宁国市康宁悦康医疗器械有限公司","宣城","宁国市","宁国市东城大道众益工业广场7幢401号","甘纪华",13905638702]
[294,"KN95口罩","应急救援类","适用于日常工作环境下，过滤空气中的颗粒物，阻隔飞沫、体液、分泌物等","社会保障 ","宁国市康宁悦康医疗器械有限公司","宣城","宁国市","宁国市东城大道众益工业广场7幢401号","甘纪华",13905638702]
[295,"一次性医用口罩","应急救援处置类","可生产医用口罩等产品，具有低抗液体、过滤细小颗粒物和细菌等效用","社会保障 ","芜湖市伍月服装有限公司","芜湖","南陵县","南陵县家发镇工业集中区","林士娟",13606756425]
[296,"一次性医用口罩","应急救援处置类","一次性使用医用口罩由口罩体、鼻夹、口罩带组成。产品以无菌和非无菌提供；用于佩戴者在不存在体液和喷溅风险的普通医疗环境下的卫生护理","社会保障 ","安徽泾县裕生医疗器械有限公司","宣城","泾县","泾县经济开发区财富东路","崔  翔",18056339696]
[297,"医用外科口罩","应急救援处置类","医用外科口罩由口罩体、鼻夹、口罩带组成，产品以非无菌提供；供临床医护人员在有创操作过程中佩带、覆盖住使用者的口、鼻及下颚，为防止病原体微生物、体液、颗粒物等的直接透过提供物理屏障","社会保障 ","安徽泾县裕生医疗器械有限公司","宣城","泾县","泾县经济开发区财富东路","崔  翔",18056339696]
[298,"隔离衣","应急救援处置类","非无菌提供，一次性使用；用于医疗机构门诊、病房、检验室等作普通隔离","社会保障 ","安徽泾县裕生医疗器械有限公司","宣城","泾县","泾县经济开发区财富东路","崔  翔",18056339696]
[299,"医用帽","应急救援处置类","本产品采用非织造布、全棉布、涤棉布为主要原材料，经裁剪、缝纫或热合而成，非无菌提供，一次性使用。用于医疗机构门诊、病房、检验室等作普通隔离","社会保障 ","安徽泾县裕生医疗器械有限公司","宣城","泾县","泾县经济开发区财富东路","崔  翔",18056339696]
[300,"医用隔离面罩","应急救援处置类","本产品采用由高分子材料制成的防护罩、泡沫条和国定装置组成，非无菌提供，一次使用；用于医疗机构中检查治疗时起防护作用，阻隔体液、血液飞溅或波溅","社会保障 ","安徽泾县裕生医疗器械有限公司","宣城","泾县","泾县经济开发区财富东路","崔  翔",18056339696]
[301,"医用检查手套","应急救援处置类","通常采用聚录乙烯、橡胶等材料制造。有足够的强度和阻隔性能。非无菌提供，一次性使用；用于戴在医生或检查人员手上或手指上对患者病情进行检查或触检","社会保障 ","安徽泾县裕生医疗器械有限公司","宣城","泾县","泾县经济开发区财富东路","崔  翔",18056339696]
[302,"医用隔离鞋套","应急救援处置类","非无菌提供，一次使用；医务人员在医疗机构中使用，防止接触到具有潜在感染性的患者血液、体液、分泌物等，起阻隔、防护作用","社会保障 ","安徽泾县裕生医疗器械有限公司","宣城","泾县","泾县经济开发区财富东路","崔  翔",18056339696]
[303,"医用防护服","应急救援处置类","为临床医务人员在工作时接触到的具有潜在感染性的患者血液、体液、分泌物等提供阻隔、防护作用","社会保障 ","安徽爱维迈得医疗用品有限公司","宣城","经开区","宣城经开区创业路168号","柯永红",18605638060]
[304,"医用防雾防溅面罩","应急救援处置类","产品规格分套头式、镜架式、口罩式。主要由防溅片、支撑海绵和松紧带组成。主要用于医疗活动中操作者面部的保护","社会保障 ","安徽省小山卫生材料有限公司","宣城","绩溪县","绩溪县经开区会山路28号","周艳芬",13856353757]
[305,"一次性医用口罩","应急救援处置类","产品以非织造布为主要原料加工制成，适用于佩戴者在不存在体液和喷溅风险的普通医疗环境下的卫生护理。","社会保障 ","安徽省小山卫生材料有限公司","宣城","绩溪县","绩溪县经开区会山路29号","周艳芬",13856353758]
[306,"医用外科口罩","应急救援处置类","产品以非织造布为主要原料加工制成，用于戴在手术室医务人员口鼻部位，以防止皮屑、呼吸道微生物传播到开放的手术创面，并阻止手术病人的体液向医务人员传播，起到双向生物防护的作用。","社会保障 ","安徽省小山卫生材料有限公司","宣城","绩溪县","绩溪县经开区会山路30号","周艳芬",13856353759]
[307,"一次性口罩","应急救援处置类","日常阻挡飞沫，粉尘。有阻隔血液、体液、飞溅物的作用，同时也能起到较好的防护作用","个体防护 ","安徽雷火医疗科技有限公司","安庆","望江县","望江县经开区蓝天路23号","钟瑞华",15800000759]
[308,"Kn95口罩、一次性口罩","应急救援处置类","对空气中的各类粉尘、非油性颗粒物、以及空气中的病毒有一定的防护作用","个体防护 ","安徽科浦环保科技有限公司","安庆","望江县","望江县经开区鸦滩路与白云路交汇处","柯结军",13955631682]
[309,"隔离衣、民用防护服","应急救援处置类","用于医疗机构门诊、病房、检验室等作普通隔离","个体防护 ","安徽百川纳包装制品有限公司","安庆","望江县","望江县经开区白云北路8号","余志才",18055612989]
["二、监测预警类（168种）"]
[1,"中新金盾抗拒绝服务系统","监测预警类","中新金盾抗拒绝服务系统是抗分布式拒绝服务攻击高性能解决方案，已应用于国家关键基础设施、政府及企事业单位，提供强大的DoS/DDoS攻击防护能力","公共卫生事件监测预警 ","中新网络信息安全股份有限公司","合肥","合肥高新区","创新大道2688号","周圣君",18605518842]
[2,"中新金盾下一代防火墙","监测预警类","中新金盾第二代防火墙是款自主可控的安全网关产品，产品具有一体化全方位防御、智能应用识别、全方位可视化与管控等性能优势，可广泛加强政府等各个机关部门的网络安全","社会安全事件监测预警 ","中新网络信息安全股份有限公司","合肥","合肥高新区","创新大道2688号","周圣君",18605518842]
[3,"H3C SecPath F1000-AI","监测预警类","H3C SecPath F1000-AI系列防火墙面向行业市场的高性能多千兆和超万兆防火墙VPN集成网关产品，硬件上基于多核处理器架构，为1U的独立盒式防火墙。","通用监测预警 ","新华三信息安全技术有限公司","合肥","合肥高新区","创新大道与彩虹路交口","陈文艳",18600090486]
[4,"H3C SecPath T1000-AI系列入侵防御系统","监测预警类","H3C SecPath T1000-AI系列IPS产品部署在客户网络的关键路径上，通过对流经该关键路径上的网络数据流进行4到7层的深度分析，能精确、实时地识别并阻断或限制黑客、蠕虫、病毒、木马、DoS/DDoS、扫描、间谍软件、协议异常、网络钓鱼、P2P、IM、网游等网络攻击或网络滥用，同时，H3C SecPath T1000-AI系列产品还具有强大、实用的带宽管理和URL过滤功能。","通用监测预警 ","新华三信息安全技术有限公司","合肥","合肥高新区","创新大道与彩虹路交口","陈文艳",18600090486]
[5,"H3C SecPath L1000-AK系列负载均衡器","监测预警类","H3C SecPath L1000-AK系列产品开创性地实现了负载分担、安全与网络的深度融合，具有强大的路由、交换、负载均衡、2~7层安全防护等功能。","通用监测预警 ","新华三信息安全技术有限公司","合肥","合肥高新区","创新大道与彩虹路交口","陈文艳",18600090486]
[6,"山地防洪综合监测预警系统","监测预警类","为山地防洪提供事前指导、 全程实时监视和事后分析，增进了国内对极端天气局部强降雨及次生灾害。监测预测的认识。","通用监测预警 ","四创电子股份有限公司","合肥","合肥高新区","习友路3366","潘芸芸",15155957017]
[7,"城市视频监控系统","监测预警类","为公安实战业务应用产品，面向公安、政府、公众构建视频图像共性应用，提供视频图像专业应用和视频图像专题应用。","社会安全事件监测预警 ","四创电子股份有限公司","合肥","合肥高新区","习友路3366","潘芸芸",15155957017]
[8,"智慧公安产品","监测预警类","智能化汇总梳理案件信息，提升公安应急办案管理水平，提高办案效率。","社会安全事件监测预警 ","科大讯飞股份有限公司","合肥","合肥高新区","望江西路666号","张莹莹","0551-65331880"]
[9,"智慧电梯物联网安全监管平台、","监测预警类","平台基于物联网、大数据和人工智能技术，实现电梯安全运行的实时监控和故障预警，保障社会公众的乘梯安全","社会安全事件监测预警 ","科大国创云网科技有限公司","合肥","合肥高新区","文曲路355号办公楼4层","陈娇娇",18055160556]
[10,"小麦四情监测系统","监测预警类","建设物联网点，利用可视化、远程化等手段，对小麦种植、田管、收割、抗灾工作进行诊断、会商、指挥和调度","自然灾害监测预警 ","科大国创云网科技有限公司","合肥","合肥高新区","文曲路355号办公楼4层","陈娇娇",18055160556]
[11,"现代农业园区监测评估信息系统","监测预警类","系统对园区进行智能化的管理分析，为农业科研、开发和成果转化提供成功范例，进而大幅度提高农业经济效益","自然灾害监测预警 ","科大国创云网科技有限公司","合肥","合肥高新区","文曲路355号办公楼4层","陈娇娇",18055160556]
[12,"科大国创瓶安宝产品","监测预警类","甁安宝基于移动互联网和RFID技术，打通气瓶检测、充装和使用环节的流程和数据，实现气瓶的智慧监管","社会安全事件监测预警 ","科大国创云网科技有限公司","合肥","合肥高新区","文曲路355号办公楼4层","陈娇娇",18055160556]
[13,"智慧灯杆监控平台","监测预警类","以集成音视频监控设备、无线基站、WIFI、多媒体、充电桩及天气、环境等各种感知器的照明灯杆为智能终端，依托云计算管理平台构建城市物联网，实现智能安防、照明、城市感知，以及智慧交通、智慧市政、智慧能源等应用","社会安全事件监测预警 ","科大国创软件股份有限公司","合肥","合肥高新区","文曲路355号","刘青梅",15156218168]
[14,"智慧管廊监控平台","监测预警类","以物联网、大数据、BIM、GIS等技术，建设城镇综合管廊智慧管控一张图和智慧运营服务、智慧应急、大数据分析等系统平台，覆盖综合管廊项目全生命周期，实现综合管理规划、建设、运行、维护及管理、服务的智慧化","社会安全事件监测预警 ","科大国创软件股份有限公司","合肥","合肥高新区","文曲路355号","刘青梅",15156218168]
[15,"网络安全监控产品","监测预警类","对网络安全全流程监控，提升网络与信息系统安全监测预警应急处置能力","公共卫生事件监测预警 ","合肥中能电力科技有限公司","合肥","合肥高新区","习友路1682号","王文丽",18255194559]
[16,"光纤光栅温度与间隙复合传感系统","监测预警类","采用温度和间隙双参量传感，实现多点、准分步监测，用于飞行器安全监测，大型建筑温度、火灾的监控等","建筑业","合肥正阳光电科技有限责任公司","合肥","合肥高新区","望江西路527号","谷永波",17730230830]
[17,"高精度惯性测量设备","监测预警类","是一种测量航向和姿态角的高精度惯性测量设备。用于舰艇、舰载测量设备及雷达的应急通信","社会安全事件监测预警 ","合肥正阳光电科技有限责任公司","合肥","合肥高新区","望江西路527号","谷永波",17730230830]
[18,"光通信产品","监测预警类","以光波为载波进行通信。用于数字阵列雷达、对抗、信号处理系统等领域的应急通信。","社会安全事件监测预警 ","合肥正阳光电科技有限责任公司","合肥","合肥高新区","望江西路527号","谷永波",17730230830]
[19,"智慧工地云平台","监测预警类","软件产品，建筑安全监测，提升建筑施工安全监测和应急处置能力","建筑业","合肥优尔电子科技有限公司","合肥","合肥高新区","大学园","周柱霞",18205606360]
[20,"热像望远镜在线测温仪","监测预警类","利用热像技术在线监测，提升应急安全监测能力","采矿业","合肥英睿系统技术有限公司","合肥","合肥高新区","望江西路800号创新产业园一期C3栋301室","虞敏",18155239463]
[21,"智能交通超限超载动态检测系统","监测预警类","交通安全监测预警产品，主要防范灾害的发生，及安全隐患消除，应用于现代交通领域的安全防控，安全应急，安全救治，安全预防等方面","道路运输业","合肥正茂科技有限公司","合肥","合肥高新区","科学大道92号","李红荣",18255162936]
[22,"智能网关系列产品","监测预警类","智能网关采用SD-WAN技术，根据业务需求和负载均衡自适应选择无线（5G）或有线（光纤、同轴电缆）等WAN口接入。整个系统极大提高了应急安全条件下的通信能力","社会安全事件监测预警 ","合肥润东通信科技股份有限公司","合肥","合肥高新区","银杏路108号","胡海丽",18656017399]
[23,"智慧安全检查站","监测预警类","通过前端安检系统与后端管控平台相结合，实现对人、车、物、证、码多要素的全面管控，打造区域外防输入、内防输出的安全检查应急防控圈","社会安全事件监测预警 ","合肥品恩智能科技有限公司","合肥","合肥高新区","望江西路800号动漫基地C3楼5层","张婷婷",15056967075]
[24,"色选机","监测预警类","根据物料光学特性的差异，利用光电探测技术将物料中的病变、霉变、异色颗粒自动分拣出来的设备","其他监测预警 ","合肥美亚光电技术股份有限公司","合肥","合肥高新区","望江西路与文曲路交口","郑贤勇","0551-65312947"]
[25,"X射线工业检测机","监测预警类","采用多重智能识别算法和领先的光源、传感器等配置，具有优质可靠的图像获取能力，适用于散装物料中金属、玻璃、石子等异物识别","采矿业","合肥美亚光电技术股份有限公司","合肥","合肥高新区","望江西路与文曲路交口","郑贤勇","0551-65312947"]
[26,"雷电探测预警系统","监测预警类","气象灾害监测预警产品，用于雷电预警监测，减少灾害损失","水利、环境和公共设施管理业","合肥佳讯科技有限公司","合肥","合肥高新区","杨林路11号","赵莹",13865996870]
[27,"化学气体红外遥感监测设备","监测预警类","监测燃气、石油、化工、煤炭等行业的化学气体泄漏，快速准确识别气体，定量计算气体浓度，精确定位泄漏源","电力、热力、燃气及水生产和供应业","合肥博雷电气有限公司","合肥","合肥高新区","香樟大道168号科技实业园C5二层","陈阿松",18755193569]
[28,"高速高分辨率扫描相机","监测预警类","具有高分辨率和高速扫描的特点，可清晰、快速地抓取并识别画面，广泛应用于交通、生产安全监测预警场景中","道路运输业","合肥埃科光电科技有限公司","合肥","合肥高新区","燕子河路388号亿智科技产业园1号楼","周雅静",13515664612]
[29,"新冠抗体IgM/IgG检测（胶体金法）","监测预警类","SARS-CoV-2抗体是患者在新冠病毒抗原刺激下产生的，抗体检测可以间接证实新冠病毒感染，可以为中后期感染提供佐证。","公共卫生事件监测预警 ","必欧瀚生物技术（合肥）有限公司","合肥","合肥高新区","孔雀台路与长安路交口东北角必欧瀚生物产业园","李纳",15155154681]
[30,"新冠抗原Elisa检测（酶联免疫法）","监测预警类","检测血液中的病毒蛋白，可用于早期诊断","公共卫生事件监测预警 ","必欧瀚生物技术（合肥）有限公司","合肥","合肥高新区","孔雀台路与长安路交口东北角必欧瀚生物产业园","李纳",15155154681]
[31,"新冠抗原快速检测（荧光免疫层析法）","监测预警类","检测血液中的病毒蛋白，可用于早期诊断","公共卫生事件监测预警 ","必欧瀚生物技术（合肥）有限公司","合肥","合肥高新区","孔雀台路与长安路交口东北角必欧瀚生物产业园","李纳",15155154681]
[32,"食品安全检验检测","监测预警类","药品食品安全监测预警产品，用于食品的安全监测，保障食品安全","公共卫生事件监测预警 ","安徽中青检验检测有限公司","合肥","合肥高新区","合欢路30号","韩红艳",18949829710]
[33,"电动客车锂离子动力电池(箱)火灾防控产品","监测预警类","系统能实时监测电池箱内部环境，实现早期火灾感知、智能判断、提前干预并高效灭火，保护司乘人员安全","道路运输业","安徽中科中涣防务装备技术有限公司","合肥","合肥高新区","创新大道2800号创新产业园二期F3楼907室","刘丽",13399693777]
[34,"电化学储能系统火灾抑制装置、","监测预警类","产品广泛应用于各种电化学储能系统，具备精准探测、高效防护等特点，为行业内客户提供一站式消防安全解决方案","社会安全事件监测预警 ","安徽中科中涣防务装备技术有限公司","合肥","合肥高新区","创新大道2800号创新产业园二期F3楼907室","刘丽",13399693777]
[35,"公共汽车固定客舱灭火系统","监测预警类","主要用于公共汽车车厢内扑灭。采用高效水剂为灭火介质，利用直流电机泵为驱动，通过特殊雾化喷头喷洒，快速灭火","社会安全事件监测预警 ","安徽中科中涣防务装备技术有限公司","合肥","合肥高新区","创新大道2800号创新产业园二期F3楼907室","刘丽",13399693777]
[36,"易燃挥发物检测告警装置","监测预警类","为公交车纵火预警产品，内置MEMS气体传感器，可快速识别乘客携带的易燃挥发物液体,有利于及时应对纵火事件","社会安全事件监测预警 ","安徽中科中涣防务装备技术有限公司","合肥","合肥高新区","创新大道2800号创新产业园二期F3楼907室","刘丽",13399693777]
[37,"公交智能化系统","监测预警类","城市公共安全监测预警产品、网络与信息系统安全监测预警产品、突发事件通用监测预警产品，应用于各种设备数字化的安全防护。数码监控报警的性能特点是：监控画面实时显示，录像图象质量单路调节功能，每路录像速度可分别设置，快速检索，多种录像方式设定功能，自动备份，云台/镜头控制功能，网络传输等","社会安全事件监测预警 ","安徽云智科技信息股份有限公司","合肥","合肥高新区","创新产业园二期H区6号楼","符贵","0551-63623066-8027"]
[38,"网络安全防火墙","监测预警类","城市公共安全监测预警产品、网络与信息系统安全监测预警产品、突发事件通用监测预警产品，主要产品摄像机，摄像头，用于山体滑坡，地质灾害，洪水监控","社会安全事件监测预警 ","安徽云智科技信息股份有限公司","合肥","合肥高新区","创新产业园二期H区6号楼","符贵","0551-63623066-8027"]
[39,"安全监控设备","监测预警类","城市公共安全监测预警产品、网络与信息系统安全监测预警产品、突发事件通用监测预警产品，主要产品摄像机，摄像头，用于山体滑坡，地质灾害，洪水监控","水利、环境和公共设施管理业","安徽云智科技信息股份有限公司","合肥","合肥高新区","创新产业园二期H区6号楼","符贵","0551-63623066-8027"]
[40,"监所智能应用平台","监测预警类","有效地协助安全人员处理危机，并最大限度地降低误报和漏报现象。","水利、环境和公共设施管理业","安徽新华博信息技术股份有限公司","合肥","合肥高新区","红枫路33号","刘青霞",13805517126]
[41,"公交车易燃挥发物检测告警装置","监测预警类","采用MEMS薄膜半导体气敏传感器技术，在敏感薄膜表面修饰不同高活性金属催化纳米微粒实现对不同气体的选择性功能。对公共交通车厢内汽油、酒精、松油等易燃挥发物进行监测，浓度达到时发出声光告警。","社会安全事件监测预警 ","安徽芯核防务装备技术股份有限公司","合肥","合肥高新区","望江西路800号D8楼2034号","黄胜男",13675601408]
[42,"新能源公交车锂电池火灾防控装置","监测预警类","采用多模传感器复合探测技术和非储压气体发生器技术。集成光电、烟雾、温度、一氧化碳等多个传感器，有效识别电池箱火情并发出告警。收到探测器指令或手动指令时，气体发生器毫秒级响应点火，推动活塞将全氟己酮雾化并释放，实现电池箱的火灾快速探测及有效抑制。","水利、环境和公共设施管理业","安徽芯核防务装备技术股份有限公司","合肥","合肥高新区","望江西路800号D8楼2034号","黄胜男",13675601408]
[43,"水质在线监测仪","监测预警类","水质在线监测仪系列产品可精准监测水质氨氮、总磷、COD等指标，在线监测并预警水质情况，是环境监管部门实现有效监测水源环境变化因子、控制环境污染的重要技术手段，主要用于污水处理、水质监测等领域","自然灾害监测预警 ","安徽皖仪科技股份有限公司","合肥","合肥高新区","望江西路与文曲路交口","赵楠楠","0551-68107045"]
[44,"VOCS在线监测系统","监测预警类","VOCS在线监测系统可在线监测气体中非甲烷总烃及苯系物等挥发性有机物的浓度及含量，实现环境中有机污染物在线监测及预警，并广泛应用于石化化工、精细化学、生物制药、印刷喷涂等行业","水利、环境和公共设施管理业","安徽皖仪科技股份有限公司","合肥","合肥高新区","望江西路与文曲路交口","赵楠楠","0551-68107045"]
[45,"智能应急指挥箱、ICVS云视频管理平台","监测预警类","智能应急指挥箱是一款功能全面、携带方便的多网融合智能通信产品，为实现应急指挥的“通信畅通、现场及时、数据完备、指挥到位”提供技术保障","社会安全事件监测预警 ","安徽清新互联信息科技有限公司","合肥","合肥高新区","创新大道2800号创新产业园二期J1区A座","汪莉莉",15375439298]
[46,"双光谱热成像测温仪","监测预警类","针对多人同时进出场景监控的热成像测温仪。产品具有热成像高精度多人测温、全实时测温、                                                                                                                                                                                                  多点异常体温报警等功能，可高效完成非接触式人员体温快速筛查、人体测温登记等人流量较                                                                                                                                                              大的公共场合体温快速排查工作，部署方便快捷，应用场景丰富","社会安全事件监测预警 ","安徽清新互联信息科技有限公司","合肥","合肥高新区","创新大道2800号创新产业园二期J1区A座","汪莉莉",15375439298]
[47,"人脸测温平板","监测预警类","集“测温+身份验证+考勤”功能于一体的智能终端。","公共卫生事件监测预警 ","安徽清新互联信息科技有限公司","合肥","合肥高新区","创新大道2800号创新产业园二期J1区A座","汪莉莉",15375439298]
[48,"应急指挥调度平台","监测预警类","平台结合前端应急终端，组成了一个功能完善的应急指挥调度系统，可广泛应用公安、城管、消防、武警、人防、边防等应急行业","水利、环境和公共设施管理业","安徽清新互联信息科技有限公司","合肥","合肥高新区","创新大道2800号创新产业园二期J1区A座","汪莉莉",15375439298]
[49,"物联网大数据平台","监测预警类","物联网大数据平台是通过无线网络，以视频为核心，将各种传感器采集到的数据汇聚到大数据平台，进行数据分析统计，以一张图的形式，对当前状态和未来趋势进行概况展示，数据预警，可对接相关部门应急预案","事故灾害监测预警 ","安徽清新互联信息科技有限公司","合肥","合肥高新区","创新大道2800号创新产业园二期J1区A座","汪莉莉",15375439298]
[50,"消防信息传输控制单元","监测预警类","装置具备采集、规转、控制和网关等功能，将接收到的火灾相关信息发送给辅助设备集中监控系统，并将辅助设备集中监控系统下发的控制指令发送给相关消防设施。可适用于变电站内各种消防设施监控","社会安全事件监测预警 ","安徽南瑞继远电网技术有限公司","合肥","合肥高新区","科学大道90号","王丽",18505511291]
[51,"输电线路防山火在线监测装置","监测预警类","装置采用红外热成像山火探测技术，通过有线或无线通讯方式将图像传输到主站系统，实现线路周边山火的全天候在线监测及预警，可以有效辅助运维部门做到火情早发现、早扑灭，保障电网安全运行。适用于春节、春耕、上坟祭祖、秸秆焚烧等易发生山火线路区段","事故灾害监测预警 ","安徽南瑞继远电网技术有限公司","合肥","合肥高新区","科学大道90号","王丽",18505511291]
[52,"智能双目摄像机","监测预警类","内嵌深度学习算法，以海量图片及视频资源为路基，通过机器自身提取目标特征，形成深层可供学习的人脸图像。极大的提升了目标人脸的检出率，适用于公共场所、变电站、营业厅、车站、航站楼等环境","社会安全事件监测预警 ","安徽南瑞继远电网技术有限公司","合肥","合肥高新区","科学大道90号","王丽",18505511291]
[53,"网络全景摄像机","监测预警类","全景球机集成了先进的视频分析算法和多目标跟踪算法程序，可实现自动或手动对全景区域内的多个目标进行侦测，满足高等级要求的安保需求。可广泛适用于变电站、机场、车站、体育馆、操场、景区、广场等需要大范围监控和细节捕捉的场景","社会安全事件监测预警 ","安徽南瑞继远电网技术有限公司","合肥","合肥高新区","科学大道90号","王丽",18505511291]
[54,"输电线路导线覆冰监测装置","监测预警类","装置采用线路图像实时监视及检测导线拉力综合方法来监测架空线路覆冰，可对线路覆冰形成的气象条件、覆冰形成过程和覆冰的严重程度进行全过程的实时监测。不仅能支持告警实时抓拍图片、传输实时视频，也能监测线路拉力和倾角数据。","事故灾害监测预警 ","安徽南瑞继远电网技术有限公司","合肥","合肥高新区","科学大道90号","王丽",18505511291]
[55,"输电线路微气象在线监测装置","监测预警类","装置实时采集线路通道环境温度、湿度、风速、风向、雨量、气压、日照等气象参数，，实时监测输电线路微气象区的气象变化，为线路安全运行提供保障。装置适用于大跨越、易覆冰区和强风区等特殊区域区段、因气象因素导致故障频发的线路区段，及传统气象监测盲区","电力、热力、燃气及水生产和供应业","安徽南瑞继远电网技术有限公司","合肥","合肥高新区","科学大道90号","王丽",18505511291]
[56,"输电线路导线温度在线监测装置","监测预警类","装置利用线上导线温度采集单元检测导线温度，实现远程实时监测导线（金具）温升及杆塔周边的气象状况，对线路动态增容及安全运行提供参考依据。装置宜安装在需要提高线路输送能力的重要线路和跨越主干铁路、高速公路、桥梁、河流、海域等区域的重要跨越段","事故灾害监测预警 ","安徽南瑞继远电网技术有限公司","合肥","合肥高新区","科学大道90号","王丽",18505511291]
[57,"智能一体化电源","监测预警类","电源系统主要应用在电力系统各等级变电站；发电系统发电厂；轨道交通变配电系统；工矿企业配电系统；港口岸电、能源化工、智能楼宇等领域的交直流电源系统","事故灾害监测预警 ","安徽南瑞继远电网技术有限公司","合肥","合肥高新区","科学大道90号","王丽",18505511291]
[58,"智能电能质量治理装置","监测预警类","装置采用电力电子功率单元，实时检测系统负载电流，运算分析得到各相需的输出电流，综合解决配电台区无功、谐波、三相负荷不平衡以及电压波动等问题。可适用于配电台区、机械制造、通讯、医疗行业、石油化工等行业","事故灾害监测预警 ","安徽南瑞继远电网技术有限公司","合肥","合肥高新区","科学大道90号","王丽",18505511291]
[59,"蓄电池在线监测与维护系统","监测预警类","具备测量、诊断和维护功能，有效规避电池组解列、电池开路和单节电池故障等事故的发生，提高运行维护效率，减轻巡视负担","事故灾害监测预警 ","安徽南瑞继远电网技术有限公司","合肥","合肥高新区","科学大道90号","王丽",18505511291]
[60,"能源路由器成套设备","监测预警类","提高对分布式电源的接纳，实现接入的电能质量管理以及电能分配，极大的提升了用电安全，广泛应用于机房于数据中心、智慧照明、直流楼宇、直流微网等场景","社会安全事件监测预警 ","安徽南瑞继远电网技术有限公司","合肥","合肥高新区","科学大道90号","王丽",18505511291]
[61,"避雷器绝缘在线监测装置","监测预警类","装置可以实时监测氧化锌避雷器的泄漏电流和动作次数来实现动态监测避雷器的绝缘状况。有效监测避雷器内部受潮导致的绝缘劣化及元件异常等发生的故障，提高运行维护效率，减轻巡视负担","事故灾害监测预警 ","安徽南瑞继远电网技术有限公司","合肥","合肥高新区","科学大道90号","王丽",18505511291]
[62,"智能交通管控平台","监测预警类","集高新技术应用为一体的智能化指挥调度集成平台，实现信息交换与共享、快速反应决策与统一调度指挥等，用于提升交通管控应急处置能力","社会安全事件监测预警 ","安徽科力信息产业有限责任公司","合肥","合肥高新区","蜀山区黄山路628","余江","0551-5338237"]
[63,"交通应急快速反应系统","监测预警类","按照“情、指、勤、督”业务新模式，为及时发现和处置突发交通事件、分析周期性拥堵成因、提出缓堵措施提供技术支撑","道路运输业","安徽科力信息产业有限责任公司","合肥","合肥高新区","蜀山区黄山路628","余江","0551-65338996"]
[64,"交通信号控制系统","监测预警类","支持国标联网联控模式，具备可视集中管控、多场景应用、任务流程化、多层次分析、全方位检测、安全性保障等特色的功能","事故灾害监测预警 ","安徽科力信息产业有限责任公司","合肥","合肥高新区","蜀山区黄山路628","余江","0551-65338996"]
[65,"道路交通警用无人机管控系统","监测预警类","空地一体化情指勤督为导向，解决交通事件中人员车辆无法快速到达现场的难题，构建自动巡逻机制","事故灾害监测预警 ","安徽科力信息产业有限责任公司","合肥","合肥高新区","蜀山区黄山路628","余江","0551-65338996"]
[66,"科大国创血液透析管理系统","监测预警类","是一套专门面向国内医疗透析的行业的信息化产品，结合当前国内血透行业的特点并借鉴了国外血液透析行业信息化的设计理念。","公共卫生事件监测预警 ","安徽科大国创软件科技有限公司","合肥","合肥高新区","文曲路355号",null,18326186575]
[67,"城市公共安全应急平台","监测预警类","动态采集城市公共场所场景信息，对城市公共安全威胁源头提前预警，提升城市公共安全监测预警应急治理能力","水利、环境和公共设施管理业","安徽鼎信科技集团有限公司","合肥","合肥高新区","望江西路800号动漫基地A4楼701室","周林蔚","0551-62753881"]
[68,"起重机","监测预警类","主要生产、制造各类起重设备、KBK轻型起重机、电动葫芦、动力驱动技术产品以及零部件，产品范围广泛，组建和设备的标准化程度高，且性能稳定，质量可靠","事故灾害监测预警 ","安徽德马泰格起重机械有限公司","合肥","合肥高新区","南岗科技园长宁大道2658号","张派生",15155164546]
[69,"道路安全预警系统","监测预警类","道路交通安全监测，对道路全方位省市监控，及时预警，保障道路安全运营的同时，强化道路突发事件应急处置能力","道路运输业","安徽超远信息技术有限公司","合肥","合肥高新区","文曲路919号","董连芳",13956003493]
[70,"测速仪","监测预警类","对违法违章车辆进行实时监测、实时报警、实时显示，达到现场处理违章超速车辆的目标，增加了文明执法手段","社会安全事件监测预警 ","安徽百诚慧通科技有限公司","合肥","合肥高新区","创新大道2800号创新产业园二期H2楼262室","邱云娟",13855658267]
[71,"区间测速系统","监测预警类","系统集车辆检测、超速抓拍、高清抓拍取证、车辆特征识别、等于一体，结构简单、性能稳定、可靠性高","道路运输业","安徽百诚慧通科技有限公司","合肥","合肥高新区","创新大道2800号创新产业园二期H2楼262室","邱云娟",13855658267]
[72,"电梯大数据平台","监测预警类","通过引入了互联网思维建设多元评价体系，让评价成为推动维保企业、维保技师、物业管理者担当的原动力。将电梯使用投诉无门、电梯故障反馈低效、被困救援响应慢、完全依赖政府监管的电梯安全问题，变成全民都可以参与监督和管理的阳光化工程","建筑业","安徽奥里奥克科技股份有限公司","合肥","合肥高新区","习友路与香樟大道交口深港城3幢","张海艳",13665693383]
[73,"火灾安全监控报警系统","监测预警类","采用分布式处理架构，由前端设备层、数据传输层及集中管理层构成，前端设备层通过多光谱视频图像的实时分析处理，实现大规模监控场所的非接触式火灾探测报警功能，具有独立式、智能化、可视化、准确度高的特点。 适用于石油、化工、煤矿、天然气等各类易燃易爆工业场所","石油、煤炭及其燃料加工业","合肥科大立安安全技术股份有限公司","合肥","合肥高新区","蜀山区天湖路13号","汪娟娟","0551-68109586"]
[74,"智能视频火灾分析系统","监测预警类","本系统基于计算机视觉图像AI智能识别技术，采用高性能并行计算服务器硬件平台，接入前端已有网络摄像机，通过视频流数据智能化分析完成烟火探测功能，实现了存量摄像机设备的智能化火灾监测和早期火灾预警AI赋能，解决了海量摄像机数据的7*24H人工监控筛选的痛点；适用基于安防监控系统附加火灾探测功能的新建或扩建工程项目，有效提升消防管理水平","事故灾害监测预警 ","合肥科大立安安全技术股份有限公司","合肥","合肥高新区","蜀山区天湖路13号","汪娟娟","0551-68109586"]
[75,"点型红外火焰探测系统","监测预警类","点型红外火焰探测器基于双波段红外热释电探测技术，能够有效探测含碳燃料产生的明火燃烧，火灾初期以火焰为主的各种场合。可广泛应用于公路隧道、弹药和爆炸品仓库、油漆工厂、石油化工企业、制药企业、发电站、印刷企业、易燃材料仓库等含碳可燃物质的场所","事故灾害监测预警 ","合肥科大立安安全技术股份有限公司","合肥","合肥高新区","蜀山区天湖路13号","汪娟娟","0551-68109586"]
[76,"自动消防炮灭火系统","监测预警类","该系统是以流量大于16L/s水或泡沫混合液为射流介质,利用火灾自动探测进行早期火灾的自动跟踪定位，并运用自动控制方式来实现射流灭火的灭火系统。适用于室内体育馆、会展中心、火车站、飞机场候机楼、石化、发电厂等大空间特殊场所","事故灾害监测预警 ","合肥科大立安安全技术股份有限公司","合肥","合肥高新区","蜀山区天湖路13号","汪娟娟","0551-68109586"]
[77,"消防设施监测主机","监测预警类","消防设施监测主机是通过NB-IoT、LoRa和RJ45、RS232、RS485等通信方式，实现电气火灾报警系统、自动喷水灭火系统、消防给水及消火栓系统等消防物联网设备的数据采集和管理，图形化数据展示，存储，统计和分析。","事故灾害监测预警 ","合肥科大立安安全技术股份有限公司","合肥","合肥高新区","蜀山区天湖路13号","汪娟娟","0551-68109586"]
[78,"消防物联网信息网关","监测预警类","依靠物联网和云计算这两项核心技术，使所有消防建筑内的消防报警系统统一起来，改变过去的每个场所都是“孤岛”的不利局面。有助于实现第一时间掌握火警，为火灾的警情确认提供及时的现场信息，为扑救赢得宝贵的救援时间","事故灾害监测预警 ","合肥科大立安安全技术股份有限公司","合肥","合肥高新区","蜀山区天湖路13号","汪娟娟","0551-68109586"]
[79,"火灾报警装备","监测预警类","采用红外+蓝光双光探测，可以判断粒子大小，区分火灾烟雾颗粒和灰尘、水蒸气颗粒，极大降低灰尘、水蒸气引起的误报。可广泛用于住宅、“三合一”场所、养老院、福利院、残疾人服务机构、特困人员供养服务机构等火灾易发、多发场所的火灾安全监控","事故灾害监测预警 ","合肥科大立安安全技术股份有限公司","合肥","合肥高新区","蜀山区天湖路13号","汪娟娟","0551-68109586"]
[80,"消防泵房前端感知系列产品","监测预警类","消防泵房前端感知系列产品是基于LoRa通信技术，具有开关量和模拟量采集的低功耗物联网产品，用于实时监测消防设施中的阀门、管网水压、消防泵、电气控制柜的工作状态，实现消防泵房设施的物联网监测功能","事故灾害监测预警 ","合肥科大立安安全技术股份有限公司","合肥","合肥高新区","蜀山区天湖路13号","汪娟娟","0551-68109586"]
[81,"建筑消防水系统监测装备","监测预警类","有效监测室外消火栓水压不足、低温结冰及非法盗水风险，为及早发现和排查隐患提供数据支持。电池型电子水位监测仪主要用于消防水池或消防水箱等需要监测水位的场合，设备可长期稳定运行 并可实时上报水位实时测量值或报警值","事故灾害监测预警 ","合肥科大立安安全技术股份有限公司","合肥","合肥高新区","蜀山区天湖路13号","汪娟娟","0551-68109586"]
[82,"智能末端试水系统","监测预警类","该系统由智能末端试水装置控制器、末端试水装置及相关附件组成，对喷淋管网和防火分区的最不利点处采集流量、压力和水温数据，进行数据分析判断是否故障，并与报警阀组、水力警铃、水流指示器等进行联动，在火灾发生时达到最好的灭火效果。适用于建筑消防喷淋管网末端","事故灾害监测预警 ","合肥科大立安安全技术股份有限公司","合肥","合肥高新区","蜀山区天湖路13号","汪娟娟","0551-68109586"]
[83,"防火门监测仪","监测预警类","支持双边检测体积小，安装便捷，低功耗，使用寿命长。防火门监测仪用于建筑物内防火门开关状态的实时监测，由信号采集传输装置和门磁感应器两个部分组成，实现门开关监测、报警上传、NB无线通信、远程配置查询参数等功能","事故灾害监测预警 ","合肥科大立安安全技术股份有限公司","合肥","合肥高新区","蜀山区天湖路13号","汪娟娟","0551-68109586"]
[84,"轨道交通智能化产品","监测预警类","通过轨道交通综合监控系统，能够实现对轨道交通中电力系统、火灾自动报警、环控、信息显示等机电系统设备监视和控制功能；可以实现紧急突发情况下各系统设备之间协调互动的联动功能","铁路、船舶、航空航天和其他运输设备制造业","合肥赛为智能有限公司","合肥","合肥高新区","创新大道666号","张媛媛",15056044790]
[85,"数据挖掘与录入服务产品","安全应急服务类","通过数据深度挖掘，确保信息系统数据安全。","其他安全应急服务 ","赛智（合肥）信息科技有限公司","合肥","合肥高新区","科学大道110号F地块F9B四层","陈星衡","0551-65318178"]
[86,"安全教育培训软件","安全应急服务类","应急安全教育培训软件，可以作为常态化或应急情况下安全教育培训","教育培训 ","合肥志诚教育股份有限公司","合肥","合肥高新区","创新产业园二期F1楼16楼整层","金全荣","0550-63850724"]
[87,"公共安全VR体验软件开发","安全应急服务类","安全应急体验、演练等软件开发","水利、环境和公共设施管理业","合肥耀安科技有限公司","合肥","合肥高新区","天元路3号留学生园2号楼306/311室","张可","0551-65390861"]
[88,"消防、气象、地震、应急、人防安全科普","安全应急服务类","消防、气象、地震、应急、人防安全科普设计，从立项咨询、可研分析、概念设计、深化设计、研发生产，落地安装、布展施工、人员培训到托管运维的全过程服务。消防、气象、地震、应急、人防安全科普文化建设","教育培训 ","合肥探奥自动化有限公司","合肥","合肥高新区","明珠大道与创新大道交口西北","徐龙梅",13855191114]
[89,"地震科普展示产品","安全应急服务类","通过趣味互动，让观众体验多个不同等级的地震效果，感受不同烈度的地震所带来的危害，学习掌握相关的避险防灾知识，提高民众在面临二次灾害时的自救能力","水利、环境和公共设施管理业","合肥金诺数码科技股份有限公司","合肥","合肥高新区","动漫产业基地","刘勇",17355101760]
[90,"放射现场检测与评价","安全应急服务类","检测认证服务，用于放射源监测，预防放射危害","化学原料和化学制品制造业","合肥金浩峰检测研究院有限公司","合肥","合肥高新区","创新产业园二期G4楼D区3层","崔云云",18005694347]
[91,"安全云平台","安全应急服务类","通过自有的云研发团队及容灾云管理服务平台，为客户提供数据备份、数据容灾和行业云的解决方案，保障客户的数据安全和业务连续","应急救援 ","合肥城市云数据中心股份有限公司","合肥","合肥高新区","玉兰大道767号机电产业园西二路科大国祯大厦二层、四层","刘孟捷",13866784817]
[92,"云计算+服务+数据","安全应急服务类","采用自主研发的运营平台（CCDCSM），整合客户侧和城市云的云计算资源，叠加技术服务能力和运维管理能力，向客户提供混合云服务，助力客户业务数字化转型，达到提质增效目的","评估咨询 ","合肥城市云数据中心股份有限公司","合肥","合肥高新区","玉兰大道767号机电产业园西二路科大国祯大厦二、四层","刘孟捷",13866784817]
[93,"皖通科技应急救援管理系统V1.0","安全应急服务类","该系统包括监控调度、养护防护、路产处置及施救处置、交警、路政等，信息交换和通信从车辆故障或事故发起，各主体之间相互沟通，做到精准调度、精准救援","道路运输业","安徽皖通科技股份有限公司","合肥","合肥高新区","皖水路589号","俞婷",15755162029]
[94,"桥梁与边坡安全监测系统","安全应急服务类","通过实时监测结构状态，分析服役性能，及时发现安全隐患，实现养护管理信息化，确保道路运营安全","道路运输业","安徽省综合交通研究院股份有限公司","合肥","合肥高新区","黄山路626号","王雪柳","0551-64387717"]
[95,"洪水灾害风险评估","安全应急服务类","当洪水超过防洪工程的设计标准或超过防洪体系的设计防御能力时，为确保防洪保护区内城市、重要工矿企业、重要交通铁路干线等重点保护对象或大部分地区的防洪安全而采取的超常规安全应急对策","评估咨询 ","安徽省水利水电勘测设计研究总院有限公司","合肥","合肥高新区","海棠路185号","刘志清",13956955251]
[96,"水利工程险情探测排查","安全应急服务类","为了工程的继续安全运行，需要对存在的问题及隐患进行应急排查、安全鉴定、除险加固","水利、环境和公共设施管理业","安徽省水利水电勘测设计研究总院有限公司","合肥","合肥高新区","海棠路185号","刘志清",13956955251]
[97,"火灾报警系统工程服务","安全应急服务类","泵站火灾报警应急处理设计","抢险救援 ","安徽省水利水电勘测设计研究总院有限公司","合肥","合肥高新区","海棠路185号","刘志清",13956955251]
[98,"食品安全检测","安全应急服务类","其他检测认证服务，本产品属于食品安全类别监测检测，在灾难预防期间，抗灾难期间，乃至灾后重建期间，本产品对灾民，救援队伍，重建队伍等人群具有安全方面的应急、预防、救治、提供安全防护性监测产品","其他安全应急服务 ","安徽科博产品检测研究院有限公司","合肥","合肥高新区","习友路2666号中科院合肥创新院1号楼","王燕",17352952062]
[99,"地质灾害评估","安全应急服务类","地质灾害评估，强化对自然地质的监测检测能力，提升自然地址灾害的应急处置能力","水利、环境和公共设施管理业","安徽金联地矿科技有限公司","合肥","合肥高新区","望江西路800号动漫基地A4幢5楼","刘亚军","0551-63453158"]
[100,"应用分发与检测业务APP","安全应急服务类","可针对APP进行功能分析、APP行为分析、APP后台的地址的溯源分析、APP网络数据报文分析，能够更为便捷、快速实现恶意应用的精准研判、并为测试留存电子证据","社会保障 ","安徽捷兴信息安全技术有限公司","合肥","合肥高新区","创新大道2800号创新产业园二期F5栋8层","张苗",15156878488]
[101,"短信安全筛查业务","安全应急服务类","安全短信平台主要基于运营商提供的短信端口，为客户指定号码提供批量发送短信服务，对短信内容安全审核。","评估咨询 ","安徽捷兴信息安全技术有限公司","合肥","合肥高新区","创新大道2800号创新产业园二期F5栋8层","张苗",15156878488]
[102,"电力设施监测软件开发及检测产品","安全应急服务类","通过“监测、告警、分析、处置”实现电力行业信息系统运行状态的主动探测和性能管理的业务闭环","电力、热力、燃气及水生产和供应业","安徽继远软件有限公司","合肥","合肥高新区","习友路1800号","郝祥云",13866180829]
[103,"360度监测影像系统、毫米波雷达","监测预警类","本公司产品可为救援车辆提供360度环视影像监测服务，并通过毫米波雷达实现对障碍物的实施监测","社会安全事件监测预警 ","合肥晟泰克汽车电子有限公司","合肥","合肥经开区","合掌路27号","赵官宏","18269779180"]
[104,"智能巡检机器人","监测预警类","移动巡检机器人可实现多场景快速部署，结合成熟的自主定位导航路径规划和人工智能巡检模块，适用于各种分离式智能巡检场景，可进行危险行为识别并实时报警，典型应用有监狱、看守所、海关等","水利、环境和公共设施管理业","合肥哈工轩辕智能科技有限公司","合肥","合肥经开区","宿松路3963号智能科技园C区3栋316室","李小龙",18656017137]
[105,"管道泄漏球形检测装置 ","监测预警类","管道泄漏球形检测装置是一种专门用来检测压力管道泄漏或气囊的球形检测设备。可适应不同管径大小或发生较大变化的管线，实现对管道泄漏或气囊检测的全范围覆盖","社会安全事件监测预警 ","安徽泽众安全科技有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院1号楼","何炜","18326630130"]
[106,"城市生命线工程安全运行监测系统","监测预警类","通过融合物联网、云计算、大数据等技术，感知桥梁、燃气、地下管廊等关键基础设施运行状况，主要用于监测城市关键基础设施运行状况并预警","电力、热力、燃气及水生产和供应业","合肥泽众城市智能科技有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院1号楼","王莎莎","15755128088"]
[107,"石油天然气管道场站安消一体化应急管理平台","监测预警类","采用倾斜摄影建立的实景三维模型，结合视频融合技术和视频监控设备以及智能化消防安全监测设备，从人员实时管控调度，设备，突发事件应急预案指挥等多个角度入手，全天候保障站场的安全运行环境，实现四维空间的实时管控","社会安全事件监测预警 ","安徽省川佰科技有限公司","合肥","合肥经开区","习友路以东、慈光路以南清华大学公共安全研究院4号楼5楼","管松","13966786786"]
[108,"石油天然气管线网络安全应急管理平台","监测预警类","实现对重点保护单位的信息资产数据和网站安全及可用性数据采集。实现对资产、漏洞、威胁和事件等基础础态势的分析跟踪与动态展现，对突发网络安全事故做到有迹可循，有技可施，提升网络空间安全风险的主动感知能力","社会安全事件监测预警 ","安徽省川佰科技有限公司","合肥","合肥经开区","习友路以东、慈光路以南清华大学公共安全研究院4号楼5楼","管松","13966786786"]
[109,"石油天然气管道关键信息基础设施安全保护应急管理平台","监测预警类","利用技术手段帮助对其重要门户网站、重要信息系统进行全面的安全漏洞监测、可用性、篡改、敏感词监测并且结合云安全中心以及网络安全设备产生的数据进行态势分析。并对爆发的网络安全事件进行通报预警、应急处置等功能。","电力、热力、燃气及水生产和供应业","安徽省川佰科技有限公司","合肥","合肥经开区","习友路以东、慈光路以南清华大学公共安全研究院4号楼5楼","管松","13966786786"]
[110,"LNG接收站安全生产应急管理平台","监测预警类","采用模块化部署方式，利用安气体、设备、资产等子系统集成语音、视频、数据调度功能，实现跨单位、跨部门之间的统一指挥协调，快速反应、统一应急、有效应对突发性安全事件。能够满足企业应急响应中心平台建设的需要","社会安全事件监测预警 ","安徽省川佰科技有限公司","合肥","合肥经开区","习友路以东、慈光路以南清华大学公共安全研究院4号楼5楼","管松","13966786786"]
[111,"消防安全服务云平台","监测预警类","基于贝叶斯信念网络的火灾动态风险人工智能推理模型，确定预警研判规则、研发技术集成原型系统，建设基于云计算、物联网、互联网+的全链条一站式消防安全云平台","事故灾害监测预警 ","辰安天泽智联技术有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院4号楼","王宇","13301168378"]
[112,"消防社会化服务产品","监测预警类","以物联网、互联网+、大数据等技术为支撑，将“物防”“技防”“人防”有机结合，提供覆盖消防设计施工、监测报警、维保检测、风险评估、课程演练、保险保障等全流程一站式服务","事故灾害监测预警 ","辰安天泽智联技术有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院4号楼","王宇","13301168378"]
[113,"一体式消火栓水压监测仪","监测预警类","本产品将压力检测单元伸入到消防供水管网中，检测管网中的水压力信号，通过无线传输单元将消防栓水压力和位置等数据信息发送至远程控制中心，控制中心根据数据信息判断消防栓管网水压是否异常","社会安全事件监测预警 ","安徽辰控智能科技有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院4号楼1-3层","李飞飞","15256988105"]
[114,"桥梁综合处理机","监测预警类","本产品是应用于桥梁建筑监测的前端数据采集处理中心设备，按照一定的策略采集、存储、上传桥梁监测传感器数据，实现了桥梁监测前端监测的标准化信息采集、分析和传输，解决了以往数据采集不标准、数据本地化计算分析困难及远传数据量大等问题","社会安全事件监测预警 ","安徽辰控智能科技有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院4号楼1-3层","李飞飞","15256988105"]
[115,"复合飞行器应急监测监控系统","监测预警类","该系统基于多旋翼无人机的空中监测平台，可以在事件发生后快速抵达现场，完成现场信息采集、传输处理，实现事发现场空地立体监测，为及时充分掌握现场情况、事件灾害评估、预警及预案启动、应急决策指挥提供重要依据和有力支持","社会安全事件监测预警 ","安徽泽众安全科技有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院1号楼","何炜","18326630130"]
[116,"应急低空飞艇监测监控系统","监测预警类","应急低空飞艇监测监控系统定位于现场空中监测平台，可以在事件发生后快速抵达现场，完成现场信息采集、传输处理，实现事发现场空地立体监测，为及时充分掌握现场情况、事件灾害评估、预警及预案启动、应急决策指挥提供重要依据和有力支持。","社会安全事件监测预警 ","安徽泽众安全科技有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院1号楼","何炜","18326630130"]
[117,"基于人机交互的主动式应急指挥调度系统","监测预警类","以“感知、监测、预警、处置、评估”五大新型能力，实现安全业务的全场景管理，培育“工业互联网+安全业务”融合创新应用","铁路、船舶、航空航天和其他运输设备制造业","中用科技有限公司","合肥","合肥经开区","宿松路3963号智能装备科技园E栋12层","王军玲","13966705825"]
[118,"小型监测预警雷达（以无人机为典型探测对象）","监测预警类","本产品系自主研发、拥有完全自主知识产权，可以提供对无人机等低慢小目标探测、拦截一体化处置，将安防由地面扩展到低空领域。并在发生突发情况时，为救援团队和人员提供相应的环境和安全监测","事故灾害监测预警 ","合肥海天电子科技有限公司","合肥","合肥经开区","蓬莱路西、汤口路南工业厂房三","张胜春","18956280159"]
[119,"微震监测与成像系统","监测预警类","该系统相比常规地震监测系统，具有更强的敏感性和更高的精确性，使得它所能监测的地下微震的震级更小、精度更高","事故灾害监测预警 ","安徽万泰地球物理技术有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院4号楼8楼","笪杜娟","15156085952"]
[120,"舆情监测平台","监测预警类","基于互联网、论坛等渠道，对通过传统和移动网络发生的群体舆情状态进行判断，为政府、企业等提供指导手段","社会安全事件监测预警 ","清创网御（合肥）科技有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院4号楼507室","李小超","13911064675"]
[121,"应急预警联动服务","监测预警类","以预防燃气爆炸、桥梁垮塌、路面坍塌、内涝等影响范围大的公共安全事故为目标，针对城市公路桥梁、城市地下管网、综合管廊、轨道交通、电梯等城市基础建设设施安全运行实时监测监控、预防预警，创新城市管理模式，提高安全管理效率","社会安全事件监测预警 ","合肥泽众城市智能科技有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院1号楼","王莎莎","15755128088"]
[122,"城市生命线整体解决方案","监测预警类","本项目实现对城市市老城区、高危地段、具有民生保障工程和敏感区域的地下管网、桥梁等城市生命线工程安全运行的实时在线监测；同时，完善城市生命线工程安全运行监测体系框架，升级扩展城市生命线工程安全运行监测系统海量数据处理能力，提高系统安全保障能力","社会安全事件监测预警 ","合肥泽众城市智能科技有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院1号楼","王莎莎","15755128088"]
[123,"桥梁安全运行监测解决方案","监测预警类","实时动态监测监测桥梁健康状况，可及时清晰的判断桥梁运行老化速度，结构弹性情况，不均匀沉降等影响桥梁使用年限的趋势，给桥梁的运行和养护提供科学支撑，确保桥梁疾病“早发现，早处置”。","社会安全事件监测预警 ","合肥泽众城市智能科技有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院1号楼","王莎莎","15755128088"]
[124,"燃气管网安全运行监测解决方案","监测预警类","在城市市主城区其他具有高泄漏概率的燃气管网相邻地下空间上共安装可燃气体采集监测仪及配套的供电、信号采集与传输、信号接收与处理设备等。应用燃气溯源扩散分析模型，结合地下管网、管道连通性分析，可以准确判断地下燃气泄漏影响的其他管网、地下密闭空间情况；地上重大危险源和重点防护目标","社会安全事件监测预警 ","合肥泽众城市智能科技有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院1号楼","王莎莎","15755128088"]
[125,"供水管网安全运行监测解决方案","监测预警类","供水管网流量、压力和声波等监测，结合大数据分析区域供水特征，实现泄漏监测和定位分析；基于水力学模型实现爆管预警分析；结合地质沉降监测及周边空洞信息实现路面塌陷分析，避免供水管网泄漏后路面塌陷引起重特大事故发生。通过管网空间分析和拓扑分析后自动生成关阀方案，为抢险抢修提供决策依据","社会安全事件监测预警 ","合肥泽众城市智能科技有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院1号楼","王莎莎","15755128088"]
[126,"排水管网安全运行监测解决方案","监测预警类","排水管网：流量、液位和汇集点水质；地面易积水点液位，河道液位、水质，泵站工作状态等监测，实现对排水管网的错接、渗漏、淤堵的识别，对城市内涝和河道水污染的预测预警和应急辅助决策支持","社会安全事件监测预警 ","合肥泽众城市智能科技有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院1号楼","王莎莎","15755128088"]
[127,"热力管网安全运行监测解决方案","监测预警类","热力管网：监测热力管网运行的流量、压力和温度，形成热力管网运行异常及时报警，进行事故预测预警，避免因爆管造成的伤害行人、影响交通和中断供热的事故的发生","社会安全事件监测预警 ","合肥泽众城市智能科技有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院1号楼","王莎莎","15755128088"]
[128,"管廊安全运行监测解决方案","监测预警类","综合管廊项目将实时监控城市地下综合管廊内的供水管网、燃气管网、热力管网等管线，对可能发生的灾害事件实现预测预警，提高了城市主动式安全防护能力","社会安全事件监测预警 ","合肥泽众城市智能科技有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院1号楼","王莎莎","15755128088"]
[129,"SecMS大数据安全监控系统","监测预警类","在发生突发情况时，在应急救援中提供数据的安全性检测和预警服务","社会安全事件监测预警 ","安徽三禾一信息科技有限公司","合肥","合肥经开区","清华路与宿松路交口合肥启迪科技城机器人产业基地1号楼4层","徐启胜","15505512911"]
[130,"可用于电子通信、安防系统等弱电系统的通信产品（电子传动与控制类产品）","监测预警类","对通讯器材核心零部件进行研发生产，用于监测预警系统建设，实现电子通信、安防系统、网络化等弱电系统的工程化集成","社会安全事件监测预警 ","合肥国声电子通信有限责任公司","合肥","合肥经开区","芙蓉路格林硅谷25幢","许文姣","13866196315"]
[131,"环境应急监测预警产品、测绘保障","监测预警类","环境应急监测预警产品：基于地理信息技术，与环保业务数据进行整合，实现信息基于 GIS 一张图的大数据平台效果展示。\n测绘保障：编制多业务专题图，通过GIS分析平台进行各要素展示","自然灾害监测预警 ","合肥亿图网络科技有限公司","合肥","合肥经开区","莲花路以东，石门路以南莲花路2#标准厂房D座303-305室","赵芳","18656975730"]
[132,"消防烟雾报警器等消防传感器","监测预警类","本产品主要应用于密闭空间内的烟雾报警系统","事故灾害监测预警 ","合肥众城电子系统工程有限责任公司","合肥","合肥经开区","创业园路一号民营一园办公楼","史维琴","15856384426"]
[133,"空气分离器","监测预警类","以过滤器、整流器、空气分离器等能有效维持流量计性能的设备为首，公司提供能够将手动阀门改造成自动阀门的小型致动器等与流体相关的产品","化学原料和化学制品制造业","合肥奥巴尔仪表有限公司","合肥","合肥经开区","天都路与紫篷路交口","韦小平",13956085069]
[134,"高纯度铜箔、铜线","监测预警类","产品应用于线路板印刷领域，是监测预警装备的核心上游供应企业","金属冶炼","合肥铜冠电子铜箔有限公司","合肥","合肥经开区","紫蓬路11号","姚蕾","15056209926"]
[135,"环境监测服务","监测预警类","环境监测服务可用于危化品泄露应急监测；火灾、爆炸产生的危害废气监测；环境污染监测","化学原料和化学制品制造业","安徽华测检测技术有限公司","合肥","合肥经开区","锦绣大道以南、习友路以东检测C楼","彭元兵","15345600269"]
[136,"工器具安全检测","监测预警类","为了防止使用中的电力安全工器具性能改变或存在隐患而导致在使用中发生触电、灼伤、高处坠落、刺穿或撞击等伤害事故，对电力安全工器具进行试验、检测和诊断","事故灾害监测预警 ","安徽恒力安全检测技术有限公司","合肥","合肥经开区","桃花工业园玉屏路276号合肥诚顺建材有限公司厂房","彭琴","18505601205"]
[137,"塞来昔布片","安全防护类","非甾体抗炎药，用于治疗成人急性疼痛","安全材料 ","大桐制药（中国）有限责任公司","合肥","合肥经开区","齐云路1号","耿瑞雪","18860467052"]
[138,"污水泄漏检测及处理等综合性服务","监测预警类","公司拥有智能巡检机器人、深度处理系统等自主创新产品和技术，自主研发的污水泄漏检测系统会提前对地下管网进行实时的泄漏检测，及时向控制中心发出预警","社会安全事件监测预警 ","合肥中盛水务发展有限公司","合肥","合肥经开区","九龙路与容成路交口东湖高新创新中心19幢","赵笑笑","15256984821"]
[139,"消防技术服务","监测预警类","对火灾隐患及失火现场提供专业的消防的现场预案和技术支持","社会安全事件监测预警 ","安徽勤志消防机电工程有限公司","合肥","合肥经开区","莲花路与石门路交口尚泽大都会独栋办公别墅A16栋2单元","谷健","13855607922"]
[140,"可用于教育场景的特种机器人","监测预警类","本公司产品可通过自主研发的图像识别及语音播报技术，集成为AI教育机器人，通过与用户的日常互动，将内置的各类安全应急知识向用户进行科普，并通过心理状态和沟通记录监测，动态调整互动模式","社会安全事件监测预警 ","合肥哈工路波机器人科技有限公司","合肥","合肥经开区","宿松路3963号智能装备科技园A区1栋107室","郭猛","15005666704"]
[141,"可用于紧急通知等场景的特种机器人（户户通机器人）","监测预警类","该机器人具备紧急通知、一键求救等功能，对于偏远地区可实现一键启动危险避难警报，在紧急灾害发生时语音通报危险情况，并能让用户一键拨通紧急通讯电话，缩短紧急信息沟通时间","社会安全事件监测预警 ","合肥哈工路波机器人科技有限公司","合肥","合肥经开区","宿松路3963号智能装备科技园A区1栋107室","郭猛","15005666704"]
[142,"航标","监测预警类","由结构钢等金属材料制造的航标和非金属材料制造的航标。标示航道（内河、海洋）方向、界限与碍航物的标志，具有导航，示位，警示作用","铁路、船舶、航空航天和其他运输设备制造业","巢湖市银环航标有限公司","巢湖市","巢湖市","凤凰山街道","徐玉军",13965434479]
[143,"土壤隐患排查","监测预警类","通过现场或者实验室检测土壤的数据，发现污染隐患，给企业或者政府主管部门提供治理相关数据依据","水利、环境和公共设施管理业","安徽海峰分析测试科技有限公司","合肥","庐阳区","庐阳中科大校友创新园13号楼","戴光玉",13905699152]
[144,"地下水隐患排查","监测预警类","通过地下水检测，识别可能造成地下水污染的污染物、污染设施和生产活动，识别可能造成地下水污染的污染物、污染设施和生产活动","社会安全事件监测预警 ","安徽海峰分析测试科技有限公司","合肥","庐阳区","庐阳中科大校友创新园13号楼","戴光玉",13905699152]
[145,"化工园区环境污染隐患排查","监测预警类","排查化工园区环境安全风险，规范化工园区环保设施建设和安全管理，系统提升化工园区本质安全水平，增强化工园区安全应急保障能力","水利、环境和公共设施管理业","安徽海峰分析测试科技有限公司","合肥","庐阳区","庐阳中科大校友创新园13号楼","戴光玉",13905699152]
[146,"消防安全物联网/消防安全物联网运营中心","监测预警类","一、线上服务：包括隐患、火警实时报警，闭环处理；任务自动派发等；二、监测值守；三、消防维保检测；四、安全教育培训、安全人员派遣等服务","事故灾害监测预警 ","安徽伭武科技有限公司（否）","亳州","亳芜园区","亳芜园区月季路369号","苏亚丽",15056798999]
[147,"胶带输送带保护控制监视系统","监测预警","煤矿井下胶带运输装备集中控制和监视系统，主要用途是对井下运输设备进行预警和处置。","采矿业","安徽恒泰电气科技股份有限公司","宿州","埇桥区","埇桥区汴河镇","范守宝",13956832996]
[148,"速凝膨胀封口剂","监测预警","主要用途是用于煤矿瓦斯综合治理的材料、设备和技术服务","采矿业","宿州市金鼎安全技术股份有限公司","宿州","埇桥区","宿州市埇桥区龙兴路","蒋  萍",15555710758]
[149,"皮带机自动化控制系统","监测预警","主要用于井下皮带机运输的安全监测和控制，具有报警、预警和设备的自诊断功能。","采矿业","安徽宝龙电器有限公司","宿州   ","埇桥区","埇桥区朱仙庄镇303省道朱仙庄工业园    ","刘新",13305579882]
[150,"矿用防爆设备","监测预警","煤矿井下皮带运输机保护装置，可以防止皮带跑偏、打滑、撕裂及通讯的设备。","采矿业","宿州中矿三杰科技有限公司","宿州","埇桥区","埇桥区城东街道十里村","王远东",13655578976]
[151,"光电感温火灾探测器","监测预警类","火灾燃烧释放热量，探测器对烟雾粒子浓度进行探测，将烟雾浓度的变化转化为电信号实现报警","事故灾害监测预警 ","蚌埠依爱消防电子有限责任公司","蚌埠","高新区","迎河路1300号（蚌埠依爱电子产业园电子厂房）","王志春",13305523119]
[152,"光电感烟火灾探测器","监测预警类","火灾燃烧产生大量烟雾，探测器利用热敏元件来探测火灾，并进行报警处理","事故灾害监测预警 ","蚌埠依爱消防电子有限责任公司","蚌埠","高新区","迎河路1300号（蚌埠依爱电子产业园电子厂房）","王志春",13305523119]
[153,"8000G火灾报警控制器","监测预警类","集火灾报警、联动控制、监管报警等多功能于一体。与EI系列探测器、模块等连接，接受报警信息，进行联动控制","采矿业","蚌埠依爱消防电子有限责任公司","蚌埠","高新区","迎河路1300号（蚌埠依爱电子产业园电子厂房）","王志春",13305523119]
[154,"可燃气体报警控制器","监测预警类","挂接本公司可燃气体探测器，接受探测器的报警信号，发出声光报警信号","事故灾害监测预警 ","蚌埠依爱消防电子有限责任公司","蚌埠","高新区","迎河路1300号（蚌埠依爱电子产业园电子厂房）","王志春",13305523119]
[155,"可燃气体探测器","监测预警类","连接EI系列火灾报警控制器及可燃气体报警控制器，用于探测建筑内部的可燃气体浓度","事故灾害监测预警 ","蚌埠依爱消防电子有限责任公司","蚌埠","高新区","迎河路1300号（蚌埠依爱电子产业园电子厂房）","王志春",13305523119]
[156,"煤矿用多气体参数测量装置","监测预警类","采用旋进漩涡流量传感器和抗振双控头插入式涡街传感器技术，结合甲烷和一氧化碳传感器，能自动监测管道内气体流量、甲烷浓度、一氧化碳浓度、压力和温度等参数，浓度超限启动声光报警器","采矿业","三正集团股份有限公司","淮南","田家庵区","国庆西路安成经济开发区","王保芝",18055442015]
[157,"KJ91X煤矿安全监控系统","监测预警类","用于对煤矿井下环境参数、工况参数的监测与控制，当井下某一局部瓦斯超限时，可根据需要切断相关区域的电源","采矿业","淮南润成科技股份有限公司","淮南","经开区","朝阳东路与吉兴路东北角","孙  超",13955488999]
[158,"矿用采空区火情监测系统","监测预警类","接入矿用采空区火情检测系统主机及各类环境参数传感器；对采空区存在自然发火隐患以及标志性气体积聚的区域，进行实时监测预警和定位","事故灾害监测预警 ","淮南润成科技股份有限公司","淮南","经开区","朝阳东路与吉兴路东北角","孙  超",13955488999]
[159,"煤矿用激光甲烷检测报警仪","监测预警类","适用于煤矿井下采掘工作面、回风巷道等场所对甲烷气体浓度进行连续检测，可由井下作业人员携带","事故灾害监测预警 ","淮南润成科技股份有限公司","淮南","经开区","朝阳东路与吉兴路东北角","孙  超",13955488999]
[160,"矿用一氧化碳传感器","监测预警类","用于煤矿井下或地面一氧化碳抽放管道内一氧化碳气体浓度的监测","事故灾害监测预警 ","淮南润成科技股份有限公司","淮南","经开区","朝阳东路与吉兴路东北角","孙  超",13955488999]
[161,"甲烷传感器","监测预警类","用于煤矿井下或地面甲烷抽放管道内甲烷气体浓度的监测","事故灾害监测预警 ","淮南润成科技股份有限公司","淮南","经开区","朝阳东路与吉兴路东北角","孙  超",13955488999]
[162,"火灾监测预警","监测预警类","融合先进的5G通信技术和物联网技术，把人工智能、智能终端和云服务等技术相结合，提供智能化物联网设备与智慧管理大数据云平台","自然灾害监测预警 ","信尔德科技有限公司","滁州","琅琊区"," 世纪大道677号","韩永超",19955002858]
[163,"5G技术多因子感应探测林火智能监测分析预警决策系统","监测预警类","以多系统集成等实现对突发林火灾害数据的收集分析等功能","自然灾害监测预警 ","安徽龙运智能有限公司","六安","霍邱县","城关镇玉泉西路","张春香",18919707640]
[164,"TK-6000荧光定量PCR仪","监测预警类","检测新型冠状病毒核酸的检测设备。检测灵敏度高、应用范围广。","公共卫生事件监测预警 ","安徽同科生物科技有限公司","六安","金寨县","开发区金梧桐产业园","何胜祥",18930701760]
[165,"新型冠状病毒（2019-nCoV）核酸检测试剂盒（PCR-荧光探针法）","监测预警类","用于筛查、鉴定新型冠状病毒感染的肺炎病人的检测和确诊。通过欧盟CE认证","公共卫生事件监测预警 ","安徽同科生物科技有限公司","六安","金寨县","开发区金梧桐产业园","何胜祥",18930701760]
[166,"摄像机及配件、安防镜头及光学制品","监测预警类","产品主要将滤光片套件装入半成品底座内加防尘盖，再装入塑胶镜头座或金属镜头座，贴防尘保护膜，底座与镜头座间用胶水固定，胶水通过UV光照固化，组装过程中UV光照操作员戴防护眼罩过UV固化，成品用12V电源测试合格，能够对突发事件进行实时监控并据此进行警示的产品","通用监测预警 ","安徽奇盟光电科技有限公司","六安","裕安区","裕安区高新技术产业开发区城南大道285号","李道红",18923811192]
[167,"环境应急监测预警产品、生产生活用水安全监测预警产品、环境检测设备","监测预警类","对生产环境和生产生活用水进行实时监测并据此对事故灾难的发生和发展趋势进行预测和警示。在突发事故发生后可以对周围环境进行检测检验","化学原料和化学制品制造业","安徽恒信通智能科技有限公司","六安","经开区","开发区五教路与衡山路交口联东U谷产业园21号楼","徐守全",18788826888]
[168,"环境监测系统","监测预警类","空气质量监测、烟气污染源监测、颗粒物监测、气溶胶激光雷达、温室气体监测仪器","通用监测预警 ","安徽蓝盾光电子股份有限公司","铜陵",null,"石城路工业园","贾强",15395624815]
["三、应急救援处置（198种）"]
[1,"应急指挥系统","应急救援处置类","是安全应急救援队伍通用装备，其机动性强、可靠性高、功能丰富，可实现现场各类信息的融汇处理及指挥决策。","道路运输业","四创电子股份有限公司","合肥","合肥高新区","习友路3366","潘芸芸",15155957017]
[2,"特种设备检测院特种设备应急处置指挥中心及视频会议","应急救援处置类","系统基于特种设备信息库，实现设备风险预警和应急决策支撑，提高应急处置效率，保障人民群众生命财产安全","石油、煤炭及其燃料加工业","科大国创云网科技有限公司","合肥","合肥高新区","文曲路355号办公楼4层","陈娇娇",18055160556]
[3,"储能系统","应急救援处置类","用于微电网建立，为无电地区提供电力，尤其在电力突然中断的情况下，提供电力支持","水利、环境和公共设施管理业","阳光电源股份有限公司","合肥","合肥高新区","习友路1699号","董继前",18855121816]
[4,"人血白蛋白","应急救援处置类","人血白蛋白是人体肝脏合成的血浆蛋白，用于失血、创伤及烧伤等引起的休克等。","公共卫生事件监测预警 ","同路生物制药有限公司","合肥","合肥高新区","燕子河路376号","武燕","0551-63613858"]
[5,"静注人免疫球蛋白","应急救援处置类"," 静注人免疫球蛋白可以增强机体的抗感染能力，用于继发性免疫球蛋白缺陷病，如重症感染等","公共卫生事件监测预警 ","同路生物制药有限公司","合肥","合肥高新区","燕子河路376号","武燕","0551-63613858"]
[6,"站所终端","应急救援处置类","配合配电子站、主站实现配电线路的运行状态监视、故障识别、 故障隔离和非故障区恢复供电等功能，保障用电安全","社会安全事件监测预警 ","科大智能电气技术有限公司","合肥","合肥高新区","望江西路5111号","刘丹",18356289296]
[7,"馈线终端","应急救援处置类","配合主站完成高压配电线路事故区的故障隔离，判别线路故障，清除瞬时故障，永久故障的隔离以及非故障区送电","社会安全事件监测预警 ","科大智能电气技术有限公司","合肥","合肥高新区","望江西路5111号","刘丹",18356289296]
[8,"智能配变终端","应急救援处置类","对非法APP应用软件识别和自动清除功能，对软件包合法性校验，支持安全启动功能，满足配网用电安全及有效","社会安全事件监测预警 ","科大智能电气技术有限公司","合肥","合肥高新区","望江西路5111号","刘丹",18356289296]
[9,"故障指示器","应急救援处置类","能够进行数据分析、告警显示、故障统计检索查询等，引导工作人员迅速准确找到故障点，提高供电安全可靠性","社会安全事件监测预警 ","科大智能电气技术有限公司","合肥","合肥高新区","望江西路5111号","刘丹",18356289296]
[10,"专变终端","应急救援处置类","负荷管理可使供电单位在电力供应总体不足的情况下，控制总用电量或负荷，从而保证电网安全和供电质量","社会安全事件监测预警 ","科大智能电气技术有限公司","合肥","合肥高新区","望江西路5111号","刘丹",18356289296]
[11,"以太网无源光网络","应急救援处置类","融合IPv6、网络安全、EPON无源光网络等技术，提供不间断转发、优雅重启、环网保护等技术，保证网络正常运行","社会安全事件监测预警 ","科大智能电气技术有限公司","合肥","合肥高新区","望江西路5111号","刘丹",18356289296]
[12,"断路器","应急救援处置类","主要用于关合电力系统中的负荷电流和开断过载电流及短路电流，对配电干线，分支线等起到安全保护作用","社会安全事件监测预警 ","科大智能电气技术有限公司","合肥","合肥高新区","望江西路5111号","刘丹",18356289296]
[13,"环网柜","应急救援处置类","整体开关装置不受外部环境影响，确保运行可靠及人身安全。扩展母线完全绝缘和屏蔽，确保高可靠性和安全性","社会安全事件监测预警 ","科大智能电气技术有限公司","合肥","合肥高新区","望江西路5111号","刘丹",18356289296]
[14,"雷达","应急救援处置类","雷达包含要地监视雷达等，集相控阵警戒雷达、光电探测、目标智能识别等高新技术于一体，广泛应用于监狱、看守所、机场、铁路、边防、营区等重要区域的周界防护","社会安全事件监测预警 ","华东（安徽）电子工程研究所","合肥","合肥高新区","蜀山区红枫路29","胡晶晶",13805516868]
[15,"卫星","应急救援处置类","商业遥感SAR卫星星座是指通过合成孔径雷达对地面发射和接受电磁波来获取陆地/海洋SAR图像及其应用产品。广泛应用于包括农业、林业水利、气象、海洋、城建、交通、减灾、环保、地质、测绘等民生领域","社会安全事件监测预警 ","华东（安徽）电子工程研究所","合肥","合肥高新区","蜀山区红枫路29","胡晶晶",13805516868]
[16,"浮空器","应急救援处置类","包含系留气球、飞艇以及无人机在内的多种空中平台，可搭载各种探测、侦察、通信、干扰等设备","社会安全事件监测预警 ","华东（安徽）电子工程研究所","合肥","合肥高新区","蜀山区红枫路29","胡晶晶",13805516868]
[17,"RTK算法的高精度定位系统","应急救援处置类","RTK算法的高精度定位系统的研发，可显著提高授时稳定性和精准性，即使在复杂信号环境下，亦可提供高精度、高完整性的精密授时服务。","社会保障 ","合肥移瑞通信技术有限公司","合肥","合肥高新区","习友路3335号中国（合肥）智能语音产业园A区1号","韩雪",13485690396]
[18,"家用制氧机","应急救援处置类","紧急医疗救护产品，氧疗有及时缓解缺氧症状的功效，纠正生理性缺氧和环境性缺氧，防治由于环境性缺氧造成的疾病，纠正病理性缺氧，氧疗是重要的辅助手段","其他救援 ","合肥雅美娜环境医疗设备有限公司","合肥","合肥高新区","天湖路9号","陈亚平",18055169621]
[19,"炉水循环泵","应急救援处置类","研制生产出具有我国自主知识产权的210kW 6kV炉水循环泵驱动电机、多种规格的炉水循环泵及驱动电机和配套辅助设备","电力、热力、燃气及水生产和供应业","合肥皖化电机技术开发有限责任公司","合肥","合肥高新区","习友路1799号","朱增娣",13856930403]
[20,"消油剂","应急救援处置类","洗消产品，用于应急安全清理消毒","其他救援 ","合肥东方美捷分子材料技术有限公司","合肥","合肥高新区","创新大道425号省科技成果转化基地D座2楼","胡俊",15255452831]
[21,"泵站排水控制系统","应急救援处置类","主要用于煤矿突水及城市防洪等应急抢险排水设备的电气及自动化控制","石油、煤炭及其燃料加工业","合肥三益江海智能科技有限公司","合肥","合肥高新区","红枫路9号中瑞科研楼B座305","徐韵菂",15155167991]
[22,"系留六旋翼无人机","应急救援处置类","通过光电复合缆，地面送电系统为空中平台及搭载设备提供能量，空中平台将信息通过线缆下传地面站系统。主要运用在公共安全应急指挥、通讯中继、空中监测等领域","抢险救援 ","合肥赛为智能有限公司","合肥","合肥高新区","创新大道666号","张媛媛",15056044790]
[23,"EPS应急电源","应急救援处置类","应急动力能源，用于突发事件的能源供应","电力、热力、燃气及水生产和供应业","合肥联信电源有限公司","合肥","合肥高新区","玉兰大道61号","袁雪峰",13615517377]
[24,"医疗变压器","应急救援处置类","医疗变压器广泛应用于医疗领域中的CT、MR等医疗设备中，主要用于隔离和电压变换作用，以满足安规要求的安全标准，是医疗行业的重要元器件。","生命救护 ","合肥博微田村电气有限公司","合肥","合肥高新区","天智路41号","秦嵩","0551-62724912"]
[25,"便携式移动电源","应急救援处置类","在野外执行任务时各种设备电量续航时间不足时，可通过便携式移动电源为通信设备、各种手持设备充电，延长单次任务时效","电力、热力、燃气及水生产和供应业","合肥博雷电气有限公司","合肥","合肥高新区","香樟大道168号科技实业园C5二层","陈阿松",18755193569]
[26,"储能变流器","应急救援处置类","可用于应急动力能源，实现电能的电压变换，单机功率大，配合储能电池或移动储能车，将电池电能转换为交流或直流电，给负荷使用，也可给储能电池充电","抢险救援 ","安徽中科海奥电气股份有限公司","合肥","合肥高新区","习友路2666号中科院合肥技术创新工程院4楼",null,13856074571]
[27,"储能系统","应急救援处置类","此产品将变流器设备和储能电池进行高度集成，安装于集装箱内，统一接口，所有线路预装，现场布置方便，可用于应急供电、储电和电能调度","电力、热力、燃气及水生产和供应业","安徽中科海奥电气股份有限公司","合肥","合肥高新区","习友路2666号中科院合肥技术创新工程院4楼",null,13856074571]
[28,"重组结核杆菌融合蛋白（EC）","应急救援处置类","紧急医疗救护产品，宜卡+灵敏度高、特异度高，可简便精准地在人群中筛查出结核感染者，是国家重大传染病结核病领域的技术突破","社会保障 ","安徽智飞龙科马生物制药有限公司","合肥","合肥高新区","浮山路100号","吴美丽","0551-65315669"]
[29,"新型冠状病毒检测试剂盒","应急救援处置类","紧急医疗救护产品，用于新冠病毒的监测，预防检测作用","社会保障 ","安徽深蓝医疗科技股份有限公司","合肥","合肥高新区","创新大道106号明珠产业园一期1#厂房D区四层","姚俊",18815605856]
[30,"应急运力共享公益平台","应急救援处置类","实现应急运力匹配全过程电子化管理，保证物资的安全、有序输送","道路运输业","安徽科大国创慧联运科技有限公司","合肥","合肥高新区","留学生园二号楼212、214、216室","储士升","0551-65396758"]
[31,"智能供配电产品","应急救援处置类","大功率数字阵列模块化UPS电源：能够提高系统的可靠性和可用性，应用场景：政府数据中心、金融、轨交、通信等行业","电力、热力、燃气及水生产和供应业","安徽博微智能电气有限公司","合肥","合肥高新区","香樟大道168号科技实业园B3号楼","祁瑶",18096609100]
[32,"重组人干扰素α2b","应急救援处置类","紧急医疗救护产品，本品具有广谱抗病毒、抗肿瘤、抑制细胞增殖以及提高免疫功能等作用，用于治疗病毒感染引起的肺炎等疾病。","生命救护 ","安徽安科生物工程（集团）股份有限公司","合肥","合肥高新区","蜀山区海关路9号","方志强","0551-65319985"]
[33,"喷射型自动射流灭火系统","应急救援处置类","该系统是利用红外线、数字图像或其他火灾探测组件进行早期火灾的自动跟踪定位，并运用自动控制方式来实现射流灭火的灭火系统。适用于会展中心、会议中心、体育馆、航站楼、商业综合体、厂房仓库、公路隧道等。","抢险救援 ","合肥科大立安安全技术股份有限公司","合肥","合肥高新区","蜀山区天湖路13号","汪娟娟","0551-68109586"]
[34,"喷洒型自动射流灭火系统","应急救援处置类","该系统是利用红外线、数字图像或其他火灾探测组件进行早期火灾的自动跟踪定位，并运用自动控制方式来实现射流灭火的灭火系统。适用于会展中心、高架仓库、大型停车场等大空间场所","抢险救援 ","合肥科大立安安全技术股份有限公司","合肥","合肥高新区","蜀山区天湖路13号","汪娟娟","0551-68109586"]
[35,"固定消防炮灭火系统","应急救援处置类","该系统可实现远距离控制固定式消防炮向保护对象喷射灭火剂灭火的系统，其中控制装置包括电控炮控制器、无线遥控器、电控器等，系统可根据需要增加视频监控功能。适用于保护面积大、火灾危险性高的室内外场所，如变电站、石油化工企业、储罐区、飞机库、仓库、港口码头、发电厂、干煤棚等。","抢险救援 ","合肥科大立安安全技术股份有限公司","合肥","合肥高新区","蜀山区天湖路13号","汪娟娟","0551-68109586"]
[36,"细水雾灭火系统","应急救援处置类","细水雾灭火系统是一种灭火效率高又对环境无污染的灭火系统,通过表面冷却、窒息、冲击乳化和稀释进行物理灭火。适用于档案馆、图书馆、医院、交通隧道、烟草仓库、汽车喷漆车间、配电机房、综合管廊等场所","抢险救援 ","合肥科大立安安全技术股份有限公司","合肥","合肥高新区","蜀山区天湖路13号","汪娟娟","0551-68109586"]
[37,"移动式细水雾枪","应急救援处置类","移动式细水雾枪产生高压细水雾射流进行灭火的消防装备产品，自带水箱也可由市政消防管网、生活用水、生产用水或天然水作为外供水源。设备雾化粒径小、灭火效率高，可用于扑救A类、B类、C类及电气火灾。抗击疫情、科学应急，研发团队临危受命","抢险救援 ","合肥科大立安安全技术股份有限公司","合肥","合肥高新区","蜀山区天湖路13号","汪娟娟","0551-68109586"]
[38,"全氟己酮气体灭火介质","应急救援处置类","通过快速吸热降温，抑制、阻断燃烧链式反应，实现高效灭火和抗复燃，不导电，110kV绝缘，性能最优；无残留、无腐蚀、安全环保。因优异的的灭火效能、安全余量、绝缘环保等特性，是哈龙、七氟丙烷等灭火介质理想完美替代品，特别设计用于高规格灭火系统使用，保护关键资产","抢险救援 ","合肥科大立安安全技术股份有限公司","合肥","合肥高新区","蜀山区天湖路13号","汪娟娟","0551-68109586"]
[39,"信息数据采集装置","应急救援处置类","采集、存储车内各席位收发的数据以及主要信息系统设备的运行和故障数据，可通过部署的数据分析管理软件为信息系统运行后的过程重演、效能评估、故障分析等工作提供数据支撑。","评估咨询 ","合肥同智机电控制技术有限公司","合肥","合肥高新区","永和路66号","刘佩",18855125298]
[40,"各类型号的彩钢板","应急救援处置类","本产品具有阻燃功能，且防腐蚀性能优良，可用于防火、防腐蚀等极端场景的安全防护，在突发情况时，可用于建设简易房屋的建筑中的地面墙面","其他救援 ","淀川盛馀（合肥）高科技钢板有限公司","合肥","合肥经开区","蓬莱路2551号","陆小凤",13956008786]
[41,"石油天然气配电设施消防应急灭火设备","应急救援处置类","作为全新一代高性能灭火剂，其优异的的灭火效能、安全余量、绝缘环保等特性，可以用于石油石化天然气高规格灭火系统使用，保护关键资产，有效解决灭火效率低，高压存储，有毒有害，喷发后不易清理的痛点","抢险救援 ","安徽省川佰科技有限公司","合肥","合肥经开区","习友路以东、慈光路以南清华大学公共安全研究院4号楼5楼","管松","13966786786"]
[42,"现场应急平台","应急救援处置类","给予领导或应急指挥人员现场意外的地方提供了解现场的动态和发展局势","采矿业","安徽辰控智能科技有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院4号楼1-3层","李飞飞","15256988105"]
[43,"龙芯、申威等系列国产计算机","应急救援处置类","通过自主研发的国产计算机生产制造，在应急情况当中提供自主可控的监测预警智能终端产品","抢险救援 ","合肥卓怡恒通信息安全有限公司","合肥","合肥经开区","云二路176号云海路工业园内","徐敏",13714690569]
[44,"特种机器人（消防/救援等）","应急救援处置类","具备爬坡、登梯及障碍物跨越，耐温和抗热辐射，防雨淋、防爆、隔爆，防化学腐蚀、防电磁干扰，遥控等行走和自卫功能。保障消防员的安全，提升抢险救灾能力 ","抢险救援 ","合肥哈工特安智能科技有限公司","合肥","合肥经开区","宿松路3963号智能装备科技园C区3栋5楼东侧","叶亚南","15755166798"]
[45,"智能清淤机器人","应急救援处置类","用来完成管道内部的缺陷检测、防腐涂层的涂敷、管壁的清洁清淤、管内修复等任务，它能够极大地提高管内检测和管内作业的准确性、可靠性和安全性，大大提高工作效率","电力、热力、燃气及水生产和供应业","合肥哈工灵顿工程科技有限公司","合肥","合肥经开区","宿松路3963号智能装备科技园A区3栋6楼","钱智超","18624000998"]
[46,"防灾应急包","应急救援处置类","防灾应急包在意外灾害发生后能帮助受困人员顺利逃生，增加生命安全保证的必备救护包，包括通用防灾应急包，车用应急包，矿用应急包等","抢险救援 ","安徽泽众安全科技有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院1号楼","何炜","18326630130"]
[47,"装载机、防爆叉车","应急救援处置类","应用于抢险救援过程中对堆积物料进行铲、装、运、挖及刮平场地等作业，其中电动叉车可应用于防爆要求高的极端场景","抢险救援 ","安徽合力股份有限公司","合肥","合肥经开区","方兴大道668号","方权","13866138949"]
[48,"挖掘机液压管路","应急救援处置类","为抢险救援的挖掘机等工程机械提供液压管路，属于该类装备的核心零部件，公司是日立建机、三一重工等知名企业的核心配套商","抢险救援 ","东海橡塑（合肥）有限公司","合肥","合肥经开区","方兴大道679号","胡婉婉",13739259701]
[49,"柴油发动机","应急救援处置类","向消防车等中重型救援车辆提供适合各个功率的柴油发动机，并可作为应急发电机的动力源","抢险救援 ","安徽康明斯动力有限公司","合肥","合肥经开区","云谷路1218号","杨玉婷","17344071497"]
[50,"挖掘机挖臂等配件","应急救援处置类","为抢险救援的挖掘机等工程机械提供挖臂等零部件，属于该类装备的核心零部件","抢险救援 ","合肥永升机械有限公司","合肥","合肥经开区","卧云路162号","陆今朝","15255191191"]
[51,"叉车等工程配件","应急救援处置类","为应用于安全应急抢险的装载机、叉车提供零部件配套","抢险救援 ","合肥和安机械制造有限公司","合肥","合肥经开区","桃花工业园汤口路","朱世利","13505514213"]
[52,"变压器等电力组件，应急发电机组","应急救援处置类","本公司生产的应急发电机组可提供24小时不间断电力供应，为电力系统持续可靠运行提供后勤保障，并可以为电力运行提供预警服务","电力、热力、燃气及水生产和供应业","合肥康尔信电力系统有限公司","合肥","合肥经开区","云门路158号厂房","周星","15256558725"]
[53,"血液处理透析等医疗器械","应急救援处置类","在发生突发情况时，我司的血液处理器械有利于手术中治疗伤员救助的反应速度","社会保障 ","尼普洛医疗器械（合肥）有限公司","合肥","合肥经开区","云谷路350号","何仁忠",13956983983]
[54,"高性能除尘设备","应急救援处置类","产品可以高效吸收、净化废气中各种有害气体及微细颗粒物，以达到减少废气排放至空气中粉尘和有害气体的含量","社会保障 ","安徽省利特环保技术有限公司","合肥","合肥经开区","汤口路2603号1号厂房","朱长效","13905513808"]
[55,"齿轮、动力传动装置","应急救援处置类","为抢险救援的挖掘机等工程机械提供齿轮、动力传动装置等核心零部件","抢险救援 ","合肥大久保机械有限公司","合肥","合肥经开区","耕耘路106号","张舒玉","18095657676"]
[56,"标准挂钩A型货叉、丝杆调距货叉、前移货叉等货叉产品","应急救援处置类","为应用于安全应急抢险的装载机、叉车提供货叉配件，属于重要零部件","抢险救援 ","安徽安鑫货叉有限公司","合肥","合肥经开区","卧云路3195号","汪文娟",13505617289]
[57,"装载机、叉车","应急救援处置类","应用于抢险救援过程中对堆积物料进行铲、装、运、挖及刮平场地等作业，可应用于救援物资的装卸、堆垛","抢险救援 ","安徽梯易优叉车有限公司","合肥","合肥经开区","方兴大道656号","张贵云","13705511512"]
[58,"刹车管、油压配管","应急救援处置类","提供可用于救援车辆生产的刹车管、燃料管、其它油压配管等零部件配套","铁路、船舶、航空航天和其他运输设备制造业","臼井管路系统（合肥）有限公司","合肥","合肥经开区","蓬莱路2353号","周安生","13605691982"]
[59,"自动化、智能化焊接装备","应急救援处置类","应用于智能机器人生产线的自动化焊接环节，是智能救援机器人生产的重要支撑","抢险救援 ","合肥哈工焊研威达自动化科技有限公司","合肥","合肥经开区","宿松路3963号智能装备科技园A区1栋711","乔俊杰","13708088229"]
[60,"机动车轮毂及配件","应急救援处置类","为救援车辆、运输车辆提供机动车轮毂配套","抢险救援 ","合肥润德车轮制造有限公司","合肥","合肥经开区","汤口路与蓬莱路西","唐善俊","18655132027"]
[61,"自动装盒机","应急救援处置类","为各种救援物资提供定制化的自动打包服务","社会保障 ","合肥哈工龙延智能装备有限公司","合肥","合肥经开区","宿松路3963号智能装备科技园A区109室","俞燕","18856068188"]
[62,"智能化焊接服务","应急救援处置类","为压力容器、钢结构、新能源提供智能化焊接服务，可应用于抢险救援过程中的应急焊接","抢险救援 ","合肥哈工易科自动化科技有限公司","合肥","合肥经开区","宿松路3963号智能科技园A3栋10楼","路冬梅","18133685016"]
[63,"堆垛式无人叉车","应急救援处置类","由电动叉车车体、KOB控制系统、导航控制系统、无线设备和调度控制系统组成。调度控制系统负责路径规划，任务调度和状态显示等工作，可应用于无人场景","环境处置 ","合肥哈工机器人有限公司","合肥","合肥经开区","宿松路3963号智能装备科技园A区3栋1705室","刘林",13856056906]
[64,"石油过滤器","应急救援处置类","在应急情况中，对物质中的石油进行过滤利用，提高能源使用率，降低环境污染风险","石油、煤炭及其燃料加工业","合肥哈工新能源科技有限公司","合肥","合肥经开区","宿松路3963号智能装备科技园A区2栋403室","方蔓蔓","15178188772"]
[65,"\t大中型移动应急平台","应急救援处置类","大中型移动应急平台面向应急现场，满足现场指挥决策需要，采用先进的数据库、应用软件，利用通信传输系统、主机与存储系统、局域网、装载平台等作为基础支撑，实现现场应急的综合应用","抢险救援 ","安徽泽众安全科技有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院1号楼","何炜","18326630130"]
[66,"\t三维电子沙盘","应急救援处置类","三维电子沙盘充分体现群体会商，指技合一的理念，具有可视、协同、分析、决策的特点。电子沙盘真实模拟了突发事件周边的地形、地貌，方便指挥人员在沙盘上进行态势推演，从而制定更为详细周全的处置方案，进行决策指挥","抢险救援 ","安徽泽众安全科技有限公司","合肥","合肥经开区","安徽省合肥市经济技术开发区习友路5999号清华大学合肥公共安全研究院1号楼","何炜","18326630130"]
[67,"\t背负式现场应急平台","应急救援处置类","背负式现场应急平台定位于穿戴式应急装备，可在第一时间抵达突发事件现场，采集突发事件现场视频、音频、地理位置等信息，并通过3G网络与指挥中心建立连接，将采集到的信息上传到指挥中心，同时建立双向语音通信，共同处置突发事件","抢险救援 ","安徽泽众安全科技有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院1号楼","何炜","18326630130"]
[68,"应急平台一体机","应急救援处置类","本产品是为基层政府量身打造的软硬件一体化的应急平台，作为国家应急平台体系的基层节点，深度融合了“分析、通讯、调度、存储”等业务环节","社会保障 ","安徽辰控智能科技有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院4号楼1-3层","李飞飞","15256988105"]
[69,"移动互联在线会商终端","应急救援处置类","该终端是基于公众移动网络的多媒体在线会商平台，具有跨领域、跨层级、跨地域的多级多方实时异地在线会商功能，解决了应急过程中实时信息共享、协同处置的难题。支持图像、双向语音传输，支持3G/4G、海事卫星传输。","抢险救援 ","安徽泽众安全科技有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院1号楼","何炜","18326630130"]
[70,"手机工作平台","应急救援处置类","该平台是应急平台的延伸，可由应急处置人员随身携带至现场，实现现场与应急指挥中心的实时信息交互。通过该平台可将事发现场的图像、视频、地理位置等信息发送至应急指挥中心，供研判人员用于辅助决策和事件处置。","抢险救援 ","安徽泽众安全科技有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院1号楼","何炜","18326630130"]
[71,"预警信息发布系统","应急救援处置类","该系统以气象、地震、旅游、水利、林业、国土、卫生、应急等部门的信息系统为支撑，根据政府授权和预警信息发布的有关规定，及时将自然灾害等突发事件预警信息在最短事件内向特定的区域、特定部门、特定人群及社会公众发布。","抢险救援 ","安徽泽众安全科技有限公司","合肥","合肥经开区","习友路5999号清华大学合肥公共安全研究院1号楼","何炜","18326630130"]
[72,"适用于越野救援车辆的轮胎","应急救援处置类","各类乘用车轮胎广泛应用于越野、涉水等极端环境下，为参与紧急救援的运输车辆，提供适合各种地形的轮胎零部件","抢险救援 ","安徽佳通乘用子午线轮胎有限公司","合肥","合肥经开区","始信路18号","方斌","13865905014"]
[73,"汽车、轨道交通空气调节器及热交换器","应急救援处置类","空气调节器及热交换器已应用于负压式救护车等救援场景，轨道交通空气调节器可有效支持各类轨道交通产品的空气交换、热量调节等需求","社会保障 ","安徽江淮松芝空调有限公司","合肥","合肥经开区","紫石路2869号","陈志平","13956001689"]
[74,"新能源汽车动力系统、汽车电池组","应急救援处置类","为特殊工况下的纯电动救援车辆、运输车辆提供动力系统总成以及电池组等，属核心零部件","社会保障 ","华霆（合肥）动力技术有限公司","合肥","合肥经开区","始信路62号动力电池厂房","周盛莹","15955139024"]
[75,"供电变压器、电力组件","应急救援处置类","本公司产品可应用于电力线路安全保障，确保电力线路平稳运行","电力、热力、燃气及水生产和供应业","合肥ABB变压器有限公司","合肥","合肥经开区","莲花路3318号","姚虹霞","13956066569"]
[76,"汽车线束","应急救援处置类","本产品系汽车内部各类信号的传输载体，属于负压救护车等应急抢险装备的核心零部件","社会保障 ","比克希汽车科技（合肥）有限公司","合肥","合肥经开区","始信路62号","张燕","18756010986"]
[77,"新能源汽车电池系统","应急救援处置类","为特殊工况下的纯电动救援车辆、运输车辆提供动力系统总成以及电池组等，属核心零部件","社会保障 ","合肥国轩电池有限公司","合肥","合肥经开区","宿松路3959号恒创智能科技园","吴海东","13355511003"]
[78,"箱式变电站","应急救援处置类","用于高低压系统配电操作与维护，可传输电能及分断阻隔故障源，起到保护和分配电源作用","电力、热力、燃气及水生产和供应业","安徽东方旭电气设备有限公司","合肥","合肥经开区","丹霞路以南、佛掌路以东钢结构厂房","王琴","18134529851"]
[79,"齿轮泵、齿轮马达","应急救援处置类","本公司生产的齿轮泵、齿轮马达及其他液压设备可适用于排涝抢险、障碍物升降等应急抢险","抢险救援 ","合肥皖液液压元件有限公司","合肥","合肥经开区","杭埠路260号","聂宗华","13615603458"]
[80,"电力线路运维及抢险服务","应急救援处置类","顺应全社会高效用能需求全新组建的首家市场化机制运营的综合能源服务供应商，提供专业的电力线路运维及抢险救援服务","电力、热力、燃气及水生产和供应业","合肥力能电力工程有限责任公司","合肥","合肥经开区","紫云路与青鸾路交口173号办公楼","程亚","18856079304"]
[81,"电力线路运维及抢险服务","应急救援处置类","在发生突发情况时，为电力线路安全运行提供专业的保障队伍及设备，多次参与电力应急抢险建设","电力、热力、燃气及水生产和供应业","安徽意通电力设备有限公司","合肥","合肥经开区","桃花工业区","曾云红",13956093325]
[82,"医用冰箱、医用深冷储存柜","应急救援处置类","在发生突发情况时，药品的运输和存储是医用冰箱的大有作为之时，作为医疗必备的产品，已用于疫苗、样本存储等领域","社会保障 ","中科美菱低温科技股份有限公司","合肥","合肥经开区","紫石路1862号","吴定刚","13956951555"]
[83,"双壁波纹管","应急救援处置类","在发生突发情况时，环境的质量是首要的保证，双壁波纹管作为污染物排放的首要设备，可及时解决应急事件现场的环境问题","社会保障 ","合肥通用环境控制技术有限责任公司","合肥","合肥经开区","蓬莱路616号","任启乐","13865917680"]
[84,"直埋蒸汽保温钢管","应急救援处置类","其承压能力高 、阻力小、耐低温、抗腐蚀、安装维修方便等优点适用于安全应急领域硬件建设","抢险救援 ","合肥华峰暖通设备有限公司","合肥","合肥经开区","合肥市肥西县紫蓬路","赵冰岩","18755180202"]
[85,"应急食品","应急救援处置类","本公司生产的营养面包等产品已应用于洪涝灾害、地震灾害等地质灾害的应急食品保障","社会保障 ","合肥华力食品有限公司","合肥","合肥经开区","莲花路2159号","王正鹏","13023096979"]
[86,"速热食品","应急救援处置类","在突发事件中，可快速满足受灾地区的食品需求，提供速热食品","社会保障 ","安徽东方航空食品有限公司","合肥","合肥经开区","新桥国际机场内","田苗苗",13956037129]
[87,"消防排烟低噪离心风机","应急救援处置类","高层建筑、地下车库、文教娱乐等大型公共建筑设施排烟及正压送风。该机具有消防排烟和通风换气的两用功能，具有效率高、噪声低、安装方便、运行平稳、流量大、耐高温等特点","环境处置 ","安徽国茂机电设备有限公司","合肥","肥东县","肥东龙塘工业区","邱灵洁",15209888896]
[88,"防火阀","应急救援处置类","材质：镀锌钢板（T），平时呈常开状态，易熔片熔断温度为70度，当风管内气流温度达到70度时，熔片熔断，可手动开启和关闭，阀门动作后手动复位阀门有六档调节风量开度阀门关闭后输出关闭信号（ＤＣ２４Ｖ）消防CCCF认证产品","环境处置 ","安徽国茂机电设备有限公司","合肥","肥东县","肥东龙塘工业区","邱灵洁",15209888896]
[89,"排烟防火阀","应急救援处置类","280℃排烟防火阀，消防CCCF认证产品，平时呈常开状态，易熔片熔断温度为70度，当风管内气流温度达到２８０度时，熔片熔断，可手动开启和关闭，阀门动作后手动复位阀门有六档调节风量开度阀门关闭后输出关闭信号（ＤＣ２４Ｖ）","环境处置 ","安徽国茂机电设备有限公司","合肥","肥东县","肥东龙塘工业区","邱灵洁",15209888896]
[90,"排烟阀","应急救援处置类","材质：镀锌钢板（T），平时呈常闭状态，火灾时烟感器通过控制中心发来电气信号（DC24v），执行机构内的电磁铁通电动作，阀门自动开启，并输出开启电信号\n阀门可手动开启，手动复位，消防CCCF认证产品","环境处置 ","安徽国茂机电设备有限公司","合肥","肥东县","肥东龙塘工业区","邱灵洁",15209888896]
[91,"应急防汛泵组","应急救援处置类","应急防汛泵组设备主要由各类水泵、户外配电柜或箱式变电站、电机或柴油发电机、管道组成。可应用于防汛抢险、应急救援、农业抗旱等领域。","电力、热力、燃气及水生产和供应业","安徽省康宇水电机械成套设备有限公司","合肥","肥东县","肥东县撮镇合马路12K","张文宇",13696526668]
[92,"应急排涝泵组","应急救援处置类","主要由户外配电柜、箱式变电站、电机或柴油发电机提供电力，将潜水泵、离心泵等水泵连接管道组成。安装形式简单，可在户外或野外进行泵组安装，完成排涝作业。可应用于防汛排涝、应急抢险等领域。","抢险救援 ","安徽省康宇水电机械成套设备有限公司","合肥","肥东县","肥东县撮镇合马路12K","张文宇",13696526668]
[93,"模块化活动厢房","应急救援处置类","模块化活动厢房产品（包括标准厢、卫生间洗漱间等功能厢），可用于应急安置房屋","社会保障 ","合肥田源精铸有限公司","合肥","肥西县","肥西县山南镇","徐庆久",13739276888]
[94,"雪橇式潜水泵","应急救援处置类","雪橇式潜水泵流量大，扬程高，在深区域连接排水软管安装便捷，可长时间稳定运行，工作效率高，能耗低，维护成本少，可应用于各种应急排水工作中","抢险救援 ","安徽正元机械有限公司","合肥","长丰县双凤工业区","凤霞路16号","丁碧春",13856084688]
[95,"高效轻型变频潜水泵","应急救援处置类","高效轻型变频潜水泵采用优质航空铝材料，重量轻，电机为永磁变频电机，控制柜采用航空快速插头连接方便快速，自身配有浮体，可适应多种环境，能充分发挥潜水泵的机动灵活性在各种应急环境中运行","抢险救援 ","安徽正元机械有限公司","合肥","长丰县双凤工业区","凤霞路16号","丁碧春",13856084688]
[96,"悬吊式潜水移动泵车","应急救援处置类","该泵车较固定式柴油机抽水泵方便于移动，适合不同应急场所使用","抢险救援 ","安徽正元机械有限公司","合肥","长丰县双凤工业区","凤霞路16号","丁碧春",13856084688]
[97,"防汛抗旱用排水设备","应急救援处置类","包含潜水泵、离心泵、自吸泵、污水泵等各类水泵应急排涝设备，在城市防洪排水、农田水利抗旱排涝等环境均可应用，能够为多种突发事件应急救援工作提供排水功能","水利、环境和公共设施管理业","安徽正元机械有限公司","合肥","长丰县双凤工业区","凤霞路16号","丁碧春",13856084688]
[98,"结构板房","应急救援处置类","以轻钢为骨架、夹芯板为围护材料、标准模数系列组合的环保经济型组合房屋，用于抗震救灾","社会保障 ","安徽富煌钢构股份有限公司","巢湖市","巢湖市","黄麓镇","赵维龙",13505650076]
[99,"纸面石膏板","应急救援处置类","以工业废渣脱硫石膏制成，用于房屋吊顶、隔墙建筑装饰装修板材，具有轻质、隔音、保温、防火、抗震、绿色环保等性能","社会保障 ","泰山石膏（巢湖）有限公司","巢湖市","巢湖市","烔炀镇","宋庆海",13856288018]
[100,"全自动特定蛋白分析仪","应急救援处置类","传染性疾病监测诊断预警产品：该产品基于免疫散射比浊法原理，与原配套的检测试剂共同使用，在临床上用于对人体样本中特定蛋白进行定量检测","生命救护 ","安徽伊普诺康生物技术股份有限公司","合肥","包河区","兰州路659号","廖爱平",18019909980]
[101,"全自动生化分析仪","应急救援处置类","传染性疾病监测诊断预警产品：基于分光光度法原理，与配套的检测试剂盒共同使用，用于人体样本中被分析物的定量检测","生命救护 ","安徽伊普诺康生物技术股份有限公司","合肥","包河区","兰州路659号","廖爱平",18019909980]
[102,"血清淀粉样蛋白A测定试剂盒","应急救援处置类","传染性疾病监测诊断预警产品：体外定量测定人血清中血清淀粉样蛋白A的含量","生命救护 ","安徽伊普诺康生物技术股份有限公司","合肥","包河区","兰州路659号","廖爱平",18019909980]
[103,"C-反应蛋白测定试剂盒","应急救援处置类","传染性疾病监测诊断预警产品：用于体外定量测定人血清中C-反应蛋白的含量","生命救护 ","安徽伊普诺康生物技术股份有限公司","合肥","包河区","兰州路659号","廖爱平",18019909980]
[104,"HFC5049XJHSZ负压救护车","应急救援处置类","用于重症及呼吸道疾病患者的转运救治，配备车载负压机，能够稀释救护舱的病原浓度，达到保护医护人员的功用","生命救护 ","安徽江淮专用汽车有限公司","合肥","包河区","繁华大道与天津路交叉口","胡汉全",13966741796]
[105,"免洗消毒凝胶","应急救援处置类","免洗消毒凝胶中的主要成分是75%乙醇，卡波姆，甘油，三乙醇胺等  ，主要用于手部的清洁消毒","个体防护 ","安徽广志药业有限公司","亳州","蒙城县","蒙城县双涧镇白杨林场阜西村","阜良军",15665693066]
[106,"84消毒液","应急救援处置类","84消毒液是一种无色或淡黄色的液体，其中是主要成分是次氯酸钠，属于一种高效的消毒剂，疫情期间主要用于宾馆、医院、家庭、学校以及各种公共场所的消毒","个体防护 ","安徽广志药业有限公司","亳州","蒙城县","蒙城县双涧镇白杨林场阜西村","阜良军",15665693066]
[107,"75%酒精消毒液（喷剂）","应急救援处置类","酒精的主要成分是75%的乙醇，酒精分子具有很强的渗透力，能穿过细菌表面的膜，进入细菌内部，使构成细菌生命基础的蛋白质凝固，将细菌杀死。适用于手与皮肤粘膜及空气、物体消毒","个体防护 ","安徽广志药业有限公司","亳州","蒙城县","蒙城县双涧镇白杨林场阜西村","阜良军",15665693066]
[108,"应急照明控制器","应急救援处置类","可配接应急照明集中电源、应急照明分配电装置、消防应急灯具，与火灾报警控制器连接，根据火警点智能疏散","社会保障 ","蚌埠依爱消防电子有限责任公司","蚌埠","高新区","迎河路1300号（蚌埠依爱电子产业园电子厂房）","王志春",13305523119]
[109,"TC400C5汽车起重机","应急救援处置类","TC400C5汽车起重机于2020年3月上市，该吨位产品采用东康国六发动机，广泛用于桥梁、道路、矿山等行业","抢险救援 ","安徽柳工起重机有限公司","蚌埠","高新区","柳工大道18号","梁爽",19856268868]
[110,"TC800C6汽车起重机","应急救援处置类","该产品充分融合行业75 吨和80 吨产品的优势，臂长最长、性能领先的四桥汽车起重机，广泛用于桥梁、道路、矿山等行业","道路运输业","安徽柳工起重机有限公司","蚌埠","高新区","柳工大道18号","梁爽",19856268868]
[111,"铝合金冲锋舟","应急救援处置类","具有轻质、高承载力、良好的快速性、耐波性、操纵稳定性和优越的适航性、省油等特点，抗撞击、抗沉、抗腐蚀、抗老化等性能优异。适用于抢险救援、水上交通、通信巡逻等勤务，以及多种商业用途","抢险救援 ","蚌埠市神舟机械有限公司","蚌埠","龙子湖区","龙子湖区交通路40号","史正波",18755210986]
[112,"机械化路面","应急救援处置类","主要由路面系统、作业车、信息化设备及附属器材等组成。装备主要用于克服江河岸浅滩、水际滩头、松软泥泞路段等障碍；快速构筑渡场进出路，也可用于市政工程建设、油田临时道路等","抢险救援 ","蚌埠市神舟机械有限公司","蚌埠","龙子湖区","龙子湖区交通路40号","史正波",18755210986]
[113,"舟桥","应急救援处置类","本装备是一种成套制式渡河器材。用于在紧急或非正常状态时,快速架设通道,保障机械重型装备、车辆及人员迅速克服江河、湖泊等水域障碍","铁路、船舶、航空航天和其他运输设备制造业","蚌埠市神舟机械有限公司","蚌埠","龙子湖区","龙子湖区交通路40号","史正波",18755210986]
[114,"高速艇","应急救援处置类","本艇双柴油机驱动，双半浸桨推进，主船体及上层建筑根据使用需要可采用船用铝合金或高强纤维增强塑料，水上速度可达到110km/h。主要用于各航区水域的巡逻、警备、执法等任务，也可用于应急救援的水上交通指挥和运输","抢险救援 ","蚌埠市神舟机械有限公司","蚌埠","龙子湖区","龙子湖区交通路40号","史正波",18755210986]
[115,"装配式钢梁桥","应急救援处置类","是一种可分解的、能快速架设的制式桥梁。具有构件互换性强，重量较轻，疲劳寿命长、通行性能好、运输拆装方便等特点。主要用14于快速架设临时性桥梁和抢修被破坏的桥梁，可保障50吨履带式、13吨以下轮式车辆通过。也用于构筑施工塔架、支撑等","抢险救援 ","蚌埠市神舟机械有限公司","蚌埠","龙子湖区","龙子湖区交通路40号","史正波",18755210986]
[116,"各型压缩机","应急救援处置类","主营产品涉及各类介质压缩机的核心装备设计及制造、常规天然气和非常规天然气的清洁利用系统解决方案、氢能储运加系统解决方案、生物质能源综合利用系统解决方案等应用领域。产品广泛用于燃气、化工、医药、食品、石油等行业","电力、热力、燃气及水生产和供应业","安瑞科（蚌埠）压缩机有限公司","蚌埠","高新区","南外环路2001号","洪二满",17755221233]
[117,"消防车","应急救援处置类","应用于消防灭火、救援、后勤保障、通讯等方面的专用车辆","抢险救援 ","蚌埠瑞祥消防机电设备有限公司","蚌埠","固镇县","固镇县王庄镇六铺路东首北侧","熊威",13909628228]
[118,"排涝车","应急救援处置类","应用于城市排涝的专用车辆","抢险救援 ","蚌埠瑞祥消防机电设备有限公司","蚌埠","固镇县","固镇县王庄镇六铺路东首北侧","熊威",13909628228]
[119,"市政专用车","应急救援处置类","应用于城市市政管道清淤、疏通等功能的专用车辆","社会保障 ","蚌埠瑞祥消防机电设备有限公司","蚌埠","固镇县","固镇县王庄镇六铺路东首北侧","熊威",13909628228]
[120,"干粉灭火剂","应急救援处置类","应用于油田、工矿企业、仓库、船舶、机场以及森林火灾。拥有灭火效能高、对环境污染小等特点","环境处置 ","蚌埠市龙泰消防药剂有限公司","蚌埠","固镇县","固镇县经济开发区纬六路南侧","卢思迪",18655259595]
[121,"建筑用升降机、高处作业电动吊篮","应急救援处置类","建筑用升降机、高处作业电动吊篮，俗称室外电梯。由设置齿轮驱动结构和安全设施的吊笼，装载人员或物料，沿着支撑在基础上和附着于建筑结构的导轨架，以齿条为阶梯，上升、下降或停靠在所要到达的层站，从而安全快捷的实现人员的垂直交通和物料的垂直运输","抢险救援 ","安徽升业工程机械有限公司","阜阳","太和县","太和县经济开发区创业路西侧钜阳路北侧","赵洋",18605685586]
[122,"改性管道","应急救援处置类","产品强度高接口方便，承受内压大，内表面光滑，水力条件好，具有高性能防腐，抗蚀耐磨性能。用于应急救援工作提供排水排烟功能","环境处置 ","安徽英标新材料科技有限公司","阜阳","界首市","界首市光武科技园繁兴西一路西段","谢兰明",13909679018]
[123,"改性管道","应急救援处置类","产品强度高接口方便，承受内压大，内表面光滑，水力条件好，具有高性能防腐，抗蚀耐磨性能。用于应急救援工作提供排水排烟功能","环境处置 ","安徽省生宸源材料科技实业发展股份有限公司","阜阳","界首市","界首市光武科技园繁兴西一路西西段","郭宗余",18908538333]
[124,"改性管道","应急救援处置类","产品强度高接口方便，承受内压大，内表面光滑，水力条件好，具有高性能防腐，抗蚀耐磨性能。用于应急救援工作提供排水排烟功能","环境处置 ","安徽超星新材料科技有限公司","阜阳","界首市","界首市光武科技园繁兴西一路西段","张玉勇",13905580333]
[125,"探针引物","应急救援处置类","IVD分子诊断核心原材料，qPCR,NGS等诊断手段或试剂盒的关键原料，临床诊断试剂开发不同阶段的核酸原料","抢险救援 ","通用生物系统（安徽）有限公司","滁州","经开区","祈福寺西路69号","何云龙",13905503222]
[126,"新冠 N 蛋白","应急救援处置类","N蛋白是冠状病毒(SARS-CoV-2)四种主要的结构蛋白之一，是一种高度免疫原性蛋白，参与基因组复制和细胞信号通路调节。常作为冠状病毒诊断检测工具，是免疫学快速诊断试剂的核心原料","生命救护 ","通用生物系统（安徽）有限公司","滁州","经开区","祈福寺西路69号","何云龙",13905503222]
[127,"核酸清洁剂","应急救援处置类","由两种无毒溶液组成，依次等量喷洒后即时起效，可在短时间内消除物品表面和空气中的DNA/RNA污染，同时对各类细菌及病毒有显著的灭活效果，并且能够高效灭活新冠病毒SARS-COV2","生命救护 ","通用生物系统（安徽）有限公司","滁州","经开区","祈福寺西路69号","何云龙",13905503222]
[128,"HCXF型消防机器人","应急救援处置类","可替代消防队员接近火灾现场实施有效的灭火救援作业，开展各项火场侦察任务","抢险救援 ","安徽恒创智能装备有限公司","滁州","南谯区","南谯区文慧路398号高教科创城无人系统制造示范区7号标准化厂房","徐必勇",13965627068]
[129,"循环水药剂","应急救援处置类","絮凝剂产品，包括有机絮凝剂、无机絮凝剂等，应用于工业生产所使用的循环冷却水中，防止系统发生结垢、腐蚀、菌藻滋生问题","生命救护 ","南京工大开元环保科技（滁州）有限公司","滁州","南谯区","南谯区高教科创城研发区浦园路2号","孙轶民",13705185558]
[130,"消防机器人、消防车","应急救援处置类","主要生产：灭火、侦察、运输等应急消防机器人","抢险救援 ","天长市安康消防设备有限公司","滁州","天长市","天长市汊涧镇工业园区永源东路","康有权",13705505935]
[131,"绷带、急救箱","应急救援处置类","专业生产一、二类医疗用品，产品有：橡筋类绷带、PBT绷带、氨纶绷带、急救绷带、急救包等","生命救护 ","安徽省康富医疗用品有限公司","滁州","天长市","天长市汊涧镇工业园区花园东路","许士珍",13605508368]
[132,"25、36米三相射流举高喷射消防车","应急救援处置类","1.适用条件：适用于各中火灾扑救，尤其适用于大型储油罐火灾扑救。2.主要用户：中石油、中石化及地方消防应急救援队伍。3.应用效果：灭火速度快，抗复燃效果好","抢险救援 ","明光浩淼安防科技股份公司","滁州","明光市","明光市体育路151号","徐晓辉",13905506302]
[133,"汕德卡涡喷消防车","应急救援处置类","1.适用条件：适用于各中火灾扑救，尤其适用火灾现场降烟除尘。2.主要用户：中石油、中石化及地方消防应急救援队伍。3.应用效果：功率大，灭火速度快，降尘除烟效果好。","抢险救援 ","明光浩淼安防科技股份公司","滁州","明光市","明光市体育路151号","徐晓辉",13905506302]
[134,"曼涡喷消防车","应急救援处置类","1.适用条件：适用于石油石化企业，隧道，港口码头，大型仓库和城市综合体火灾扑救，尤其适用火灾现场降烟除尘。2.主要用户：中石油、中石化及地方消防应急救援队伍。3.应用效果：功率大，灭火速度快，降尘除烟效果好。","抢险救援 ","明光浩淼安防科技股份公司","滁州","明光市","明光市体育路151号","徐晓辉",13905506302]
[135,"曼55、59万排烟消防车","应急救援处置类","1.适用条件：适用于石油石化企业，隧道，港口码头，大型仓库和城市综合体火灾现场降烟除尘。2.主要用户：中石油、中石化及地方消防应急救援队伍。3.应用效果：降尘除烟效果好","抢险救援 ","明光浩淼安防科技股份公司","滁州","明光市","明光市体育路151号","徐晓辉",13905506302]
[136,"远程供水大炮车","应急救援处置类","1.适用条件：适用于石油石化企业，隧道，港口码头，大型仓库和城市综合体火灾扑救。2.主要用户：中石油、中石化及地方消防应急救援队伍。 3.应用效果：流量大，射程远。","抢险救援 ","明光浩淼安防科技股份公司","滁州","明光市","明光市体育路151号","徐晓辉",13905506302]
[137,"远程供水系统泵浦消防车","应急救援处置类","1.适用条件：适用于石油石化企业，隧道，港口码头，大型仓库和城市综合体火灾扑救。2.主要用户：中石油、中石化及地方消防应急救援队伍。 3.应用效果：取水能力强大","抢险救援 ","明光浩淼安防科技股份公司","滁州","明光市","明光市体育路151号","徐晓辉",13905506302]
[138,"远程供水系统水带敷设车","应急救援处置类","1.适用条件：适用于水带敷设，水带回收。2.主要用户：中石油、中石化及地方消防应急救援队伍。 3.应用效果：取水能力强大","抢险救援 ","明光浩淼安防科技股份公司","滁州","明光市","明光市体育路151号","徐晓辉",13905506302]
[139,"4*4抢险救援消防车","应急救援处置类","1.适用条件：中石油、中石化及地方消防应急救援队伍现场救援。2.主要用户：中石油、中石化及地方消防应急救援队伍。3.应用效果：机动、灵活","抢险救援 ","明光浩淼安防科技股份公司","滁州","明光市","明光市体育路151号","徐晓辉",13905506302]
[140,"6吨供粉消防车","应急救援处置类","1.适用条件：石油石化企业油罐区火灾，工矿企业、厂房大型火灾扑救；2.主要用户：中石油、中石化及地方消防应急救援队伍。 3.应用效果：机动、灵活","抢险救援 ","明光浩淼安防科技股份公司","滁州","明光市","明光市体育路151号","徐晓辉",13905506302]
[141,"24吨供液消防车","应急救援处置类","1.适用条件：石油石化企业油罐区火灾，工矿企业、厂房大型火灾扑救及泡沫灭火剂保障；2.主要用户：中石油、中石化及地方消防应急救援队伍。 3.应用效果：泡沫灭火剂供应能力强","抢险救援 ","明光浩淼安防科技股份公司","滁州","明光市","明光市体育路151号","徐晓辉",13905506302]
[142,"120KW照明消防车","应急救援处置类","1.适用条件：石油石化生产装置，设备及路面洗消冲洗，危险品道路运输救援等；2.主要用户：中石油、中石化及地方消防应急救援队伍。 3.应用效果：供电距离远","抢险救援 ","明光浩淼安防科技股份公司","滁州","明光市","明光市体育路151号","徐晓辉",13905506302]
[143,"多功能泡沫车","应急救援处置类","1.适用条件：1）山地、丘陵地区远程供水；2）高层建筑供水3）远程供水；4）洪灾排涝；2.主要用户：中石油、中石化及地方消防应急救援队伍。 3.应用效果： 既可以满足火灾扑救需要，也可以为高层供水，或洪灾排涝","抢险救援 ","明光浩淼安防科技股份公司","滁州","明光市","明光市体育路151号","徐晓辉",13905506302]
[144,"高倍数排烟消防车","应急救援处置类","1.适用条件：适用于大型仓库、地下建筑、液化烃的流淌火、加油加气站等地方出现的火灾；2.主要用户：中石油、中石化及地方消防应急救援队伍。 3.应用效果： 既可以满足火灾扑救需要，也可以为高层供水，或洪灾排涝","抢险救援 ","明光浩淼安防科技股份公司","滁州","明光市","明光市体育路151号","徐晓辉",13905506302]
[145,"大功率发电照明车","应急救援处置类","1.适用条件：适用于大型仓库、地下建筑、液化烃的流淌火、加油加气站等地方出现的火灾；2.主要用户：中石油、中石化及地方消防应急救援队伍。3.应用效果：既可以满足火灾现场照明需要，也可以供电","抢险救援 ","明光浩淼安防科技股份公司","滁州","明光市","明光市体育路151号","徐晓辉",13905506302]
[146,"自行走增压灭火机器人","应急救援处置类","1.适用条件：适用于石油、化工企业及大型火灾现在远程供水增压、灭火、城市排涝；2.主要用户：中石油、中石化及地方消防应急救援队伍。 3.应用效果：既可以满足火灾现场照明需要，也可以供电。","抢险救援 ","明光浩淼安防科技股份公司","滁州","明光市","明光市体育路151号","徐晓辉",13905506302]
[147,"冲锋舟","应急救援处置类","应急救援用冲锋舟，产品通过中国船级社认定。船底深V型兴设计，小水阻，热融合双侧热压技术，多间隔膜双充气泵设计","铁路、船舶、航空航天和其他运输设备制造业","安徽明翊塑胶有限公司","六安","霍邱县","彭塔镇工业园区","李永好",15156933332]
[148,"多场景大功率应急电源（BP-Ⅱ型）","应急救援处置类","产品可用于可再生能源发电侧、输送侧及用户侧，实现大功率应急备电。既可以储存电，也可以输送交直流电，为新能源汽车、家用电器设备等供电","抢险救援 ","安徽绿沃循环能源科技有限公司","六安","舒城县","舒城县杭埠镇","邵振东",13395645796]
[149,"移动应急电源车","应急救援处置类","产品采用磷酸铁锂电池，安全环保，实现户外野炊、户外活动设备的供电。同时持续220V交流可达1.1C放电 ；24V、12V、5V直流放电功能","电力、热力、燃气及水生产和供应业","安徽沃博源科技有限公司","六安","舒城县","舒城县杭埠镇","邵振东",13395645796]
[150,"移动储能柜","应急救援处置类","整个系统由电池系统、直流充电桩、消防系统、照明系统、监控系统等组成，配备2个320KW车载直流充电桩，可为各种车辆等提供就地快速的补电服务","抢险救援 ","安徽星玛新能源有限公司","六安","舒城县","舒城县杭埠镇","陈宝华",13178332273]
[151,"新能源储能柜","应急救援处置类","分时错峰储能/供电，缓解电网供配电压力，在系统负荷小的时候储存电能，而在系统负荷大的时候释放电能，“削峰填谷”，提高电网运营的经济性。同时广泛用于风能、光能等多种能源发电储电","电力、热力、燃气及水生产和供应业","安徽舒玛新能源科技有限公司","六安","舒城县","舒城县杭埠镇","刘泽华",15586792450]
[152,"应急综合保障车","应急救援处置类","满足运载、宿营、饮食、饮水、被服洗涤、淋浴、如厕、环控、后勤保障、应急救治等需求","电力、热力、燃气及水生产和供应业","安徽博微长安电子有限公司专用汽车制造分公司","六安","经开区","开发区文翁路与迎宾大道交叉口","陈昌友",15856462503]
[153,"安科曼智能污水处理设备","应急救援处置类","安科曼智能污水处理设备，适用于农村污水处理、河道及池塘应急旁路治理","水利、环境和公共设施管理业","安徽黄河水处理科技股份有限公司","马鞍山","雨山区","雨山西路1800号7栋","夏然",17355595299]
[154,"消防栓","应急救援处置类","一种固定式消防设施， 主要作用是控制可燃物、隔绝助燃物、消除着火源。主要用于消防供消防车从市政给水管网或室外消防给水管网取水实施灭火","抢险救援 ","安徽驰安消防设备制造有限公司","马鞍山","含山县","含山县关镇（高速）道口工业集中区","贾启贵",18315508888]
[155,"干粉灭火器","应急救援处置类","产品为利用压缩的二氧化碳吹出干粉(主要含有碳酸氢钠)来灭火，用于各类灭火场所","抢险救援 ","安徽驰安消防设备制造有限公司","马鞍山","含山县","含山县关镇（高速）道口工业集中区","贾启贵",18315508888]
[156,"防火门","应急救援处置类","是建筑物防火分隔的设施，主要用在防火墙上、楼梯间出入口或管道井开口部位","抢险救援 ","安徽驰安消防设备制造有限公司","马鞍山","含山县","含山县关镇（高速）道口工业集中区","贾启贵",18315508888]
[157,"电动机消防泵组","应急救援处置类","公司生产的电动机消防泵组为XBD型，用于输送清水及物理化学性质类似于清水的液体，液体最高温度不得超过80度，广泛适用于工业与民用建筑等各类消防及生活（生产）用水","电力、热力、燃气及水生产和供应业","三联泵业股份有限公司","马鞍山","和县","经济技术开发区牛屯河路","李俊","0555-5307828"]
[158,"柴油机消防泵组","应急救援处置类","公司生产的柴油机消防泵组为XBC型，用于输送清水及物理化学性质类似于清水的液体，液体最高温度不得超过80度，广泛适用于工业与民用建筑等各类消防及生活（生产）用水","抢险救援 ","三联泵业股份有限公司","马鞍山","和县","经济技术开发区牛屯河路","李俊","0555-5307828"]
[159,"矿用耐磨多级离心泵","应急救援处置类","公司主要生产MD型矿用耐磨多级离心泵，具有效率高、性能范围广、运转安全和平稳、噪音低、寿命长、安装维修方便等优点。该类型的矿用多级离心泵适用于钢厂、矿山排水、污水输送等场合。用于煤矿应急时井下排水","采矿业","安徽三环水泵有限责任公司","马鞍山","和县","经济技术开发区太阳河路","周祖妹","0555-5389866"]
[160,"七氟丙烷自动灭火系统","应急救援处置类","以化学方工为主的气体灭火剂，具有无色、无味、不导电、无二次污染，对臭氧层的耗损潜能值为0，具有良好的环保性能，属于无毒、无腐蚀、无污染绿色环保产品,主要用于通讯机房、图书馆、电子计算机房等场所灭火","抢险救援 ","安徽飞达消防设备工程有限公司","马鞍山","当涂县","当涂工业园","张洵如","18955588119\n0555-6712919、6712119"]
[161,"混合气体自动灭火系统（IG541)","应急救援处置类","由氮气、氩气和二氧化碳按一定比例混合而成，无色、无味，不产生温室效应，对人体不构成伤害，属于无毒、无腐蚀、无污染绿色环保产品,主要用于通讯机房、图书馆、电子计算机房等场所灭火","抢险救援 ","安徽飞达消防设备工程有限公司","马鞍山","当涂县","当涂工业园","张洵如","18955588119\n0555-6712919、6712119"]
[162,"液压破碎锤","应急救援处置类","该产品属于挖掘机属具，可配合挖机进行房屋、路面、石块的破拆救援作业，以便于对人员进行快速施救","抢险救援 ","马鞍山市金拓液压机械制造有限公司","马鞍山","雨山区","雨山区工业园2-15号","王一",15212388875]
[163,"MPP森林防火飞机","应急救援处置类","可应用于自然灾害、事故灾难、社会安全事件等多场景的应急通信任务","抢险救援 ","中电科芜湖钻石飞机制造有限公司","芜湖","湾沚区","湾沚区安徽新芜经济开发区钻石路1号","林琳",18855310767]
[164,"MPP应急通信飞机","应急救援处置类","可应用于自然灾害、事故灾难、社会安全事件等多场景的应急空间规划、地理国情监测、资源管理、工程勘测施工信息决策及灾害评估等领域","抢险救援 ","中电科芜湖钻石飞机制造有限公司","芜湖","湾沚区","湾沚区安徽新芜经济开发区钻石路1号","林琳",18855310768]
[165,"干粉灭火器","应急救援处置类","干粉灭火器可扑灭一般火灾，还可扑灭油，气等燃烧引起的失火。 干粉灭火器是利用二氧化碳气体或氮气气体作动力，将筒内的干粉喷出灭火的。","抢险救援 ","安徽华星消防设备（集团）有限公司","芜湖","湾沚区","湾沚区迎宾大道1号","王飞",13855329058]
[166,"水基灭火器","应急救援处置类","水基药剂可在可燃物表面形成并扩展一层薄水膜，使可燃物与空气隔离，实现灭火。经雾化喷嘴，喷射出细水雾，漫布火场并蒸发热量，迅速降低火场温度，同时降低燃烧区空气中氧的浓度，防止复燃","抢险救援 ","安徽华星消防设备（集团）有限公司","芜湖","湾沚区","湾沚区迎宾大道1号","王飞",13855329059]
[167,"消火栓","应急救援处置类","一种固定式消防设施， 主要作用是控制可燃物、隔绝助燃物、消除着火源。消火栓主要供消防车从市政给水管网或室外消防给水管网取水实施灭火，也可以直接连接水带、水枪出水灭火","抢险救援 ","安徽华星消防设备（集团）有限公司","芜湖","湾沚区","湾沚区迎宾大道1号","王飞",13855329060]
[168,"84消毒液","应急救援处置类","消毒杀菌","社会保障 ","芜湖融汇化工有限公司","芜湖","鸠江区","鸠江区长江北路243号","丁有生",13605596707]
[169,"红外体温监测设备","应急救援处置类","红外线人体温度监测仪，是红外线体温筛选矩阵，适用于人流量大的公共场合快速监测人体体表温度的专业仪器。具有非接触式测温、超温语音报警等优点。特别适合于出入境口岸、港口、机场、码头、车站、机关、学校、影剧院等场合使用","建筑业","芜湖宏景电子股份有限公司","芜湖","经开区","经济开发区银湖北路 26号","郝希婵",13955312189]
[170,"（加）减压舱","应急救援处置类","供潜水员水下居住并能控制舱内外压力差的装置，主要用于潜水员和被救人员出水后的水面减压，潜水员加压锻炼和减压病的治疗","生命救护 ","上海打捞局芜湖潜水装备厂","芜湖","鸠江区","中国（安徽）自由贸易试验区芜湖片区永昌路58号","汪洪流",13637130679]
[171,"开式潜水钟","应急救援处置类","用于潜水员在水下作业的中继站和下潜、上升的运载工具，可提高水下作业效率，减轻劳动强度","社会保障 ","上海打捞局芜湖潜水装备厂","芜湖","鸠江区","中国（安徽）自由贸易试验区芜湖片区永昌路58号","汪洪流",13637130679]
[172,"潜水吊笼","应急救援处置类","用于潜水员在水下作业的另外一种下潜、上升的运载工具，可提高水下作业效率，减轻劳动强度","社会保障 ","上海打捞局芜湖潜水装备厂","芜湖","鸠江区","中国（安徽）自由贸易试验区芜湖片区永昌路58号","汪洪流",13637130679]
[173,"饱和潜水系统","应急救援处置类","用于援潜救生人员或者执行水下特种作战人员潜水员在饱和舱内通过加压使体内惰性气体完全饱和，然后乘坐潜水钟下潜至与舱内压力相同的水下进行作业，完成后带压返回饱和舱内，极大地提高潜水作业效率","社会保障 ","上海打捞局芜湖潜水装备厂","芜湖","鸠江区","中国（安徽）自由贸易试验区芜湖片区永昌路58号","汪洪流",13637130679]
[174,"打捞浮筒","应急救援处置类","  辅助沉船、沉物的打捞，难船的扶正、拖带","社会保障 ","上海打捞局芜湖潜水装备厂","芜湖","鸠江区","中国（安徽）自由贸易试验区芜湖片区永昌路58号","汪洪流",13637130679]
[175,"链式提升器","应急救援处置类","用于潜艇援助、舰船海上救助及打捞工程，特别适用于环境恶劣工况下的沉船残骸板正、拖拉、提升、沉船切割等作业","社会保障 ","上海打捞局芜湖潜水装备厂","芜湖","鸠江区","中国（安徽）自由贸易试验区芜湖片区永昌路58号","汪洪流",13637130679]
[176,"潜水热水机","应急救援处置类","用于潜水员在工作时能够连续供应热水的专用设备。通过可控制的加热方式，将外界持续输入的海水或淡水加热到所需温度，再通过加压装置加压输出，经脐带热水管送至潜水钟、潜水员热水服，为上述使用人员身体保温加热","水利、环境和公共设施管理业","上海打捞局芜湖潜水装备厂","芜湖","鸠江区","中国（安徽）自由贸易试验区芜湖片区永昌路58号","汪洪流",13637130679]
[177,"负压救护车","应急救援处置类","将车内的空气进行无害化处理后排出，避免更多的人感染，在救治和转运传染病等特殊疾病时可以最大限度地减少医务人员交叉感染的机率。清创缝合手术和心肺复苏等抢救都可以在救护车上进行。主要用于危重病人和传染病等特殊疾病的抢救","道路运输业","安徽奇瑞瑞弗特种车辆技术有限公司","芜湖","弋江区","弋江区高新技术开发区天井山路32号","王璐",17755330219]
[178,"篷布、帐篷","应急救援处置类"," 纱线、帆布、篷布、帐篷，用于防汛抗洪及其它民用","社会保障 ","芜湖强力帆布制品有限公司","芜湖","弋江区","弋江区珩琅山路30号","张萍",15155380826]
[179,"环卫应急处置方案；电动洗地机、电动扫地车","应急救援处置类","从事新能源环卫车辆生产、研发、销售的厂家，专业为人行道、辅道、背街小巷提供环卫综合解决应急处置方案","道路运输业","安徽爱瑞特新能源专用汽车股份有限公司","芜湖","繁昌区","繁昌区横山大道西50米","时兆前",18356213801]
[180,"大容量注射剂","应急救援处置类","大容量注射剂俗称输液（infusions），容量≥50ml并直接输入静脉的液体灭菌制剂，临床应用极为广泛。","生命救护 ","安徽双鹤药业有限责任公司","芜湖","繁昌区","三山经济开发区天成路2号","丁剑飞",13855326296]
[181,"节能环保工程设计、土建、安装以及相关设备的设计、开发、采购和销售，并提供相关咨询与服务","应急救援处置类","城市固体废物、污泥、危险废物的收集、运输、贮存、处置运营管理和技术服务","建筑业","芜湖海创环保科技有限责任公司","芜湖","繁昌区","繁昌区繁阳镇（芜湖海螺厂区内）","张苓鹏",15282407282]
[182,"智能移动泵站","应急救援类","以柴油机为动力，全液压驱动，子母式结构，工作部配置排水机器人，全套系统采用智能化控制，可实现无人值守。主要应用于应急排涝、应急消防、抗洪救险、森林防火等","抢险救援 ","安徽阿莫斯流体技术有限公司","宣城","宁国市","宁国经济技术开发区外环西路108号","黄运春",13856384397]
[183,"排水抢险车","应急救援类","吸水象系列皮卡泵车主要有四种车型：排涝抗旱车、吸污清淤车、应急消防车、民用特种车。是以皮卡车发动机为动力， 工作部采用全液压驱动、全隐形化设计的高度机动化、智能化、越野型、多功能应急救援工程车","抢险救援 ","安徽阿莫斯流体技术有限公司","宣城","宁国市","宁国经济技术开发区外环西路108号","黄运春",13856384397]
[184,"自扶正气胀救生筏","应急处置救援","产品有16人、20人、25人、32人、37人等五种规格。该系列救生筏是在抛投式气胀救生筏的基础上增加了自动扶正和吊车起吊救生筏降落面的功能。","抢险救援 ","广德富燕橡塑制品有限公司","宣城","广德市","广德市经济开发区国安路 98 号","杨林权",15695636988]
[185,"橡皮救生艇","应急处置救援","海上救助艇","抢险救援 ","广德富燕橡塑制品有限公司","宣城","广德市","广德市经济开发区国安路 98 号","杨林权",15695636988]
[186,"一次性使用穿刺输注类医疗器械","应急救援处置类","适用于供抽吸药液或注入药液后立即用于人体皮内、皮下、肌肉、静脉等注射或加药用的手动带针注射器","安全材料 ","安徽宏宇五洲医疗器械股份有限公司","安庆","太湖县","太湖县经济开发区观音路2号","余刚",13399566980]
[187,"分子筛除湿消毒专有技术设备(消毒机）","应急救援处置","利用分子筛转轮的超强吸水和耐高温的特性，采用洁净过滤+分子筛转轮干燥及高温消毒+UV灯管对空气进行杀菌净化的技术","环境处置 ","黄山天之都环境科技发展有限公司","黄山","高新区","高新技术产业开发区徽光路109号","杨邹巍","0559-2327730"]
[188,"浮箱","应急救援类","高分子低密度聚乙烯材质，内部填充EPS泡沫，重量轻、浮力大，可用于应急浮桥、救生储物平台、停泊码头","化学原料和化学制品制造业","黄山耀利水上设施有限公司","黄山","黄山区"," 黄山区浦园大道001号","王洁如",13399596229]
[189,"防潮垫","应急救援处置类","采用高密度PVC、春亚纺、涤塔夫面料，内置高回弹海绵。应用场景：家庭/办公室/汽车/郊游/露营","社会保障 ","祁门县昆腾户外用品有限公司","黄山","祁门县","祁门县开发区","曹咛",18955959269]
[190,"帐篷","应急救援处置类","采用PU牛津布、支架，便捷弹簧支架，一提即成，三秒速开免搭建，轻轻一压，帐篷便可自动收账，大空间设计，可容纳三到四人，可提可背省心省力。应用场景：家庭/郊游/露营","社会保障 ","祁门县昆腾户外用品有限公司","黄山","祁门县","祁门县开发区","曹咛",18955959269]
[191,"液压动力站系列","应急救援处置类","为液压工具提供动力的泵站，用于应急抢险救援","抢险救援 ","徽瑞智能装备（黄山）有限责任公司","黄山","歙县","歙县经济开发区二期纬五路","吴成志",18621893919]
[192,"液压排水泵系列","应急救援处置类","由液压动力站驱动的离心泵，用于应急抢险救援包括TP系列渣浆泵和AFP系列大排量轴流水泵","抢险救援 ","徽瑞智能装备（黄山）有限责任公司","黄山","歙县","歙县经济开发区二期纬五路","吴成志",18621893919]
[193,"履带式清淤、排水液压机器人系列","应急救援处置类","由液压动力站驱动，用于应急抢险救援，履带自行走，具备清淤及排水功能","抢险救援 ","徽瑞智能装备（黄山）有限责任公司","黄山","歙县","歙县经济开发区二期纬五路","吴成志",18621893919]
[194,"液压工具系列","应急救援处置类","由液压动力站驱动，用于应急抢险救援，可实现破拆、高压清洗、焊接、爬管、排风等功能","抢险救援 ","徽瑞智能装备（黄山）有限责任公司","黄山","歙县","歙县经济开发区二期纬五路","吴成志",18621893919]
[195,"液压多功能车","应急救援处置类","液压驱动多功能车，可以实现应急抢险、道路养护、清扫除雪等上百种功能，覆盖应急、消防、建筑等行业","建筑业","徽瑞智能装备（黄山）有限责任公司","黄山","歙县","歙县经济开发区二期纬五路","吴成志",18621893919]
[196,"大型矿用水冷却装置","应急救援处置类","用于矿业通风系统水冷却，给矿用设备生产企业做配套，根据不同流量及采掘面要求进行非标化设计及供货","抢险救援 ","徽瑞智能装备（黄山）有限责任公司","黄山","歙县","歙县经济开发区二期纬五路","吴成志",18621893919]
[197,"消防水带","应急救援类","涤纶长丝编织水带，水带内管采用聚氨酯材料，水带编织层与内管间采用的是自制的粘合剂，通过水蒸气的高温高压（通过试验设定值）将内管膨胀并受热粘合在编织层外管上。","抢险救援 ","黄山市龙潭消防水带有限责任公司","黄山","屯溪区","屯溪区九龙低碳经济园区","张琦璐",15005598170]
[198,"灭火防护服","应急救援类","生产消防员灭火防护服，工艺：原材料采购，电脑排版，断布裁剪，单件分拣，小部件熨烫，分件缝制，总体组合缝制，成衣熨烫。","社会保障 ","黄山博盛消防装备有限公司","黄山","屯溪区","屯溪区九龙低碳经济园区","朱江河",13731849159]